Single Axis PUP operating notes

June 13 2007

*******************************************

In lab 283 bench testing

Baseline current 260 mA at 120 VDC

Motor takes 100 mA on extension

Motor takes 100 mA on retraction

Humidity sensor reading 82

Pressure sensor reading 13 psi

******************************************
Cold Room testing (3 deg C)
Humidity sensor reading 70

Pressure sensor reading 12.5

Cycled actuator several times and successfully homed the actuator.  Left system powered up to monitor humidity over time (hours).

