Summary of SeaDevil Internal Cabling Modifications

Original Internal Cabling:

	J1 – 1
	Power +

	J1-2
	N/C

	J1-3
	DVL RS422 out/RS232 In

	J1-4
	DVL Comm Rtn

	J1-5
	DVL RS422 Out B/Rs232 Out

	J1-6
	Power -

	J1-7
	DVL RS422 Trig A

	J1-8
	DVL RS422 Trig B


	J2-1
	INS RS422 Out Hi/RS232 TxD to DVL

	J2-2
	INS RS422 Out Hi To MVC

	J2-3
	INS RS422 In Hi To MVC

	J2-4
	GPS RS422 Out Hi (Aux Out)

	J2-5
	INS RS422 Out Lo to DVL (N/C for RS232

	J2-6
	INS RS422 Out Lo/RS232 TXD to MVC

	J2-7
	INS RS422 In Lo/RS232 RxD from MVC

	J2-8
	GPS RS422 Out Lo (Aux Out)

	J2-9
	N/C

	J2-10
	N/C


	J3-1
	GPS RS232 TxD

	J3-2
	INS RS232 GPS In

	J3-3
	GPS Time Mark Pulse Out

	J3-4
	INS Time Mark Pulse In

	J3-5
	GPS RS232 Port A Out

	J3-6
	INS RS232 Out

	J3-7
	GPS RS232 Port A In

	J3-8
	INS Time Mark Pulse Rtn

	J3-9
	N/C

	J3-10
	N/C


MBARI Modifications

In order to support trigger and serial I/O to multibeam housing, and support GPS Port A access by MVC, make the following modifications:

Move J1-7 to J3-5

Move J1-8 to J3-7

Move J3-5 to J2-4

Move J3-7 to J2-8

Internally short J3-1 to J3-2

Move J2-4 to J3-1

Move J2-8 to J3-2

