DC/DC Converter requirements –

18-36VDC Input

R/N <60

Sync

5 volts/5A & 12V/3A

Sense

What if we eliminate the 12V loads (the freewave)?

Can’t – freewave requires 12V power.

Kearfott might be putting ripple on the bus. We should filter 24V power outputs from MVC power board to minimize ripple/hash making it onto board. This goes for tailcone as well as kearfott.

Kearfott converter frequency 600 Khz (per MTR data sheet). 

PC104 does NOT seem to be big noise contributor – mostly high frequency noise, probably suppressed locally. Need to quantify this better.

Need to check for tailcone noise.

