Mapping AUV Tail Critical Design Review

21 October 2003

Attending:

Dave Caress, Mark Sibenac, Hans Thomas, Rob McEwen, Farley Shane, Andy Hamilton, Bill Kirkwood, Ray Thompson

CDR Presented by Hans Thomas

This document captures comments and action items.

1. Section has +14-15 kg reserve buoyancy without cables.
2. Tail section hull is 69 inches long.
3. Need lifting point for tail section.

4. Want to either use single-piece rails or put joint in rails at spot weld aft of the joint in the ABS skin.

5. Need to lower the MVC sphere by 0.2 inch or so.

6. Homerpro position should be raised to avoid acoustic shadows. Perhaps it should poke through the ABS skin.

7. We are worried about the tail section bending when lifted in air. 

a. Adding screws through lower skin into bulkheads will strengthen the section.

b. We may need to add additional structure if it bends too much – will see what happens when we build it.

8. Design will take another two weeks. Foam drawings to CRP by end of this week. This should result in foam delivery by last week of this year.

