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1. Address fiber optic cable weight issue.

2. Test Point Connector, sixth connector on BIN to allow Ventana plug-in testing?

3. Calculate cable height off bottom allowable for given current flow.

4. Add handhold on RIN/BIN for ROV stabilization?

5. Modify Instrument cage to provide sloped front face for cable clearance?

6. Alternately (#5) reinforce frame corner and remove upper bar (channel) behind door?

7. Aeration or water injection system to break anchor suction of base ( for lifting).

8. Floor of Instrument cage – remove to prevent sedimentation.

9. Collar for mast Nobska to take out vibration in ODI connector?

10. Larry/T.C. to work on DVL for clearance to drop down into sled space.

11. Drop Weight – Fail safe open or closed?  ( not to drop weight with Hyd’s off)

12. ODI Bulkhd penetrators to case cap drawing for Mark C.

13. Homer Pro mount on RIN/BIN Inst. Cage.

14. Tiburon / Ventana depth calculation.  Are they the same?

15. Provide synthetic pigtail above lifting sling to release to allow unloading on touch down rather than freefall.

16. Tell “D” cell manufacturer –batteries wired in series. Therefore provide all in same prod. run

