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If your need Failure Analysis (FA), please fill in a form & send with failed unit

WORKING CONDITIONS OF FAILURE UNIT

Model GEN 40-60-LAN-1P230
Unit s/n:    LOC426A0710003
Time in use_____________________________

Customer Application:

Industrial (production flour)________________________

ATE___________________________________________

Laboratory______________________________________

Other_Research Boat, located in shipping container on deck_

Loading:

Output Voltage_______36 V max____________________

Output Current_______45 V max____________________

Load:  inductive_yes, long cables__ capacitive__________

electrical equipment_Load: Li Ion Batteries___________

Is more than one power supply connected

to the load/system?____NO_________________________

If so, please send us how power suppliers

are connected?   Parallel or serial ?___N/A_______

Input Line Parameters_220 VAC, 60 hz, ship power
Other Interfaces/option:

IEEE_________, Isolated Analog________, LAN___YES___

Analog programming  - Vprog/Iprog_______N/A__________

Communication: RS232_________________N/A__________

Remote sense (Yes/No)______________YES_____________
 Other  special options: Fast, Low noise, Other____________

                Please send a simple draft of system wire diagram
to the power supply including input line and additional

filtration when applicable.

   Possible failure reason (customer  version)_Unknown__


