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If your need Failure Analysis (FA), please fill in a form & send with failed unit

WORKING CONDITIONS OF FAILURE UNIT

Model GEN 40-60-LAN-1P230
Unit s/n:    LOC426A0690003
Time in use_____________________________

Customer Application:

Industrial (production flour)________________________

ATE___________________________________________

Laboratory______________________________________

Other_ Research Boat, located in shipping container on deck _

Loading:

Output Voltage________36 V max ___________________

Output Current________45 V max ___________________

Load:  inductive_ yes, long cables __  capacitive________

electrical equipment__ Load: Li Ion Batteries _________

Is more than one power supply connected

to the load/system?_____________________NO__________

If so, please send us how power suppliers

are connected?   Parallel or serial ?_______N/A_____

Input Line Parameter_220 VAC, 60 hz, ship power ___

Other Interfaces/option:

IEEE_________, Isolated Analog________, LAN___YES____

Analog programming  - Vprog/Iprog__________N/A________

Communication: RS232____________________N/A________

Remote sense (Yes/No)_____________________YES________
 Other  special options: Fast, Low noise, Other______________

                Please send a simple draft of system wire diagram
to the power supply including input line and additional

filtration when applicable.

   Possible failure reason (customer  version)Unknown__


