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MVC Address Map

Address Range(Hex)
Size(Hex) 
Description

0000-000F

16 Bytes 
DMA Controller 1 (8237)

0020-0021 

2 Bytes 
Interrupt Controller 1 (8259)

0022-0023 

2 Bytes 
ST486 Specific Registers

0040-0043 

4 Bytes 
Timer Controller (8254)

0060 


1 Bytes 
Keyboard Controller Data Byte

0061 


1 Byte 

NMI, Speaker Control

0064 


1 Byte 

Kbd Ctlr, CMD,STAT Byte

0070, bit 7 

1 bit 

Enable

0070, bit6:0 

7 bits 

Real Time Clock Address

0078 


1 Byte 

internal

0079 


1 Byte 

Watchdog

0080-008F 

16 Bytes 
DMA Page Registers

00A0-00A1 

2 Bytes 
Interrupt Controller 2 (8259)

00C0-00DE 

31 Bytes 
DMA Controller 1 (8237)

00F0 


1 Byte 

Reset Numeric Error

0102 


1 Byte 

VGA Setup Register

0150-0157

8 Bytes

Serial Port 11

0158-015F

8 Bytes

Serial port 12

0160-0167

8 Bytes

Serial Port 13

0168-016F

8 Bytes

Serial Port 14

0170-0177 

8 Bytes 
Secondary IDE Channel

01F0-01F7 

8 Bytes

Primary IDE Channel

0201 


1 Byte 

Super I/O

0278-027B 

4 Bytes 
Parallel Port 2 (Bidir)

02F8-02FF 

8 Bytes 
Serial Port 2

0300-0307

8 Bytes

Serial Port 7

0308-030F

8 Bytes

Serial Port 8

0310-0317

8 Bytes

Serial Port 9

0318-031F

8 Bytes

Serial Port 10

0340-035F

32 Bytes
PCFW-104-ETH NE2k Ethernet Device

0360-0367

8 Bytes

Parvus Fan Card



0378-037F 

8 Bytes 
Parallel Port 1

0380-0387

8 Bytes

Serial Port 3

0388-038F

8 Bytes

Serial Port 4

0390-0397

8 Bytes

Serial Port 5

0398-039F

8 Bytes

Serial Port 6

03B4, 03B5, 03BA 
3 bytes 

VGA Registers

03D4, 03D5, 03DA 
3 Bytes 
VGA Registers

03C0-03CF 

16 Bytes 
VGA Registers

03F0-03F5 

6 Bytes 
Floppy Controller Registers

03F6 


1 Byte 

IDE Command Port

03F7 (Write) 

1 Byte 

Floppy Command Port

03F7, bit 7 

1 bit 

Floppy Disk Change

03F7, bits 6:0 

7 bits 

IDE Status Port

03F8-03FF 

8 Bytes

Serial Port 2

0CF8 


1 Byte

PCI Configuration Address Register

0CFC-0CFF 

8 Bytes

PCI Configuration Data Registers

046E8 


1 Byte 

VGA Add-in mode enable Register

C000-C0FF 

256 Bytes 
PCI Configuration Registers
Interrupts

IRQ 
System Resource

NMI 
Parity Error

0 
Timer

1 
Keyboard

2 
Interrupt Controller 2

3 
Serial Port 2

4 
Serial Port 1

5 
PCFW-104-ETH NE2k Ethernet Device
6 
Floppy

7 
Parallel Port 1

8 
Real Time Clock

9 
Connecttech Xtreme Iso 12 Port serial card

10 
User available (PC/104 or -Plus)

11 
Ethernet Controller

12 
PS/2 Mouse

13 
Math coprocessor

14 
EIDE

15 
EIDE, if the Secondary IDE controller is disabled in BIOS

setup, IRQ15 can be used on the PC/104 or -Plus bus.

