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QUOTE

(1)  PK18500MD Palfinger Marine Knuckle Boom Crane:

• Maximum lifting moment 132,761 ft lbs.

• D - 5-section hydraulic boom extension

• H1/B3 classification according to DIN 15018.

• Hydraulic outreach 48ft.

• Lifting capacities:

· 17,636 lbs. @ 6.5 ft

· 12,626 lbs. @ 10 ft

· 8,179 lbs. @ 14 feet

· 5,643 lbs. @ 20 feet

· 3,650 lbs. @ 30 feet

· 2,072 lbs. @ 48 feet (Maximum Reach)

• Overall dimensions acc. to data sheet.

• Slewing angle 400° non continuous.

• Net slewing moment 16,963.9 ft lbs.

• Slewing cylinders bolted design.

• Dead weight of standard crane 5,002 lbs. plus extra equipment if added.

• Torsion resistant and fully closed hexagonal box type boom.

• Special crane base of cylindrical design for welding to deck with crane to base

    bolts provided.

• Standard height of mounting base ½ meter.

• Danfoss marine specification control valve in a control stand with 3 meter

     interconnecting hose kit. High pressure filter mounted to control stand.

• Special protection against corrosion for piston rods and pins.

• Load holding valves on slewing, inner, outer and extension boom cylinder.

• Electric over hydraulic emergency cut-off, requires 24 VDC if used.

• OMPSI Gauge mounted in control stand.

• Stainless steel pipe clamps.

• Stainless steel grease nipples.          

• All pins with thread holes for dismantling tools.

• All Crane Power / Palfinger Marine fitted bolts and nuts except mounting

    bolts are stainless steel.

• All steel components grit blasted SA2.5 acc. ISO8501-1 (DIN55928).

• Special sea water resistant 3-layer marine paint finish, blue RAL 5013,

   minimum total dry thickness 210 micron.

• JIC stainless steel adapters at crane valve. Installer will need to provide

   hosing (4) between the HPU and the valve stand. PHE can include in order if

   specified.

• One set metric to JIC adapters with 2 hoses to replace any hose on the machine for 
    emergency.

• 1 set of technical documentation:

· Crane Power / Palfinger Marine test certificate including 25% static overload test for the crane.

· Operator’s manual in English.

· Spare parts list in English.

· Instructions for installation.

· Hydraulic diagram.

· Maximum operating pressure acc. to hydraulic diagram.

· Recommended oil flow acc. to hydraulic diagram.
CRANE TOTAL







$ 88,614.38
(1) PHE Supplied Hydraulic Winch and Rigging Kit


• Includes Hydraulic Winch

• 10,000lb Line Pull Bare Drum Single Part

• 7,800 lbs Line Pull Full Drum Single Part

• 137 FPM Line Speed Bare Drum

• 176 FPM Line Speed Full Drum

• Spring applied hydraulically released dynamic and failsafe brake. 

• Hoses and fittings

• Labor to Install and Plumb Winch

• (1) 200 ft shot of 5/8” Non rotating wire rope w/ socket eye

• 5 Ton Crosby hook with safety latch

WINCH AND RIGGING KIT TOTAL




$ 10,792.65
(1)  PHE 2-Part Rigging Kit Adder (Optional to increase pull of winch, please note 





this also decreases the line speed of the winch)

• 20,000lb Line Pull Bare Drum Two Part

• 15,600 lbs Line Pull Full Drum Two Part

• 68.5 FPM Line Speed Bare Drum

• 88 FPM Line Speed Full Drum

ADDER TOTAL







$ 1,500.00 
(1) Five function fully proportional radio activated remote control system, including:

• Appropriate quantity of fully proportional high performance coils installed to         
    existing Danfoss marine specification control valve.  Includes all crane and winch     
    functions.

• Miratron radio receiver with the following features:

• Compact Housing, mounted in crane console.

• IP67 rated for most extreme environments.

• 7 factory preset outputs.

• Deutch DTM connectors.
• Cable harness to suit.

• External antenna.

• Miratron radio transmitter with the following features:

• Belly pack style with adjustable waist belt and neck harness w/buckles.

• Operating Range up to 500 feet.

• Frequency Hopping Spread Spectrum (FHSS) transceiver uses two-way 
    communication for maximum reliability and safety.

• Operates 902-928MHz (North America, Israel, Australia).

• Powered by two “D” alkaline (standard)or rechargeable batteries (optional).

• Blue faceplate color on transmitter, with PHE Logo.

• Routed labeling of faceplate on transmitter.

• Additional Logo’s or customer information can be custom routed on the transmitter.

• IP65 rated housing, for rugged environments

• Communication / Power Tether 15’ (see cut sheet) For emergency use if batteries are 
    low and for transmitter “learning” (see cut sheet).

• Battery life LED.

• (4) Single axis proportional thumb paddles, standard (other configurations are 
    available).

• Labeling per Palfinger Specs.

• (1) Emergency Stop switch and output cabling for existing emergency stop solenoid 
    coil on crane, to interrupt oil flow to the crane. 16mm Mushroom style.

• All of above installed, wired, tested and commissioned on crane at PHE.

• The radio system requires 24 VDC input.

• 5 week delivery


REMOTE TOTAL







$  13,290.82
(1) 30ELPUFD Hydraulic Powerunit

• 30HP, 60 HZ, 220/440 VAC, 3 PH motor close coupled to 10.5 GPM pump

• Rated at 4,500 PSI.

• Pump circuit is open center.

• Units are assembled to 50 gallon steel reservoir. 



• Reservoir is pre-piped with suction filter, 25 micron return filter, baffles, clean out 
    door, oil level/ thermometer, oil drain valve and filler/breather cap.

• Units are painted Palfinger Blue.

• Units are built to IP55 protection class.







HPU TOTAL







$ 9,117.05

(1) 30HPMSGRP Motor Starter (no Power Supply)

• Motor starter mounted in fiberglass enclosure with motor start/stop buttons

• Unit is across the line starters – not delta star style.

• 208-115 VAC transformer for control voltage, pre-wired.

• IP65 protection class.

MOTOR STARTER TOTAL






$ 2,626.93
SUB TOTAL







$ 125,941.83

(1) AGOR Style Bolt Down Skid

• Engineered to customers specification (shipping container storage)

• Galvanized, structural steel

• Baxter Bolt pattern (1” holes on 24” centers)

• Lifting eyes on corners

• Assembles

• HPU and Control Station installed on Skid

• Stainless Steel pipe and hose ends

• Testing of complete unit
AGOR SKID TOTAL






$ 20,769.23

TOTAL QUOTE







$ 146,711.06

Terms & delivery:

• The crane is in stock at Westport, MA.  

• Crane can be outfitted and ready to ship in 7 to 10 business days.

• Radio Requires 4-5 week delivery. 

• 50% deposit payment ARO, and the balance at completion of order at PHE.

• All prices are in U.S.D. and pricing is valid for 30 days.

• Crane is quoted FOB Westport, MA USA.

This quote does not include, but can be added for additional costs: 


• Welding the mounting column on to the deck.

• Any tools for welding, assembling, lifting gear etc.

• Load testing of the crane on board the ship including test weights.

• Classification company costs.

• Spare parts.

• Installing the crane according to our instructions.

• Or any other extras. 

