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Model name: SeaCatchCopy3
Current Configuration: Default

	Solid Bodies

	Document Name and Reference
	Treated As
	Volumetric Properties
	Document Path/Date Modified

	Fillet3
[image: ]
	Solid Body
	Mass:1.78493 lb
Volume:11.1558 in^3
Density:0.16 lb/in^3
Weight:1.78372 lbf

	Y:\Solid Models\Mapper Recovery Hook\SeaCatchCopy3-Thick.SLDPRT
Oct 31 10:33:51 2012
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	Properties
	Components
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		Name:
	Ti-6Al-4VSolution treated and aged (SS)

	Model type:
	Linear Elastic Isotropic

	Default failure criterion:
	Max von Mises Stress

	Yield strength:
	120000 psi

	Tensile strength:
	152290 psi



	SolidBody 1(Fillet3)(SeaCatchCopy3)
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	Fixture name
	Fixture Image
	Fixture Details

	Fixed-1
	[image: ]
		Entities:
	1 face(s)

	Type:
	Fixed Geometry






	Load name
	Load Image
	Load Details

	Force-3
	[image: ]
		Entities:
	1 face(s), 1 plane(s)

	Reference:
	Top Plane

	Type:
	Apply force

	Values:
	---, ---, -2000 lbf
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	Mesh type
	Solid Mesh

	Mesher Used: 
	Standard mesh

	Automatic Transition: 
	Off

	Include Mesh Auto Loops: 
	Off

	Jacobian points
	4 Points

	Element Size
	0.169793 in

	Tolerance
	0.00848964 in

	Mesh Quality
	High



Mesh Information - Details
	Total Nodes
	25369

	Total Elements
	16244

	Maximum Aspect Ratio
	31.662

	% of elements with Aspect Ratio < 3
	99.7

	% of elements with Aspect Ratio > 10
	0.0554

	% of distorted elements(Jacobian)
	0

	Time to complete mesh(hh;mm;ss): 
	00:00:01

	Computer name: 
	DEUTSCHLAND
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	Name
	Type
	Min
	Max

	Stress
	VON: von Mises Stress
	0.000863328 psi
Node: 19109
	23767.6 psi
Node: 23372
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SeaCatchCopy3-SimulationXpress Study-Stress-Stress



	Name
	Type
	Min
	Max

	Displacement
	URES: Resultant Displacement
	0 mm
Node: 151
	0.529241 mm
Node: 19450
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SeaCatchCopy3-SimulationXpress Study-Displacement-Displacement



	Name
	Type

	Deformation
	Deformed Shape
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SeaCatchCopy3-SimulationXpress Study-Displacement-Deformation



	Name
	Type
	Min
	Max

	Factor of Safety
	Max von Mises Stress
	5.0489 
Node: 23372
	1.38997e+008 
Node: 19109
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SeaCatchCopy3-SimulationXpress Study-Factor of Safety-Factor of Safety
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