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Model name: 20190610 Crane Crutch Assembly
Current Configuration: Default

	Solid Bodies

	Document Name and Reference
	Treated As
	Volumetric Properties
	Document Path/Date Modified

	Combine1
[image: ]
	Solid Body
	Mass:24.6528 kg
Volume:0.00314048 m^3
Density:7,850 kg/m^3
Weight:241.598 N

	C:\Users\enolasco\Desktop\RC Boom Crutch Atached to ROV Winch Chassis\Crane Parts\Crane Cradle Arm Tubing.SLDPRT
Jun 10 16:02:06 2019

	Boss-Extrude2[2]
[image: ]
	Solid Body
	Mass:0.385915 kg
Volume:4.91612e-05 m^3
Density:7,850 kg/m^3
Weight:3.78197 N

	C:\Users\enolasco\Desktop\RC Boom Crutch Atached to ROV Winch Chassis\Crane Parts\Crutch Base Mount.SLDPRT
Jun 10 10:35:49 2019

	Boss-Extrude2[1]
[image: ]
	Solid Body
	Mass:0.385915 kg
Volume:4.91612e-05 m^3
Density:7,850 kg/m^3
Weight:3.78197 N

	C:\Users\enolasco\Desktop\RC Boom Crutch Atached to ROV Winch Chassis\Crane Parts\Crutch Base Mount.SLDPRT
Jun 10 10:35:49 2019

	Fillet1
[image: ]
	Solid Body
	Mass:0.975889 kg
Volume:0.00069212 m^3
Density:1,410 kg/m^3
Weight:9.56371 N

	C:\Users\enolasco\Desktop\RC Boom Crutch Atached to ROV Winch Chassis\Crane Parts\UHMW Cradle.SLDPRT
Jun 10 11:23:52 2019
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	Study name
	Static 1

	Analysis type
	Static

	Mesh type
	Mixed Mesh

	Thermal Effect: 
	On

	Thermal option
	Include temperature loads

	Zero strain temperature
	298 Kelvin

	Include fluid pressure effects from SOLIDWORKS Flow Simulation
	Off

	Solver type
	Direct sparse solver

	Inplane Effect: 
	Off

	Soft Spring: 
	Off

	Inertial Relief: 
	Off

	Incompatible bonding options
	Automatic

	Large displacement
	Off

	Compute free body forces
	On

	Friction
	Off

	Use Adaptive Method: 
	Off

	Result folder
	SOLIDWORKS document (C:\Users\enolasco\Desktop\RC Boom Crutch Atached to ROV Winch Chassis\Crane Parts)
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	Unit system:
	SI (MKS)

	Length/Displacement
	mm

	Temperature
	Kelvin

	Angular velocity
	Rad/sec

	Pressure/Stress
	N/m^2
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	Model Reference
	Properties
	Components

	[image: ]
		Name:
	ASTM A36 Steel

	Model type:
	Linear Elastic Isotropic

	Default failure criterion:
	Unknown

	Yield strength:
	2.5e+08 N/m^2

	Tensile strength:
	4e+08 N/m^2

	Elastic modulus:
	2e+11 N/m^2

	Poisson's ratio:
	0.26  

	Mass density:
	7,850 kg/m^3

	Shear modulus:
	7.93e+10 N/m^2



	SolidBody 1(Combine1)(Crane Cradle Arm Tubing-1),
SolidBody 1(Convert-Solid1)(Crane Foot  Attachment-1),
SolidBody 1(Fillet1)(Crutch Base Mount-1),
SolidBody 2(Boss-Extrude2[2])(Crutch Base Mount-1),
SolidBody 3(Boss-Extrude2[1])(Crutch Base Mount-1)

	Curve Data:N/A

	[image: ]
		Name:
	Delrin 2700 NC010, Low Viscosity Acetal Copolymer (SS)

	Model type:
	Linear Elastic Isotropic

	Default failure criterion:
	Unknown

	Yield strength:
	6.3e+07 N/m^2

	Tensile strength:
	4.07e+07 N/m^2

	Elastic modulus:
	2.9e+09 N/m^2

	Poisson's ratio:
	0.3  

	Mass density:
	1,410 kg/m^3



	SolidBody 1(Fillet1)(UHMW Cradle-1)

	Curve Data:N/A
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	Fixture name
	Fixture Image
	Fixture Details

	Fixed-2
	[image: ]
		Entities:
	1 face(s)

	Type:
	Fixed Geometry




	Resultant Forces
	Components
	X
	Y
	Z
	Resultant

	Reaction force(N)
	-18,871.6
	33,809.6
	0.0162602
	38,719.9

	Reaction Moment(N.m)
	0
	0
	0
	1e-33


 



	Load name
	Load Image
	Load Details

	Force-1
	[image: ]
		Entities:
	2 face(s)

	Type:
	Apply normal force

	Value:
	9,533 lbf
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	Contact
	Contact Image
	Contact Properties

	Global Contact
	[image: ]
		Type:
	Bonded

	Components:
	1 component(s)

	Options:
	Compatible mesh
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	Mesh type
	Mixed Mesh

	Mesher Used: 
	Standard mesh

	Automatic Transition: 
	Off

	Include Mesh Auto Loops: 
	Off

	Jacobian points
	4 Points

	Jacobian check for shell
	On

	Element Size
	0.555272 in

	Tolerance
	0.0277636 in

	Mesh Quality Plot
	High

	Remesh failed parts with incompatible mesh
	Off



Mesh information - Details
	Total Nodes
	40410

	Total Elements
	20385

	Time to complete mesh(hh;mm;ss): 
	00:00:10

	Computer name: 
	ORIGINATOR

	[image: ]
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Reaction forces
	Selection set
	Units
	Sum X
	Sum Y
	Sum Z
	Resultant

	Entire Model
	N
	-18,871.6
	33,809.6
	0.0162602
	38,719.9


Reaction Moments
	Selection set
	Units
	Sum X
	Sum Y
	Sum Z
	Resultant

	Entire Model
	N.m
	0
	0
	0
	1e-33
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	Name
	Type
	Min
	Max

	Stress1
	VON: von Mises Stress
	2.752e-07 N/mm^2 (MPa)
Node: 28006
	3.697e+02 N/mm^2 (MPa)
Node: 28249

	[image: ]
20190610 Crane Crutch Assembly-Static 1-Stress-Stress1



	Name
	Type
	Min
	Max

	Displacement1
	UZ: Z Displacement
	-5.351e-03in
Node: 36633
	8.295e-03 in
Node: 37102

	[image: ]
20190610 Crane Crutch Assembly-Static 1-Displacement-Displacement1



	Name
	Type
	Min
	Max

	Strain1
	ESTRN: Equivalent Strain
	9.181e-13 
Element: 8279
	4.185e-03 
Element: 19314

	[image: ]
20190610 Crane Crutch Assembly-Static 1-Strain-Strain1



	Name
	Type

	Displacement1{1}
	Deformed shape

	[image: ]
20190610 Crane Crutch Assembly-Static 1-Displacement-Displacement1{1}



	Name
	Type
	Min
	Max

	Factor of Safety1
	Automatic
	6.763e-01 
Node: 28249
	9.085e+08 
Node: 28006
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20190610 Crane Crutch Assembly-Static 1-Factor of Safety-Factor of Safety1



	Name
	Type

	Displacement2
	Deformed shape
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20190610 Crane Crutch Assembly-Static 1-Displacement-Displacement2



	Name
	Type

	Design Insight1
	Design Insight

	[image: ]
20190610 Crane Crutch Assembly-Static 1-Design Insight-Design Insight1



	Name
	Type
	Min
	Max

	Stress2
	P1: 1st Principal Stress
	-3.350e+07N/m^2
Node: 28244
	1.860e+08 N/m^2
Node: 3911

	[image: ]
20190610 Crane Crutch Assembly-Static 1-Stress-Stress2



	Name
	Type

	Design Insight2
	Design Insight

	[image: ]
20190610 Crane Crutch Assembly-Static 1-Design Insight-Design Insight2
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