BASE  = HEX
MAP ICE
MAP  1000 TO  1fff USER
MAP  2000 to  5fff ICE
MAP  6000 TO 0dfff ICE
MAP 0E000 TO 0ffff USER
PRESRC  = 0
POSTSRC = 0
SOURCE = TRUE
WSR = 0F
TIMER1 = 0
WSR = 0
HSIO_EN = TRUE
load C:\TEMP\tailcone
namescope = :TAILCONE
DYNASCOPE = TRUE
define literally len = 'length'
define literally l = 'showsrc'
define literally b = 'define brkreg b1 = '
define literally gb = 'go using b1'
set :microlib to   \lib\microlib.lst
set :serial to     \lib\serial.lst
set :applay to     \lib\applay.lst
set :syslib to     \hardware\ibc\syslib.lst
set :pic to       ..\boards\cpu196\pic.lst
set :high_pwr to  ..\boards\high_pwr\high_pwr.lst
set :gf_board to  ..\boards\gf_5v\gf_board.lst
set :atod to      ..\boards\atod\atod.lst
set :nav_if to    ..\boards\nav_if\nav_if.lst
set :proto  to     \lib\proto.lst
set :malloc to     \lib\malloc.lst
set :regen to     ..\boards\regen\regen.lst
set :vicor to     ..\boards\vicor\vicor.lst
set :low_pwr to   ..\boards\low_pwr\low_pwr.lst
set :quad_ser to  ..\boards\quad_ser\quad_ser.lst
set :iso_io to    ..\boards\iso_io\iso_io.lst
set :ibc to       ..\ibc\ibc.lst
set :ibc_cmd to   ..\ibc\ibc_cmd.lst
reset ice
byte 2018 = 0F4
byte 2018 = 0F4
