Modifications for Motor Control Box Assembly:

1. ELMO L-Bracket: extend #8-32 slots (connects bracket to bottom lid) by 0.040” to allow bracket assembly to slide closer to the housing wall and hence relieve the tight fit between the ELMO connector and the PWM board heatsink.

2. PWM Board Mounts: Round specified corners (see updated drawings) to avoid any possible electrical short to the bottom lid. The larger mount also has a 0.025” in-cut for the same purpose.

3. PWM Board: Countersink transistor holes on the outside of the board, 82 degrees, such that the #4-40 (brass, Philips flat machine screw, 3/8”L) lies flush when the heatsink is attached.

4. SwageLok assembly note: For insertion of the elbow connectors on the bottom lid, at least one of the nuts (and ferrules) must be removed for adequate clearance to swivel.

5. Tailcone Frame Back-Plate (gray G10 material): modify to obtain clearance for the oil-compensator fitting and the MINK connector. See modification drawing FRAME BACKPLATE MODS.

