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SALES SHEET CHECKLIST  
Please fill in this configuration worksheet by circling the desired options and/or making notations on the worksheet and then return it to EdgeTech to receive a quote. 
CUSTOMER: 	 
DATE: 	 
	1210313


If this is a repeat order of a previously delivered system, please provide sales order number or system part number:  
 	 
	Vehicle Type: 

		• 	AUV/ROV/USV, etc:  

	DEPTH RATING: 

		• 	Max depth requirement: 6000m

	SYSTEM VOLTAGE: 

		• 	24v (20-35v range) 	 

		• 	48v (36-60v range) 	 

	SYSTEM CURRENT & POWER: 

		• 	Maximum current available for the EdgeTech 2200/2205 System: 

		• 	Budgeted power available for the EdgeTech 2200/2205 System: 

	SYSTEM ELECTRONICS: 

	EdgeTech can supply the system electronics as an individual board set, mounted onto a chassis or in a pressure bottle rated to the appropriate depth. 

	• 	Individual Board Set 	 

	• 	Board set mounted on chassis 	 

	• 	Pressure bottle 	 
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	SIDE SCAN SONAR FREQUENCY: 

	If ordering a Bathymetry system, leave this section blank and make your frequency selection in the Bathymetry section below.  Consult Engineering for custom configurations. 

		• 	None 	 

		• 	120/410 kHz 	 

		• 	230/540 kHz 	 

		• 	230/850 kHz 	 

		• 	540/1600 kHz 	 

		• 	75/410 kHz 	 

		• 	850 kHz Dynamically Focused 	 

		• 	230/850 kHz (850 kHz frequency is Dynamically Focused) 	 

		• 	230/540/1600 kHz or 75/230/410 Tri-frequency (any two frequencies can 
 be run at the same time) 

		• 	CUSTOM (Must be Verified with Engineering BEFORE SO is issued) 
 
SS1 = __________  SS2= __________  SS3= ___________  SB=__________ 

	SIDE SCAN SONAR EXTENSION CABLES: 

	The standard side scan array pigtail length is 12” (30.5 cm).  We can provide any of the extension cables listed below.  For custom lengths an additional charge would apply.  96” (2.4m) is the standard cable that we stock; all other cables carry a 14-week lead time.   

		• 	None 	 

		• 	96” (2.4 m) (stock) 	 

		• 	38” (1 m) 	 

		• 	60” (1.5 m) 	 

		• 	 16 inch	 

	SUB-BOTTOM PROFILER FREQUENCY: 

	Each Sub-Bottom profiler kit comes with one transmit transducer, two receive hydrophones or PVDF Panel  with TX & RX sections mounted to a plate for simplified installation.  Cabling is provided separately 

		• 	None 	 

		• 	4-24 kHz 	 

		• 	2-16 kHz 	 

		• 	1-6 kHz 	 

	SUB-BOTTOM PROFILER CABLING: 

	There are three standard lengths to choose from for the transmit cable; 39” (1m), 66” (1.7m) or 118” (3m). You have a choice of receive spider cable lengths as outlined below. The specified lengths are on either side of the molded junction box. 

		• 	68 + 68” (1.7 + 1.7 m) 	 

		• 	88 + 16” (2.2 + 0.4 m) 	 

		• 	79 + 114” (2 + 3 m) 	 

		• 	16 + 12” (0.4 + 0.3 m) 	 

		• 	Custom:  Pigtail 1 (to elex) __96’’_____  Pigtail2 ___12’’______  Pigtail 3 _____12’'____ 	 


 	 
	SUB-BOTTOM PROFILER PVDF RECEIVERS 

	Legacy Line Arrays are still available [36” (106), 22” (216), 13” (424)].  An additional option is the use of PVDF panels which offer higher sensitivity and higher array gain (noise rejection).  When a single panel is purchased, no SB spider is required.  PVDF Pigtails are 12” (std) in length but can be customized up to 90” (nominal, NRE applicable).  Stock extension cable is shown below; custom lengths require 14weeks.  Custom panels require NRE Costs and Mold Fabrication. 

		• 	PVDF Extension Cable (stock);  7.2ft (22200mm)                (p/n 0017985) 	 

		• 	Standard PVDF Panel for 106 SB;     20.0” (W) x 29.0” (L)       (ICD 0017354 & 
 p/n 0017356) 

		• 	Standard PVDF Panel for 216 SB;     11.75” (W) x 23.75” (L)   (ICD 0017353 & 
 p/n 0017355) 

		• 	Standard PVDF Panel for 424 SB;       9.5” (W) x 16” (L)           (ICD 0017352 & 
 p/n 0017513) 

		• 	PVDF Panel for 216/424;     11.5” (W) x 16.0” (L)                      (ICD 0016760 & 
	p/n 0016751) 	 
      Note:  This is a special unterminated panel.  A termination can be added. 
 

		• 	PVDF Panel for 424 (AUV)     7.4” (W) x 18.0”(L)                       (ICD 0015586 & 
 p/n 0015590) 

		• 	PVDF Panel for 424 (AUV)     6.5” (W) x 5.9” (L)                        (ICD 0017458 & 
	p/n 0017456) 	 
Note:  This is a special unterminated panel.  A termination can be added. 
 


Side Scan Sonar Arrays 
	ICD 
	DESCRIPTION / COMMENT 
	DEPTH RATING 
	FREQUENCY SETS 

	0013168 
	SSS only, small AUV (mounted on outside) Anodized Aluminum housing 
	2000m 
	230 / 850 DF : main option 
230 / 850 (has not been made) 
410 / 850 (has not been made) 
540 / 1600 (has not been made) 

	0012011 
	SSS only, large AUV - typically mounted looking through a cut-out in the hull. Rear bulkhead connector, so requires extension cables 
	6000m 
	120 / 410 230 / 540 
230 / 850 
230 / 540 / 1600 (Tri-Freq) 

	0013717 
	SSS only, large AUV - typically mounted looking through a cut-out in the hull. 
	6000m 
	75 / 410 
As above, but longer to accommodate 75 kHz 

	0010481 
	SSS only, ROV and large AUV. 
4200 Rx / 2000 style arrays – aluminium channel 
	2000m  or  
6000m 
	120 / 410 230 / 540 
230 / 850 410 / 850 

	 
0013266 
0013267 
0013268 
 
	For ROV’s : 
Cover – SP modified 
Bracket – Port 2000 SP modified 
Bracket – Strb 2000 SP modified 
	 
	 

	0010490 
	Standard SS Extension cable (MCIL5F/M) 
8ft 
	 
	 

	ICD 
	DESCRIPTION / COMMENT 
	DEPTH RATING 
	
	FREQUENCY SETS 

	0016090 
	Standard SS-DF Extension Cable (MCIL8F/M) 2m 
	 
	 
	


Sub-Bottom Profiler Arrays 
	ICD 
	DESCRIPTION / COMMENT 
	DEPTH RATING 
	FREQUENCY SETS 

	0011003 
0017352 
	KT-424 transmit 
Standard 424 PVDF array (9.5” x 16”) 
	6000m 
6000m 
	AUV version 4-24 kHz 

	0012552 
0017353 
	KT-216 transmit 
Standard 216 PVDF array (11.75” x 23.75”) 
	6000m 
	AUV version 2-16 kHz 

	0019412 
	DW-216 
Above mounted on a skid plate 
	6000m 
	ROV version 

	0011029 
0017354 
	KT-106 transmit 
Standard 106 PVDF array (20” x 29”) 
	6000m 
	AUV version 

	0019410 
	DW-106 
Above mounted on a skid plate 
	6000m 
	ROV version 

	0009855 
	Default Tx cable 
	 
	 

	0017985 
	Default PVDF Rx cable  
	 
	 


 
CONFIGURABLE ITEM 
SELECTION 
BATHYMETRY & SIDE SCAN SONAR FREQUENCY: 
All offerings below are simultaneous dual frequency Side Scan Sonar with Bathymetry on one frequency.  
 
•
 
None
 
 
•
 
 kHz (Bathymetry on 540 kHz
540/1600
)
 
 
•
 
230/540
 kHz (Bathymetry on 230 kHz
)
 
 
•
 
230/540
)
 kHz (Bathymetry on 540 kHz
 
 
•
 
 kHz (Bathymetry on 540 kHz) 
540/850
 
 SYSTEM OPTIONS: 
2205
•
 
 480 GB (std) or 1TB Solid State Drive (SSD)within 2200/2205 electronics 
 
•
 
RS232 (bidirectional) Serial Port (4 available; dependent on available connectors)
 
 
•
 
EdgeTech MRU (note: will require use of one of the RS-232 serial ports) 
 
SYSTEM TRIGGERS: 
Non
-
Optically isolated triggers are software programmable. Availability of all triggers is dependent on connector 
configuration.
 
•
 
Trigger A (output, default)
 
 
•
 
Trigger B (input, default) wired to MCIL8 ethernet/power bukhead
 
 
•
 
Trigger C (user defined, input or 
output)
 
 
•
 
Optical Isolation available (triggers not software programmable) 
 
 
 
 
 

	CONFIGURABLE ITEM 	SELECTION 
	2205 PRESSURE HOUSINGS (SS/SB) 

	Side Scan/Sub-Bottom pressure housings are available in Aluminum and Titanium. The standard end cap supports a 13 pin Ethernet/Power/Trigger B I/O Interface, Side Scan (2), Sub-Bottom (2) and an 8 pin User Defined connector for additional triggers or serial ports. Unused connectors are sealed with pressure rated plugs. Additional bottle and end cap mechanical configurations are available (typical 8-10 week lead time). Add 6” to length to account for cable bend. 

	• 	500m, Aluminum;    5.5” (OD) x 19.8” (length)   ICD 0018854 	 

	• 	3000m, Aluminum;  6.2” (OD) x 20.0” (length)   ICD 0018561 	 

	[bookmark: _GoBack]• 	6000m, Titanium;     5.7” (OD) x 20.0” (length)   ICD 0017887 	 

	2205 BATHY PRESSURE HOUSINGS (SS/SB/BATHY) 

	Side Scan/Bathy pressure housings are available in Aluminum and Titanium. The standard end cap supports a 13 pin Ethernet/Power/Trigger B I/O Interface, Side Scan (2), Bathy (2) and several User Defined connectors for additional triggers or serial ports. Unused connectors are sealed with pressure rated plugs. Additional bottle and end cap mechanical configurations are available (typical 8-10-week lead time). Add 12” to length to account for cable bend. Titanium Bottles are filled with a heat dissipative fluid (Fluorinert). 7075 Aluminum can be used in place of Titanium (to eliminate fluid) but the size will increase. To date, there has not been a lot of standards. The bottles below represent two Aluminum volumes that should be used to meet customer objectives. Alternative bottles are always possible but due to Bathy’s complexity will definitely increase delivery time. The addition of Sub-Bottom will require a nominal 6” increase in length. 
 

	• 	3000m, Aluminum;   7.2” (OD) x 21” (length)               ICD 0018919 	 

	• 	6000m, Aluminum (7075);    7.95” (OD) x 23” (length)   ICD 0020007 	 
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