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Wire up U1, upside down

Remove D15

Remove R39

add 22awg wire from (F3,D17,C66, TP160)-pad to 3.3V side of C49 to reduce resistance

Add 10k between pin 1 and pin 2 on Freewave Connector

Cut trace to gate of Q1, bluewire TP90 to CPU GPIO connector J12, pin 13

Remove Q4   Q5  Q6

Remove R134   R135

Add connection: U31 pin 1 to D15 - Anode ( EXT_RESET_N )

Swap A3 pins 13 and 14 ( Rx and Tx lines into GNSS-5-CLICK )

Add 22 AWG wire from U31 pin 1 ( 7 NOT pin 1 !! ) to positive junction of C159 and C160

Add 1uF 0603 Caps in parallel with C159, C160, C156, C155

Add 100uF, 100nF and 10nF Cap in parallel with C50

Add 100uF Cap in parallel with C200

R26 is now 909k 0603 1%

R28 is now 274k 0603 1%

R21 is now 237k 0603 1%

Add 0.1uF 0603 cap in parallel with R24

U39 is not installed:
   Add blue wire from CN2-93 to J25-2
   Add blue wire from CN2-95 to J25-3
