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PAROSCI:
Do not install U1 "upside down"; we will not be using this IC

TS4100:
Remove D15
Remove R139
Add 1uF 0603 Caps in parallel with C159, C160, C156, C155

SUPERCAP:
Add 22awg wire from (F3,D17,C66, TP160)-pad to positive side of C49
  ( to reduce resistance )
Remove Q6
Remove Q5
Remove R135
Remove R134
Add blue wire connection: U31 pin 7 to D15 - Anode
  ( EXT_RESET_N )
Add 22 AWG wire from U31 pin 1 to positive junction of C159 and C160
  ( to reduce resistance )
Add 100uF, 100nF and 10nF Cap in parallel with C50
Add 100uF Cap in parallel with C200
R26 is now 909k 0603 1%
R28 is now 274k 0603 1%
R21 is now 237k 0603 1%
Add 0.1uF 0603 cap in parallel with R24

FREEWAVE:
Add 10k resistor between pin 1 and pin 2 on U52 ( Freewave Connector )
Cut trace to gate of Q1, bluewire gate to CPU GPIO connector J12, pin 13 ( CN1-21 )
   ( Pulling the line to ground is required to get the radio into programming mode for setup. )
[bookmark: _GoBack]Add blue wire between TP90 and TP93, restoring the "OFF_BD_RESET_N" net to the UARTs.

GNSS5-CLICK:
Swap A3 pins 13 and 14 ( Rx and Tx lines into GNSS-5-CLICK )
Cut trace from A3 pin 2 ( GNSS_5_CLICK "RESET" ) to signal "OFF_BD_RESET" 

CONSOLE RS232:
U39 is not installed:
   Add blue wire from CN2-93 to J25-2
     ( Same as blue wire U39 pin 9 to 11 )
   Add blue wire from CN2-95 to J25-3
     ( Same as blue wire U39 pin 7 to 6 )

VECTORNAV VN100:
Remove Q4

USB OTG: 
  remove R18

  
