<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.2">
<drawing>
<library>
<description>&lt;b&gt;TS-SOCKET Baseboard layout&lt;/b&gt;&lt;p&gt;

The TS-SOCKET is the standard interconnect format for Technologic Systems' Macrocontroller series of SBCs and Baseboards.  This library is provided to ease Technologic Systems' customers in building their own baseboard for use with the Macrocontroller series of SBCs.
&lt;p&gt;
*NOTE*  This library is provided as-is for customer use with Technologic Systems' Macrocontroller series of SBCs.  Technologic Systems is not responsible for any losses resulting from use of this part library.  Pin assignments and names can vary between products in the Macrocontroller series of SBCs, be sure to check the schematic of the Macrocontroller in order to confirm correct pin assignments.
&lt;p&gt;
&lt;author&gt;Copyright 2010, Technologic Systems&lt;/author&gt;</description>
<packages>
<package name="TS-SOCKET">
</package>
</packages>
<symbols>
<symbol name="TS-SOCKET">
<pin name="L$1.FPGA_JTAG_TMS"/>
<pin name="L$2.EXT_RESET#"/>
<pin name="L$3.FPGA_JTAG_TCK"/>
<pin name="L$4.EN_USB_5V"/>
<pin name="L$5.FPGA_JTAG_TDO"/>
<pin name="L$6.SDCARD_D2"/>
<pin name="L$7.FPGA_JTAG_TDI"/>
<pin name="L$8.SDCARD_D3"/>
<pin name="L$9.OFF_BD_RESET#"/>
<pin name="L$10.SDCARD_CMD"/>
<pin name="L$11.BOOT_OVERRIDE"/>
<pin name="L$12.SDCARD_3.3V"/>
<pin name="L$13.SPIO_CLK"/>
<pin name="L$14.SDCARD_CLK"/>
<pin name="L$15.5V"/>
<pin name="L$16.5V"/>
<pin name="L$17.POWER_FAIL#"/>
<pin name="L$18.SDCARD_D0"/>
<pin name="L$19.LCD_D08"/>
<pin name="L$20.SDCARD_D1"/>
<pin name="L$21.LCD_D09"/>
<pin name="L$22.SER_FLASH_WP#"/>
<pin name="L$23.LCD_10"/>
<pin name="L$24.LCD_D00"/>
<pin name="L$25.LCD_D11"/>
<pin name="L$26.LCD_D01"/>
<pin name="L$27.LCD_D12"/>
<pin name="L$28.LCD_D02"/>
<pin name="L$29.5V"/>
<pin name="L$30.LCD_D03"/>
<pin name="L$31.LCD_D13"/>
<pin name="L$32.LCD_D04"/>
<pin name="L$33.LCD_D14"/>
<pin name="L$34.LCD_D05"/>
<pin name="L$35.LCD_D15"/>
<pin name="L$36.V_BAT"/>
<pin name="L$37.LCD_D16"/>
<pin name="L$38.LCD_D06"/>
<pin name="L$39.LCD_D17"/>
<pin name="L$40.LCD_D07"/>
<pin name="L$41.LCD_D18"/>
<pin name="L$42.LCD_D21"/>
<pin name="L$43.LCD_D19"/>
<pin name="L$44.LCD_D22"/>
<pin name="L$45.LCD_D20"/>
<pin name="L$46.LCD_D23"/>
<pin name="L$47.5V"/>
<pin name="L$48.EN_LCD_3.3V"/>
<pin name="L$49.LCD_CLK"/>
<pin name="L$50"/>
<pin name="L$51.LCD_HSYNC"/>
<pin name="L$52"/>
<pin name="L$53.LCD_VSYNC"/>
<pin name="L$54"/>
<pin name="L$55.LCD_DE"/>
<pin name="L$56"/>
<pin name="L$57.LCD_PWM"/>
<pin name="L$58"/>
<pin name="L$59"/>
<pin name="L$60"/>
<pin name="L$61"/>
<pin name="L$62.GND"/>
<pin name="L$63.DIO"/>
<pin name="L$64.MUX_AD_15"/>
<pin name="L$65.DIO"/>
<pin name="L$66.MUX_AD_14"/>
<pin name="L$67.DIO"/>
<pin name="L$68.MUX_AD_13"/>
<pin name="L$69.DIO"/>
<pin name="L$70.MUX_AD_12"/>
<pin name="L$71.DIO"/>
<pin name="L$72.MUX_AD_11"/>
<pin name="L$73.DIO"/>
<pin name="L$74.MUX_AD_10"/>
<pin name="L$75.GND"/>
<pin name="L$76.MUX_AD_09"/>
<pin name="L$77.DIO"/>
<pin name="L$78.MUX_AD_08"/>
<pin name="L$79.DIO"/>
<pin name="L$80.MUX_AD_07"/>
<pin name="L$81.DIO"/>
<pin name="L$82.MUX_AD_06"/>
<pin name="L$83.DIO"/>
<pin name="L$84.MUX_AD_05"/>
<pin name="L$85.DIO"/>
<pin name="L$86.MUX_AD_04"/>
<pin name="L$87.DIO"/>
<pin name="L$88.MUX_AD_03"/>
<pin name="L$89.DIO"/>
<pin name="L$90.MUX_AD_02"/>
<pin name="L$91.DIO"/>
<pin name="L$92.MUX_AD_01"/>
<pin name="L$93.DIO"/>
<pin name="L$94.MUX_AD_00"/>
<pin name="L$95.GND"/>
<pin name="L$96.BUS_ALE#"/>
<pin name="L$97.BUS_WAIT#"/>
<pin name="L$98.BUS_DIR"/>
<pin name="L$99.BUS_BHE#"/>
<pin name="L$100.BUS_CS#"/>
<pin name="R$1.ETH_RX+"/>
<pin name="R$2.ETH_LEFT_LED"/>
<pin name="R$3..ETH_RX-"/>
<pin name="R$4.ETH_RIGHT_LED"/>
<pin name="R$5.ETH_CT"/>
<pin name="R$6.RED_LED#"/>
<pin name="R$7..ETH_TX+"/>
<pin name="R$8.GREEN_LED#"/>
<pin name="R$9.ETH_TX-"/>
<pin name="R$10.MFP_105"/>
<pin name="R$11.ETH_CT"/>
<pin name="R$12.MFP_106"/>
<pin name="R$13"/>
<pin name="R$14.MFP_122"/>
<pin name="R$15.GND"/>
<pin name="R$16.PC0"/>
<pin name="R$17.SATA_RX-"/>
<pin name="R$18.PC1"/>
<pin name="R$19.SATA_RX+"/>
<pin name="R$20.PC2"/>
<pin name="R$21.GND"/>
<pin name="R$22.PC3_SPI_CS3#"/>
<pin name="R$23.DEV_USB_M"/>
<pin name="R$24.AN_VREF"/>
<pin name="R$25.DEV_USB_P"/>
<pin name="R$26.MFP_84"/>
<pin name="R$27.1.0V_BU"/>
<pin name="R$28.I2C_CLK"/>
<pin name="R$29.HOSTA_USB_M"/>
<pin name="R$30.I2C_DAT"/>
<pin name="R$31.HOSTA_USB_P"/>
<pin name="R$32.MFP_104"/>
<pin name="R$33.CPU_CORE"/>
<pin name="R$34.AUD_MCLK"/>
<pin name="R$35.USB_OTG_M"/>
<pin name="R$36.AUD_CLK"/>
<pin name="R$37.USB_OTG_P"/>
<pin name="R$38.AUD_FRM"/>
<pin name="R$39.3.3V"/>
<pin name="R$40.AUD_TXD"/>
<pin name="R$41"/>
<pin name="R$42.AUD_RXD"/>
<pin name="R$43"/>
<pin name="R$44.CPU_JTAG_TMS"/>
<pin name="R$45.GND"/>
<pin name="R$46.CPU_JTAG_TCK"/>
<pin name="R$47.PCIE_TXD-"/>
<pin name="R$48.CPU_JTAG_TDI"/>
<pin name="R$49.PCIE_TXD+"/>
<pin name="R$50.CPU_JTAG_TDO"/>
<pin name="R$51.GND"/>
<pin name="R$52.CAM_PCLK"/>
<pin name="R$53.PCIE_RXD-"/>
<pin name="R$54.CAM_VCLK"/>
<pin name="R$55.PCIE_RXD+"/>
<pin name="R$56.CAM_MCLK"/>
<pin name="R$57.DDR_1.8V"/>
<pin name="R$58.CAM_D0"/>
<pin name="R$59.PCIE_CLK-"/>
<pin name="R$60.CAM_D1"/>
<pin name="R$61.PCIE_CLK+"/>
<pin name="R$62.CAM_D2"/>
<pin name="R$63.1.2V"/>
<pin name="R$64.CAM_D5"/>
<pin name="R$65.SPI_FRM"/>
<pin name="R$66.CAM_D6"/>
<pin name="R$67.SPI_MOSI"/>
<pin name="R$68.CAM_D7"/>
<pin name="R$69.SPI_MISO"/>
<pin name="R$70.CAM_HSYNC"/>
<pin name="R$71.SPI_CLK"/>
<pin name="R$72.CAM_VSYNC"/>
<pin name="R$73.GND"/>
<pin name="R$74.USB_OTG_ID"/>
<pin name="R$75.PC4_SPI_CS2#"/>
<pin name="R$76.USB_5V_LINE"/>
<pin name="R$77.PC5_SPI_CS1#"/>
<pin name="R$78.UART0_TXD"/>
<pin name="R$79.CPU_JTAG_VCC"/>
<pin name="R$80.UART0_RXD"/>
<pin name="R$81.CAM_D3"/>
<pin name="R$82.UART1_TXD"/>
<pin name="R$83.CAM_D4"/>
<pin name="R$84.UART1_RXD"/>
<pin name="R$85.MFP_49"/>
<pin name="R$86.UART2_TXD"/>
<pin name="R$87.MFP_51"/>
<pin name="R$88.UART2_RXD"/>
<pin name="R$89.MFP_52"/>
<pin name="R$90.UART3_TXD"/>
<pin name="R$91.MFP_43"/>
<pin name="R$92.UART3_RXD"/>
<pin name="R$93.DEBUG_TXD"/>
<pin name="R$94.UART4_TXD"/>
<pin name="R$95.DEBUG_RXD"/>
<pin name="R$96.UART4_RXD"/>
<pin name="R$97.CAN_TXD"/>
<pin name="R$98.UART5_TXD"/>
<pin name="R$99.CAN_RXD"/>
<pin name="R$100.UART5_RXD"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="TS-SOCKET">
<description>TS-SOCKET Baseboard layout</description>
<gates>
<gate name="G$1" symbol="TS-SOCKET"/>
</gates>
<devices>
<device name="" package="TS-SOCKET">
<connects>
<connect gate="G$1" pin="L$1.FPGA_JTAG_TMS" pad="L$1"/>
<connect gate="G$1" pin="L$10.SDCARD_CMD" pad="L$10"/>
<connect gate="G$1" pin="L$100.BUS_CS#" pad="L$100"/>
<connect gate="G$1" pin="L$11.BOOT_OVERRIDE" pad="L$11"/>
<connect gate="G$1" pin="L$12.SDCARD_3.3V" pad="L$12"/>
<connect gate="G$1" pin="L$13.SPIO_CLK" pad="L$13"/>
<connect gate="G$1" pin="L$14.SDCARD_CLK" pad="L$14"/>
<connect gate="G$1" pin="L$15.5V" pad="L$15"/>
<connect gate="G$1" pin="L$16.5V" pad="L$16"/>
<connect gate="G$1" pin="L$17.POWER_FAIL#" pad="L$17"/>
<connect gate="G$1" pin="L$18.SDCARD_D0" pad="L$18"/>
<connect gate="G$1" pin="L$19.LCD_D08" pad="L$19"/>
<connect gate="G$1" pin="L$2.EXT_RESET#" pad="L$2"/>
<connect gate="G$1" pin="L$20.SDCARD_D1" pad="L$20"/>
<connect gate="G$1" pin="L$21.LCD_D09" pad="L$21"/>
<connect gate="G$1" pin="L$22.SER_FLASH_WP#" pad="L$22"/>
<connect gate="G$1" pin="L$23.LCD_10" pad="L$23"/>
<connect gate="G$1" pin="L$24.LCD_D00" pad="L$24"/>
<connect gate="G$1" pin="L$25.LCD_D11" pad="L$25"/>
<connect gate="G$1" pin="L$26.LCD_D01" pad="L$26"/>
<connect gate="G$1" pin="L$27.LCD_D12" pad="L$27"/>
<connect gate="G$1" pin="L$28.LCD_D02" pad="L$28"/>
<connect gate="G$1" pin="L$29.5V" pad="L$29"/>
<connect gate="G$1" pin="L$3.FPGA_JTAG_TCK" pad="L$3"/>
<connect gate="G$1" pin="L$30.LCD_D03" pad="L$30"/>
<connect gate="G$1" pin="L$31.LCD_D13" pad="L$31"/>
<connect gate="G$1" pin="L$32.LCD_D04" pad="L$32"/>
<connect gate="G$1" pin="L$33.LCD_D14" pad="L$33"/>
<connect gate="G$1" pin="L$34.LCD_D05" pad="L$34"/>
<connect gate="G$1" pin="L$35.LCD_D15" pad="L$35"/>
<connect gate="G$1" pin="L$36.V_BAT" pad="L$36"/>
<connect gate="G$1" pin="L$37.LCD_D16" pad="L$37"/>
<connect gate="G$1" pin="L$38.LCD_D06" pad="L$38"/>
<connect gate="G$1" pin="L$39.LCD_D17" pad="L$39"/>
<connect gate="G$1" pin="L$4.EN_USB_5V" pad="L$4"/>
<connect gate="G$1" pin="L$40.LCD_D07" pad="L$40"/>
<connect gate="G$1" pin="L$41.LCD_D18" pad="L$41"/>
<connect gate="G$1" pin="L$42.LCD_D21" pad="L$42"/>
<connect gate="G$1" pin="L$43.LCD_D19" pad="L$43"/>
<connect gate="G$1" pin="L$44.LCD_D22" pad="L$44"/>
<connect gate="G$1" pin="L$45.LCD_D20" pad="L$45"/>
<connect gate="G$1" pin="L$46.LCD_D23" pad="L$46"/>
<connect gate="G$1" pin="L$47.5V" pad="L$47"/>
<connect gate="G$1" pin="L$48.EN_LCD_3.3V" pad="L$48"/>
<connect gate="G$1" pin="L$49.LCD_CLK" pad="L$49"/>
<connect gate="G$1" pin="L$5.FPGA_JTAG_TDO" pad="L$5"/>
<connect gate="G$1" pin="L$50" pad="L$50"/>
<connect gate="G$1" pin="L$51.LCD_HSYNC" pad="L$51"/>
<connect gate="G$1" pin="L$52" pad="L$52"/>
<connect gate="G$1" pin="L$53.LCD_VSYNC" pad="L$53"/>
<connect gate="G$1" pin="L$54" pad="L$54"/>
<connect gate="G$1" pin="L$55.LCD_DE" pad="L$55"/>
<connect gate="G$1" pin="L$56" pad="L$56"/>
<connect gate="G$1" pin="L$57.LCD_PWM" pad="L$57"/>
<connect gate="G$1" pin="L$58" pad="L$58"/>
<connect gate="G$1" pin="L$59" pad="L$59"/>
<connect gate="G$1" pin="L$6.SDCARD_D2" pad="L$6"/>
<connect gate="G$1" pin="L$60" pad="L$60"/>
<connect gate="G$1" pin="L$61" pad="L$61"/>
<connect gate="G$1" pin="L$62.GND" pad="L$62"/>
<connect gate="G$1" pin="L$63.DIO" pad="L$63"/>
<connect gate="G$1" pin="L$64.MUX_AD_15" pad="L$64"/>
<connect gate="G$1" pin="L$65.DIO" pad="L$65"/>
<connect gate="G$1" pin="L$66.MUX_AD_14" pad="L$66"/>
<connect gate="G$1" pin="L$67.DIO" pad="L$67"/>
<connect gate="G$1" pin="L$68.MUX_AD_13" pad="L$68"/>
<connect gate="G$1" pin="L$69.DIO" pad="L$69"/>
<connect gate="G$1" pin="L$7.FPGA_JTAG_TDI" pad="L$7"/>
<connect gate="G$1" pin="L$70.MUX_AD_12" pad="L$70"/>
<connect gate="G$1" pin="L$71.DIO" pad="L$71"/>
<connect gate="G$1" pin="L$72.MUX_AD_11" pad="L$72"/>
<connect gate="G$1" pin="L$73.DIO" pad="L$73"/>
<connect gate="G$1" pin="L$74.MUX_AD_10" pad="L$74"/>
<connect gate="G$1" pin="L$75.GND" pad="L$75"/>
<connect gate="G$1" pin="L$76.MUX_AD_09" pad="L$76"/>
<connect gate="G$1" pin="L$77.DIO" pad="L$77"/>
<connect gate="G$1" pin="L$78.MUX_AD_08" pad="L$78"/>
<connect gate="G$1" pin="L$79.DIO" pad="L$79"/>
<connect gate="G$1" pin="L$8.SDCARD_D3" pad="L$8"/>
<connect gate="G$1" pin="L$80.MUX_AD_07" pad="L$80"/>
<connect gate="G$1" pin="L$81.DIO" pad="L$81"/>
<connect gate="G$1" pin="L$82.MUX_AD_06" pad="L$82"/>
<connect gate="G$1" pin="L$83.DIO" pad="L$83"/>
<connect gate="G$1" pin="L$84.MUX_AD_05" pad="L$84"/>
<connect gate="G$1" pin="L$85.DIO" pad="L$85"/>
<connect gate="G$1" pin="L$86.MUX_AD_04" pad="L$86"/>
<connect gate="G$1" pin="L$87.DIO" pad="L$87"/>
<connect gate="G$1" pin="L$88.MUX_AD_03" pad="L$88"/>
<connect gate="G$1" pin="L$89.DIO" pad="L$89"/>
<connect gate="G$1" pin="L$9.OFF_BD_RESET#" pad="L$9"/>
<connect gate="G$1" pin="L$90.MUX_AD_02" pad="L$90"/>
<connect gate="G$1" pin="L$91.DIO" pad="L$91"/>
<connect gate="G$1" pin="L$92.MUX_AD_01" pad="L$92"/>
<connect gate="G$1" pin="L$93.DIO" pad="L$93"/>
<connect gate="G$1" pin="L$94.MUX_AD_00" pad="L$94"/>
<connect gate="G$1" pin="L$95.GND" pad="L$95"/>
<connect gate="G$1" pin="L$96.BUS_ALE#" pad="L$96"/>
<connect gate="G$1" pin="L$97.BUS_WAIT#" pad="L$97"/>
<connect gate="G$1" pin="L$98.BUS_DIR" pad="L$98"/>
<connect gate="G$1" pin="L$99.BUS_BHE#" pad="L$99"/>
<connect gate="G$1" pin="R$1.ETH_RX+" pad="R$1"/>
<connect gate="G$1" pin="R$10.MFP_105" pad="R$10"/>
<connect gate="G$1" pin="R$100.UART5_RXD" pad="R$100"/>
<connect gate="G$1" pin="R$11.ETH_CT" pad="R$11"/>
<connect gate="G$1" pin="R$12.MFP_106" pad="R$12"/>
<connect gate="G$1" pin="R$13" pad="R$13"/>
<connect gate="G$1" pin="R$14.MFP_122" pad="R$14"/>
<connect gate="G$1" pin="R$15.GND" pad="R$15"/>
<connect gate="G$1" pin="R$16.PC0" pad="R$16"/>
<connect gate="G$1" pin="R$17.SATA_RX-" pad="R$17"/>
<connect gate="G$1" pin="R$18.PC1" pad="R$18"/>
<connect gate="G$1" pin="R$19.SATA_RX+" pad="R$19"/>
<connect gate="G$1" pin="R$2.ETH_LEFT_LED" pad="R$2"/>
<connect gate="G$1" pin="R$20.PC2" pad="R$20"/>
<connect gate="G$1" pin="R$21.GND" pad="R$21"/>
<connect gate="G$1" pin="R$22.PC3_SPI_CS3#" pad="R$22"/>
<connect gate="G$1" pin="R$23.DEV_USB_M" pad="R$23"/>
<connect gate="G$1" pin="R$24.AN_VREF" pad="R$24"/>
<connect gate="G$1" pin="R$25.DEV_USB_P" pad="R$25"/>
<connect gate="G$1" pin="R$26.MFP_84" pad="R$26"/>
<connect gate="G$1" pin="R$27.1.0V_BU" pad="R$27"/>
<connect gate="G$1" pin="R$28.I2C_CLK" pad="R$28"/>
<connect gate="G$1" pin="R$29.HOSTA_USB_M" pad="R$29"/>
<connect gate="G$1" pin="R$3..ETH_RX-" pad="R$3"/>
<connect gate="G$1" pin="R$30.I2C_DAT" pad="R$30"/>
<connect gate="G$1" pin="R$31.HOSTA_USB_P" pad="R$31"/>
<connect gate="G$1" pin="R$32.MFP_104" pad="R$32"/>
<connect gate="G$1" pin="R$33.CPU_CORE" pad="R$33"/>
<connect gate="G$1" pin="R$34.AUD_MCLK" pad="R$34"/>
<connect gate="G$1" pin="R$35.USB_OTG_M" pad="R$35"/>
<connect gate="G$1" pin="R$36.AUD_CLK" pad="R$36"/>
<connect gate="G$1" pin="R$37.USB_OTG_P" pad="R$37"/>
<connect gate="G$1" pin="R$38.AUD_FRM" pad="R$38"/>
<connect gate="G$1" pin="R$39.3.3V" pad="R$39"/>
<connect gate="G$1" pin="R$4.ETH_RIGHT_LED" pad="R$4"/>
<connect gate="G$1" pin="R$40.AUD_TXD" pad="R$40"/>
<connect gate="G$1" pin="R$41" pad="R$41"/>
<connect gate="G$1" pin="R$42.AUD_RXD" pad="R$42"/>
<connect gate="G$1" pin="R$43" pad="R$43"/>
<connect gate="G$1" pin="R$44.CPU_JTAG_TMS" pad="R$44"/>
<connect gate="G$1" pin="R$45.GND" pad="R$45"/>
<connect gate="G$1" pin="R$46.CPU_JTAG_TCK" pad="R$46"/>
<connect gate="G$1" pin="R$47.PCIE_TXD-" pad="R$47"/>
<connect gate="G$1" pin="R$48.CPU_JTAG_TDI" pad="R$48"/>
<connect gate="G$1" pin="R$49.PCIE_TXD+" pad="R$49"/>
<connect gate="G$1" pin="R$5.ETH_CT" pad="R$5"/>
<connect gate="G$1" pin="R$50.CPU_JTAG_TDO" pad="R$50"/>
<connect gate="G$1" pin="R$51.GND" pad="R$51"/>
<connect gate="G$1" pin="R$52.CAM_PCLK" pad="R$52"/>
<connect gate="G$1" pin="R$53.PCIE_RXD-" pad="R$53"/>
<connect gate="G$1" pin="R$54.CAM_VCLK" pad="R$54"/>
<connect gate="G$1" pin="R$55.PCIE_RXD+" pad="R$55"/>
<connect gate="G$1" pin="R$56.CAM_MCLK" pad="R$56"/>
<connect gate="G$1" pin="R$57.DDR_1.8V" pad="R$57"/>
<connect gate="G$1" pin="R$58.CAM_D0" pad="R$58"/>
<connect gate="G$1" pin="R$59.PCIE_CLK-" pad="R$59"/>
<connect gate="G$1" pin="R$6.RED_LED#" pad="R$6"/>
<connect gate="G$1" pin="R$60.CAM_D1" pad="R$60"/>
<connect gate="G$1" pin="R$61.PCIE_CLK+" pad="R$61"/>
<connect gate="G$1" pin="R$62.CAM_D2" pad="R$62"/>
<connect gate="G$1" pin="R$63.1.2V" pad="R$63"/>
<connect gate="G$1" pin="R$64.CAM_D5" pad="R$64"/>
<connect gate="G$1" pin="R$65.SPI_FRM" pad="R$65"/>
<connect gate="G$1" pin="R$66.CAM_D6" pad="R$66"/>
<connect gate="G$1" pin="R$67.SPI_MOSI" pad="R$67"/>
<connect gate="G$1" pin="R$68.CAM_D7" pad="R$68"/>
<connect gate="G$1" pin="R$69.SPI_MISO" pad="R$69"/>
<connect gate="G$1" pin="R$7..ETH_TX+" pad="R$7"/>
<connect gate="G$1" pin="R$70.CAM_HSYNC" pad="R$70"/>
<connect gate="G$1" pin="R$71.SPI_CLK" pad="R$71"/>
<connect gate="G$1" pin="R$72.CAM_VSYNC" pad="R$72"/>
<connect gate="G$1" pin="R$73.GND" pad="R$73"/>
<connect gate="G$1" pin="R$74.USB_OTG_ID" pad="R$74"/>
<connect gate="G$1" pin="R$75.PC4_SPI_CS2#" pad="R$75"/>
<connect gate="G$1" pin="R$76.USB_5V_LINE" pad="R$76"/>
<connect gate="G$1" pin="R$77.PC5_SPI_CS1#" pad="R$77"/>
<connect gate="G$1" pin="R$78.UART0_TXD" pad="R$78"/>
<connect gate="G$1" pin="R$79.CPU_JTAG_VCC" pad="R$79"/>
<connect gate="G$1" pin="R$8.GREEN_LED#" pad="R$8"/>
<connect gate="G$1" pin="R$80.UART0_RXD" pad="R$80"/>
<connect gate="G$1" pin="R$81.CAM_D3" pad="R$81"/>
<connect gate="G$1" pin="R$82.UART1_TXD" pad="R$82"/>
<connect gate="G$1" pin="R$83.CAM_D4" pad="R$83"/>
<connect gate="G$1" pin="R$84.UART1_RXD" pad="R$84"/>
<connect gate="G$1" pin="R$85.MFP_49" pad="R$85"/>
<connect gate="G$1" pin="R$86.UART2_TXD" pad="R$86"/>
<connect gate="G$1" pin="R$87.MFP_51" pad="R$87"/>
<connect gate="G$1" pin="R$88.UART2_RXD" pad="R$88"/>
<connect gate="G$1" pin="R$89.MFP_52" pad="R$89"/>
<connect gate="G$1" pin="R$9.ETH_TX-" pad="R$9"/>
<connect gate="G$1" pin="R$90.UART3_TXD" pad="R$90"/>
<connect gate="G$1" pin="R$91.MFP_43" pad="R$91"/>
<connect gate="G$1" pin="R$92.UART3_RXD" pad="R$92"/>
<connect gate="G$1" pin="R$93.DEBUG_TXD" pad="R$93"/>
<connect gate="G$1" pin="R$94.UART4_TXD" pad="R$94"/>
<connect gate="G$1" pin="R$95.DEBUG_RXD" pad="R$95"/>
<connect gate="G$1" pin="R$96.UART4_RXD" pad="R$96"/>
<connect gate="G$1" pin="R$97.CAN_TXD" pad="R$97"/>
<connect gate="G$1" pin="R$98.UART5_TXD" pad="R$98"/>
<connect gate="G$1" pin="R$99.CAN_RXD" pad="R$99"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
