/**********************************************************************
* $Id$		abstract.txt 			
*//**
* @file		abstract.txt 
* @brief	Example description file
* @version	2.0
* @date		
* @author	NXP MCU SW Application Team/Micromint USA Support
*
* Copyright(C) 2010, NXP Semiconductor
* All rights reserved.
*
***********************************************************************
* Software that is described herein is for illustrative purposes only
* which provides customers with programming information regarding the
* products. This software is supplied "AS IS" without any warranties.
* NXP Semiconductors assumes no responsibility or liability for the
* use of the software, conveys no license or title under any patent,
* copyright, or mask work right to the product. NXP Semiconductors
* reserves the right to make changes in the software without
* notification. NXP Semiconductors also make no representation or
* warranty that such application will be suitable for the specified
* use without further testing or modification.
**********************************************************************/
  
@Example description:
Purpose:
	This example describes how to test GPDMA function by transferring data
	from Flash to Ram memory
Process:
	This example will transfer a block of data from Flash memory to Ram 
        memory.	Transferred block is initialized by defining const array 
        'DMAScr_Buffer'. This buffer will be burned into flash when compile. 
        Received block data is 'DMADest_Buffer' will be stored in ram when 
        compile. GPDMA channel 0 is configured in this example.	Transfer size is
        16 words. After transferring completed, "Buffer_Verify()" will be called
        to compare data block in memory source and destination. If not similar, 
        program will enter infinite loop. Open serial display to see DMA 
        transfer result.
					
@Directory contents:
	\EWARM: includes EWARM (IAR) project and configuration files
	\Keil:	includes RVMDK (Keil)project and configuration files 
	
	lpc17xx_libcfg.h: Library configuration file - include needed driver 
        library for this example 
	makefile: Example's makefile (to build with GNU toolchain)
	flash_2_ram.c: Main program

@How to run:
Hardware configuration:		
     Serial display configuration:(e.g: TeraTerm, Hyperterminal, Flash Magic...) 
		– 115200bps 
		– 8 data bit 
		– No parity 
		– 1 stop bit 
		– No flow control 
	
Running mode:
This example can run on RAM/ROM mode.

Step to run:
	- Step 1: Build example.
	- Step 2: Burn hex file into board (if run on ROM mode)
	- Step 3: Connect COM1 on the Lincoln board to COM port on your computer
	- Step 4: Configure hardware and serial display as above instruction 
	- Step 5: Run example and observe DMA result on serial display
				
@Tip:
	- Open \EWARM\*.eww project file to run example on IAR
	- Open \RVMDK\*.uvproj project file to run example on Keil