/**********************************************************************
* $Id$		abstract.txt 			
*//**
* @file		abstract.txt 
* @brief	Example description file
* @version	2.0
* @date		
* @author	NXP MCU SW Application Team/Micromint USA Support
* Copyright(C) 2010, NXP Semiconductor
* All rights reserved.
*
***********************************************************************
* Software that is described herein is for illustrative purposes only
* which provides customers with programming information regarding the
* products. This software is supplied "AS IS" without any warranties.
* NXP Semiconductors assumes no responsibility or liability for the
* use of the software, conveys no license or title under any patent,
* copyright, or mask work right to the product. NXP Semiconductors
* reserves the right to make changes in the software without
* notification. NXP Semiconductors also make no representation or
* warranty that such application will be suitable for the specified
* use without further testing or modification.
**********************************************************************/
  
@Example description:
Purpose:
  This example describes how to use ADC conversion in polling mode.

Process:
  An analog voltage needs to be applied to AD0.2 (J7 pin 5) on the Lincoln.
  The ADC conversion rate is 200KHz. A fully accurate conversion 
  requires 65 of these clocks. So ADC clock = 200KHz * 65 = 13MHz. Note that 
  maximum ADC clock input is 13MHz.    
	
  After start ADC operation, polling "DONE" bit. If "DONE" bit is set, store 
  ADC converted data in "adc_value" and display this data via UART0 and 
  re-start ADC for next conversion.
			
  Adjust the analog voltage to change ADC signal input.

@Directory contents:
  \EWARM: includes EWARM (IAR) project and configuration files
  \Keil:	includes RVMDK (Keil)project and configuration files 
	
  lpc17xx_libcfg.h: Library configuration file - include needed driver library
  for this example makefile: Example's makefile (to build with GNU toolchain)
  adc_polling_test.c: Main program

@How to run:
				
Serial display configuration: (e.g: TeraTerm, Hyperterminal, Flash Magic...) 
	– 115200bps 
	– 8 data bit 
	– No parity 
	– 1 stop bit 
	– No flow control 
	
Running mode:
	This example can run on RAM/ROM mode.
	
Step to run:
  - Step 1: Build example.
  - Step 2: Burn hex file into board (if run on ROM mode)
  - Step 3: Connect COM1 on the Lincoln board to COM port on your computer
  - Step 4: Configure the serial display as above instruction 
  - Step 5: Run example, turn potetiometer and observe data on serial display
		
(Pls see "LPC17xx Example Description" document - chapter 
 "Examples > ADC > Polling" for more details)
		
@Tip:
	- Open \EWARM\*.eww project file to run example on IAR
	- Open \RVMDK\*.uvproj project file to run example on Keil