# Static Call Graph for image .\Flash\uart_rs485_slave.axf

#<CALLGRAPH># ARM Linker, 4.1 [Build 644]: Last Updated: Tue Jan 17 15:08:42 2012

### Maximum Stack Usage = 216 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ c_entry ⇒ UART_Init ⇒ uart_set_divisors ⇒ __aeabi_uldivmod

### Mutually Recursive functions

- NMI_Handler ⇒ NMI_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- BusFault_Handler ⇒ BusFault_Handler
- UsageFault_Handler ⇒ UsageFault_Handler
- SVC_Handler ⇒ SVC_Handler
- DebugMon_Handler ⇒ DebugMon_Handler
- PendSV_Handler ⇒ PendSV_Handler
- SysTick_Handler ⇒ SysTick_Handler
- ADC_IRQHandler ⇒ ADC_IRQHandler

  ### Function Pointers

  - ADC_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - BOD_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - BusFault_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - CANActivity_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - CAN_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - DMA_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - DebugMon_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - EINT0_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - EINT1_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - EINT2_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - EINT3_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - ENET_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - HardFault_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - I2C0_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - I2C1_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - I2C2_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - I2S_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - MCPWM_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - MemManage_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - NMI_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - PLL0_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - PLL1_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - PWM1_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - PendSV_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - QEI_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - RIT_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - RTC_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - Reset_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - SPI_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - SSP0_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - SSP1_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - SVC_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - SysTick_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - SystemInit from system_lpc17xx.o(.text) referenced from startup_lpc17xx.o(.text)
  - TIMER0_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - TIMER1_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - TIMER2_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - TIMER3_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - UART0_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - UART1_IRQHandler from rs485_slave.o(.text) referenced from startup_lpc17xx.o(RESET)
  - UART2_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - UART3_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - USBActivity_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - USB_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - UsageFault_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - WDT_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_lpc17xx.o(.text)
  - main from rs485_slave.o(.text) referenced from entry7.o(.ARM.Collect$$$$00000007)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry7.o(.ARM.Collect$$$$00000007))

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> SVC_Handler
  [Called By]
  - >> SVC_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> DebugMon_Handler
  [Called By]
  - >> DebugMon_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> SysTick_Handler
  [Called By]
  - >> SysTick_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  ADC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> ADC_IRQHandler
  [Called By]
  - >> ADC_IRQHandler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  BOD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  CANActivity_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  CAN_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  DMA_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  EINT0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  EINT1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  EINT2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  EINT3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  ENET_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  I2C0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  I2C1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  I2C2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  I2S_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  MCPWM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  PLL0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  PLL1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  PWM1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  QEI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  RIT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  SPI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  SSP0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  SSP1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  TIMER0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  TIMER1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  TIMER2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  TIMER3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  UART0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  UART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  UART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  USBActivity_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  USB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  WDT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  CLKPWR_SetPCLKDiv (Thumb, 106 bytes, Stack size 8 bytes, lpc17xx_clkpwr.o(.text), UNUSED)

  CLKPWR_GetPCLKSEL (Thumb, 34 bytes, Stack size 0 bytes, lpc17xx_clkpwr.o(.text))
  [Called By]

  - >> CLKPWR_GetPCLK

  CLKPWR_GetPCLK (Thumb, 78 bytes, Stack size 16 bytes, lpc17xx_clkpwr.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = CLKPWR_GetPCLK
  [Calls]
  - >> CLKPWR_GetPCLKSEL
  [Called By]
  - >> uart_set_divisors

  CLKPWR_ConfigPPWR (Thumb, 50 bytes, Stack size 0 bytes, lpc17xx_clkpwr.o(.text))
  [Called By]

  - >> UART_DeInit
  - >> UART_Init

  CLKPWR_Sleep (Thumb, 12 bytes, Stack size 0 bytes, lpc17xx_clkpwr.o(.text), UNUSED)

  CLKPWR_DeepSleep (Thumb, 22 bytes, Stack size 0 bytes, lpc17xx_clkpwr.o(.text), UNUSED)

  CLKPWR_PowerDown (Thumb, 22 bytes, Stack size 0 bytes, lpc17xx_clkpwr.o(.text), UNUSED)

  CLKPWR_DeepPowerDown (Thumb, 22 bytes, Stack size 0 bytes, lpc17xx_clkpwr.o(.text), UNUSED)

  __aeabi_uldivmod (Thumb, 100 bytes, Stack size 40 bytes, uldiv.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = __aeabi_uldivmod
  [Calls]
  - >> __aeabi_llsr
  - >> __aeabi_llsl
  [Called By]
  - >> uart_set_divisors

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  SystemCoreClockUpdate (Thumb, 316 bytes, Stack size 0 bytes, system_lpc17xx.o(.text), UNUSED)

  SystemInit (Thumb, 296 bytes, Stack size 0 bytes, system_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(.text)

  PINSEL_ConfigTraceFunc (Thumb, 34 bytes, Stack size 0 bytes, lpc17xx_pinsel.o(.text), UNUSED)

  PINSEL_SetI2C0Pins (Thumb, 22 bytes, Stack size 0 bytes, lpc17xx_pinsel.o(.text), UNUSED)

  PINSEL_ConfigPin (Thumb, 54 bytes, Stack size 8 bytes, lpc17xx_pinsel.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = PINSEL_ConfigPin ⇒ set_ResistorMode
  [Calls]
  - >> set_OpenDrainMode
  - >> set_ResistorMode
  - >> set_PinFunc
  [Called By]
  - >> c_entry

  UART_Init (Thumb, 590 bytes, Stack size 16 bytes, lpc17xx_uart.o(.text))
  [Stack]

  - Max Depth = 176
  - Call Chain = UART_Init ⇒ uart_set_divisors ⇒ __aeabi_uldivmod
  [Calls]
  - >> check_failed
  - >> uart_set_divisors
  - >> CLKPWR_ConfigPPWR
  [Called By]
  - >> c_entry

  UART_TxCmd (Thumb, 136 bytes, Stack size 16 bytes, lpc17xx_uart.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = UART_TxCmd
  [Calls]
  - >> check_failed
  [Called By]
  - >> c_entry
  - >> UART_DeInit

  UART_DeInit (Thumb, 112 bytes, Stack size 8 bytes, lpc17xx_uart.o(.text), UNUSED)
  [Calls]

  - >> check_failed
  - >> UART_TxCmd
  - >> CLKPWR_ConfigPPWR

  UART_ConfigStructInit (Thumb, 22 bytes, Stack size 0 bytes, lpc17xx_uart.o(.text))
  [Called By]

  - >> c_entry

  UART_SendByte (Thumb, 58 bytes, Stack size 16 bytes, lpc17xx_uart.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = UART_SendByte
  [Calls]
  - >> check_failed
  [Called By]
  - >> UART_Send

  UART_ReceiveByte (Thumb, 56 bytes, Stack size 8 bytes, lpc17xx_uart.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = UART_ReceiveByte
  [Calls]
  - >> check_failed
  [Called By]
  - >> UART_Receive

  UART_Send (Thumb, 198 bytes, Stack size 56 bytes, lpc17xx_uart.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = UART_Send ⇒ UART_SendByte
  [Calls]
  - >> UART_SendByte
  [Called By]
  - >> c_entry
  - >> print_menu
  - >> UART_IntErr
  - >> UART_RS485Send

  UART_Receive (Thumb, 154 bytes, Stack size 40 bytes, lpc17xx_uart.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = UART_Receive ⇒ UART_ReceiveByte
  [Calls]
  - >> UART_ReceiveByte
  [Called By]
  - >> UART_IntErr
  - >> UART_IntReceive

  UART_ForceBreak (Thumb, 68 bytes, Stack size 8 bytes, lpc17xx_uart.o(.text), UNUSED)
  [Calls]

  - >> check_failed

  UART_IntConfig (Thumb, 298 bytes, Stack size 24 bytes, lpc17xx_uart.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = UART_IntConfig
  [Calls]
  - >> check_failed
  [Called By]
  - >> c_entry
  - >> UARTReceive

  UART_GetLineStatus (Thumb, 56 bytes, Stack size 8 bytes, lpc17xx_uart.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = UART_GetLineStatus
  [Calls]
  - >> check_failed
  [Called By]
  - >> UART1_IRQHandler

  UART_GetIntId (Thumb, 52 bytes, Stack size 8 bytes, lpc17xx_uart.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = UART_GetIntId
  [Calls]
  - >> check_failed
  [Called By]
  - >> UART1_IRQHandler

  UART_CheckBusy (Thumb, 18 bytes, Stack size 0 bytes, lpc17xx_uart.o(.text), UNUSED)

  UART_FIFOConfig (Thumb, 272 bytes, Stack size 16 bytes, lpc17xx_uart.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = UART_FIFOConfig
  [Calls]
  - >> check_failed
  [Called By]
  - >> c_entry

  UART_FIFOConfigStructInit (Thumb, 18 bytes, Stack size 0 bytes, lpc17xx_uart.o(.text))
  [Called By]

  - >> c_entry

  UART_ABCmd (Thumb, 210 bytes, Stack size 24 bytes, lpc17xx_uart.o(.text), UNUSED)
  [Calls]

  - >> check_failed

  UART_ABClearIntPending (Thumb, 70 bytes, Stack size 16 bytes, lpc17xx_uart.o(.text), UNUSED)
  [Calls]

  - >> check_failed

  UART_IrDAInvtInputCmd (Thumb, 80 bytes, Stack size 16 bytes, lpc17xx_uart.o(.text), UNUSED)
  [Calls]

  - >> check_failed

  UART_IrDACmd (Thumb, 78 bytes, Stack size 16 bytes, lpc17xx_uart.o(.text), UNUSED)
  [Calls]

  - >> check_failed

  UART_IrDAPulseDivConfig (Thumb, 130 bytes, Stack size 24 bytes, lpc17xx_uart.o(.text), UNUSED)
  [Calls]

  - >> check_failed

  UART_FullModemForcePinState (Thumb, 138 bytes, Stack size 24 bytes, lpc17xx_uart.o(.text), UNUSED)
  [Calls]

  - >> check_failed

  UART_FullModemConfigMode (Thumb, 142 bytes, Stack size 24 bytes, lpc17xx_uart.o(.text), UNUSED)
  [Calls]

  - >> check_failed

  UART_FullModemGetStatus (Thumb, 28 bytes, Stack size 8 bytes, lpc17xx_uart.o(.text), UNUSED)
  [Calls]

  - >> check_failed

  UART_RS485Config (Thumb, 314 bytes, Stack size 16 bytes, lpc17xx_uart.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = UART_RS485Config
  [Calls]
  - >> check_failed
  [Called By]
  - >> c_entry

  UART_RS485ReceiverCmd (Thumb, 32 bytes, Stack size 0 bytes, lpc17xx_uart.o(.text), UNUSED)

  UART_RS485Send (Thumb, 88 bytes, Stack size 32 bytes, lpc17xx_uart.o(.text))
  [Stack]

  - Max Depth = 104
  - Call Chain = UART_RS485Send ⇒ UART_Send ⇒ UART_SendByte
  [Calls]
  - >> UART_Send
  [Called By]
  - >> UART_RS485SendData
  - >> UART_RS485SendSlvAddr

  UART_RS485SendSlvAddr (Thumb, 20 bytes, Stack size 16 bytes, lpc17xx_uart.o(.text), UNUSED)
  [Calls]

  - >> UART_RS485Send

  UART_RS485SendData (Thumb, 24 bytes, Stack size 16 bytes, lpc17xx_uart.o(.text))
  [Stack]

  - Max Depth = 120
  - Call Chain = UART_RS485SendData ⇒ UART_RS485Send ⇒ UART_Send ⇒ UART_SendByte
  [Calls]
  - >> UART_RS485Send
  [Called By]
  - >> c_entry

  UART_IntReceive (Thumb, 76 bytes, Stack size 16 bytes, rs485_slave.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = UART_IntReceive ⇒ UART_Receive ⇒ UART_ReceiveByte
  [Calls]
  - >> UART_Receive
  [Called By]
  - >> UART1_IRQHandler

  UART_IntErr (Thumb, 36 bytes, Stack size 16 bytes, rs485_slave.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = UART_IntErr ⇒ UART_Send ⇒ UART_SendByte
  [Calls]
  - >> UART_Receive
  - >> UART_Send
  [Called By]
  - >> UART1_IRQHandler

  UART1_IRQHandler (Thumb, 56 bytes, Stack size 16 bytes, rs485_slave.o(.text))
  [Stack]

  - Max Depth = 104
  - Call Chain = UART1_IRQHandler ⇒ UART_IntErr ⇒ UART_Send ⇒ UART_SendByte
  [Calls]
  - >> UART_IntErr
  - >> UART_IntReceive
  - >> UART_GetIntId
  - >> UART_GetLineStatus
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  UARTReceive (Thumb, 112 bytes, Stack size 24 bytes, rs485_slave.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = UARTReceive ⇒ UART_IntConfig
  [Calls]
  - >> UART_IntConfig
  [Called By]
  - >> c_entry

  print_menu (Thumb, 16 bytes, Stack size 8 bytes, rs485_slave.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = print_menu ⇒ UART_Send ⇒ UART_SendByte
  [Calls]
  - >> UART_Send
  [Called By]
  - >> c_entry

  c_entry (Thumb, 498 bytes, Stack size 40 bytes, rs485_slave.o(.text))
  [Stack]

  - Max Depth = 216
  - Call Chain = c_entry ⇒ UART_Init ⇒ uart_set_divisors ⇒ __aeabi_uldivmod
  [Calls]
  - >> print_menu
  - >> UARTReceive
  - >> UART_RS485SendData
  - >> UART_RS485Config
  - >> UART_FIFOConfigStructInit
  - >> UART_FIFOConfig
  - >> UART_IntConfig
  - >> UART_Send
  - >> UART_ConfigStructInit
  - >> UART_TxCmd
  - >> UART_Init
  - >> PINSEL_ConfigPin
  [Called By]
  - >> main

  main (Thumb, 4 bytes, Stack size 0 bytes, rs485_slave.o(.text))
  [Stack]

  - Max Depth = 216
  - Call Chain = main ⇒ c_entry ⇒ UART_Init ⇒ uart_set_divisors ⇒ __aeabi_uldivmod
  [Calls]
  - >> c_entry
  [Address Reference Count : 1]
  - entry7.o(.ARM.Collect$$$$00000007)

  check_failed (Thumb, 4 bytes, Stack size 0 bytes, rs485_slave.o(.text))
  [Called By]

  - >> UART_RS485Config
  - >> UART_FullModemGetStatus
  - >> UART_FullModemConfigMode
  - >> UART_FullModemForcePinState
  - >> UART_IrDAPulseDivConfig
  - >> UART_IrDACmd
  - >> UART_IrDAInvtInputCmd
  - >> UART_ABClearIntPending
  - >> UART_ABCmd
  - >> UART_FIFOConfig
  - >> UART_GetIntId
  - >> UART_GetLineStatus
  - >> UART_IntConfig
  - >> UART_ForceBreak
  - >> UART_ReceiveByte
  - >> UART_SendByte
  - >> UART_DeInit
  - >> UART_TxCmd
  - >> UART_Init

  __aeabi_llsl (Thumb, 30 bytes, Stack size 0 bytes, llshl.o(.text))
  [Called By]

  - >> __aeabi_uldivmod
  - >> uart_set_divisors

  _ll_shift_l (Thumb, 0 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)

  __aeabi_llsr (Thumb, 32 bytes, Stack size 0 bytes, llushr.o(.text))
  [Called By]

  - >> __aeabi_uldivmod
  - >> uart_set_divisors

  _ll_ushift_r (Thumb, 0 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  ### Local Symbols

  set_PinFunc (Thumb, 82 bytes, Stack size 20 bytes, lpc17xx_pinsel.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = set_PinFunc
  [Called By]
  - >> PINSEL_ConfigPin

  set_ResistorMode (Thumb, 82 bytes, Stack size 20 bytes, lpc17xx_pinsel.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = set_ResistorMode
  [Called By]
  - >> PINSEL_ConfigPin

  set_OpenDrainMode (Thumb, 54 bytes, Stack size 12 bytes, lpc17xx_pinsel.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = set_OpenDrainMode
  [Called By]
  - >> PINSEL_ConfigPin

  uart_set_divisors (Thumb, 574 bytes, Stack size 120 bytes, lpc17xx_uart.o(.text))
  [Stack]

  - Max Depth = 160
  - Call Chain = uart_set_divisors ⇒ __aeabi_uldivmod
  [Calls]
  - >> __aeabi_llsr
  - >> __aeabi_llsl
  - >> __aeabi_uldivmod
  - >> CLKPWR_GetPCLK
  [Called By]
  - >> UART_Init

  ### Undefined Global Symbols