/**********************************************************************
* $Id$		abstract.txt 			
*//**
* @file		abstract.txt 
* @brief	Example description file
* @version	2.0
* @date		
* @author	NXP MCU SW Application Team/Micromint USA Support
*
* Copyright(C) 2010, NXP Semiconductor
* All rights reserved.
*
***********************************************************************
* Software that is described herein is for illustrative purposes only
* which provides customers with programming information regarding the
* products. This software is supplied "AS IS" without any warranties.
* NXP Semiconductors assumes no responsibility or liability for the
* use of the software, conveys no license or title under any patent,
* copyright, or mask work right to the product. NXP Semiconductors
* reserves the right to make changes in the software without
* notification. NXP Semiconductors also make no representation or
* warranty that such application will be suitable for the specified
* use without further testing or modification.
**********************************************************************/
  
@Example description:
Purpose:
	This is a simple UART example using auto baudrate mode
Process:	
	COM1 is configured as the default settings:
		- Baudrate set to auto mode
 		- 8 data bit
 		- 1 Stop bit
 		- None parity
	After reset,  first, type 'A' or 'a' character to start Auto baud rate 
        mode. Once Auto baud rate mode completed, print welcome screen, then 
        press any key to have it read in from the terminal and returned back to 
        the terminal.
	
Note: If using this example to test with UART1, pls add conversion type 
      (LPC_UART_TypeDef *)LPC_UART1 because UART1 has different structure type

   Ex: UART_Send((LPC_UART_TypeDef *)LPC_UART1, menu1, sizeof(menu1), BLOCKING);

@Directory contents:
\EWARM: includes EWARM (IAR) project and configuration files
\Keil:	includes RVMDK (Keil)project and configuration files 
	
lpc17xx_libcfg.h: Library configuration file - include needed driver library for
this example makefile: Example's makefile (to build with GNU toolchain)
uart_autobaud_test.c: Main program

@How to run:
Hardware configuration:		

Serial display configuration: (e.g: TeraTerm, Hyperterminal, Flash Magic...) 
	– set any baudrate 
	– 8 data bit 
	– No parity 
	– 1 stop bit 
	– No flow control 
        
Running mode:
This example can run on RAM/ROM mode.
					
Step to run:
	- Step 1: Build example.
	- Step 2: Burn hex file into board (if run on ROM mode)
	- Step 3: Connect COM1 on the Lincoln board to COM port on your computer
	- Step 4: Configure hardware and serial display as above instruction 
	- Step 5: Run example:
		+ Chose any baudrate
		+ Press 'A' or 'a' to synchronize
		+ Press any key and see echo on serial display
					
(Pls see "LPC17xx Example Description" document - chapter "Examples > UART > 
AutoBaud" for more details)
		
@Tip:
	- Open \EWARM\*.eww project file to run example on IAR
	- Open \RVMDK\*.uvproj project file to run example on Keil