/**********************************************************************
* $Id$		abstract.txt 			
*//**
* @file		abstract.txt 
* @brief	Example description file
* @version	2.0
* @date		
* @author	NXP MCU SW Application Team
*
* Copyright(C) 2010, NXP Semiconductor
* All rights reserved.
*
***********************************************************************
* Software that is described herein is for illustrative purposes only
* which provides customers with programming information regarding the
* products. This software is supplied "AS IS" without any warranties.
* NXP Semiconductors assumes no responsibility or liability for the
* use of the software, conveys no license or title under any patent,
* copyright, or mask work right to the product. NXP Semiconductors
* reserves the right to make changes in the software without
* notification. NXP Semiconductors also make no representation or
* warranty that such application will be suitable for the specified
* use without further testing or modification.
**********************************************************************/
  
@Example description:
Purpose:
	This example describes how to relocation vetor table.
Process:
	Vector Table will be remapped at new address VTOR_OFFSET.
	In ROM mode: Vector Table will be initialized at 0x00000000
	In RAM mode: Vector Table will be initialized at 0x10000000
	So, we need copy vector table from init address to new address.
	Check VT remapping is successful or not, use SysTick interrupt to blink 
        LEDs on board.
					
@Directory contents:
	\EWARM: includes EWARM (IAR) project and configuration files
	\Keil:	includes RVMDK (Keil)project and configuration files 
	
	lpc17xx_libcfg.h: Library configuration file - include needed driver 
        library for this example 
	makefile: Example's makefile (to build with GNU toolchain)
	vt_relocation.c: Main program

@How to run:
Hardware configuration:		
			
	Serial display configuration:(e.g: TeraTerm, Hyperterminal, Flash Magic...) 
		– 115200bps 
		– 8 data bit 
		– No parity 
		– 1 stop bit 
		– No flow control 

Running mode:
This example can run on RAM/ROM mode.
					
Step to run:
	- Step 1: Build example.
	- Step 2: Burn hex file into board (if run on ROM mode)
	- Step 3: Connect COM1 on the Lincoln board to COM port on your computer
	- Step 4: Configure hardware and serial display as above instruction 
	- Step 5: Run example and see LED1 blinks or not.
	          If it is blinking, Vector Table remapping is successful.
				
@Tip:
	- Open \EWARM\*.eww project file to run example on IAR
	- Open \RVMDK\*.uvproj project file to run example on Keil