/**********************************************************************
* $Id$		abstract.txt 			
*//**
* @file		abstract.txt 
* @brief	Example description file
* @version	2.0
* @date		
* @author	NXP MCU SW Application Team/Micromint USA Support
*
* Copyright(C) 2010, NXP Semiconductor
* All rights reserved.
*
***********************************************************************
* Software that is described herein is for illustrative purposes only
* which provides customers with programming information regarding the
* products. This software is supplied "AS IS" without any warranties.
* NXP Semiconductors assumes no responsibility or liability for the
* use of the software, conveys no license or title under any patent,
* copyright, or mask work right to the product. NXP Semiconductors
* reserves the right to make changes in the software without
* notification. NXP Semiconductors also make no representation or
* warranty that such application will be suitable for the specified
* use without further testing or modification.
**********************************************************************/
  
@Example description:
Purpose:
	This example describes how to use Timer Match to generate different
	delay signals.
Process:
	1) Initialize COM1 and display information menu.
	2) Ask user to input delay time for T1 and T2 (unit in ms)
	   Configure J2 pin 19 (P1.28) as MAT0.0
	3) Configure TIMER0:
		- Prescale register = 100 us.
		- Match register = T1/100us = T1 ms/ 100us = T1*10
		- Interrupt, no stop, no reset timer counter on match.
	4) Timer0 ISR:
		- Stop timer.
		- Reset and synchronize timer and prescal counter.
		- Update new timer match value.
		- Start timer.
	5) Start TIMER0.
	   Press ESC if we intend to test with other frequencies.
	   TIMER0 and TIMER0 interrupt service are de-initialized.

@Directory contents:
	\EWARM: includes EWARM (IAR) project and configuration files
	\Keil:	includes RVMDK (Keil)project and configuration files 
	 
lpc17xx_libcfg.h: Library configuration file - include needed driver library for
this example 
makefile: Example's makefile (to build with GNU toolchain)
gen_diff_delay.c: Main program

@How to run:
Hardware configuration:		
				
Serial display configuration: (e.g: TeraTerm, Hyperterminal, Flash Magic...) 
	– 115200bps 
	– 8 data bit 
	– No parity 
	– 1 stop bit 
	– No flow control 
	
Running mode:
	This example can run on RAM/ROM mode.
					
(Please reference "LPC1000 Software Development Toolchain" - chapter 4 "Creating
and working with LPC1000CMSIS project" for more information)
	
Step to run:
	- Step 1: Build example.
	- Step 2: Burn hex file into board (if run on ROM mode)
	- Step 3: Connect COM1 on the Lincoln board to COM port on your computer
	- Step 4: Configure hardware and serial display as above instruction 
	- Step 5: Run example and observe J2 pin 19 (MAT0.0) waveform by 
                  oscilloscope.

(Pls see "LPC17xx Example Description" document - chapter "Examples > TIMER > 
Gen_Diff_Delay"	for more details)
		
@Tip:
	- Open \EWARM\*.eww project file to run example on IAR
	- Open \RVMDK\*.uvproj project file to run example on Keil