/**********************************************************************
* $Id$		abstract.txt 			
*//**
* @file		abstract.txt 
* @brief	Example description file
* @version	2.0
* @date		
* @author	Micromint USA Support
*
* Copyright(C) 2010, Micromint
* All rights reserved.
*
***********************************************************************
* Software that is described herein is for illustrative purposes only
* which provides customers with programming information regarding the
* products. This software is supplied "AS IS" without any warranties.
* NXP Semiconductors assumes no responsibility or liability for the
* use of the software, conveys no license or title under any patent,
* copyright, or mask work right to the product. NXP Semiconductors
* reserves the right to make changes in the software without
* notification. NXP Semiconductors also make no representation or
* warranty that such application will be suitable for the specified
* use without further testing or modification.
**********************************************************************/
  
@Example description:
Purpose:
	This example describes how to use optional 4 channel 12-Bit SSP DAC on 
        the Lincoln 60.
	
Process:
	Channel VOUT A will outout a triangle wave while VOUT B will be set to 
        1.0V, VOUT C to 2.0V, and VOUT D to 3.0V. 
					
@Directory contents:
	\EWARM: includes EWARM (IAR) project and configuration files
	\Keil:	includes RVMDK (Keil)project and configuration files 

@How to run:
Serial display configuration: (e.g: TeraTerm, Hyperterminal, Flash Magic...) 
	– 115200bps 
	– 8 data bit 
	– No parity 
	– 1 stop bit 
	– No flow control 
	
Running mode:
        This example can run on RAM/ROM mode.
					
Step to run:
	- Step 1: Build example.
	- Step 2: Burn hex file into board (if run on ROM mode)
	- Step 3: Connect COM1 on the Lincoln board to COM port on your computer
	- Step 4: Configure hardware and serial display as above instruction 
	- Step 5: Run example and observe DAC channel VOUT A on pin 1 of J8 by 
                  oscilloscope.
        - Step 6: Measure VOUT B, C, and D (pins 2, 3, and 4 of J8) with a 
                  voltmeter.
                    VOUT B = 1.0V
                    VOUT C = 2.0V
                    VOUT D = 3.0V
                    
@Tip:
	- Open \EWARM\*.eww project file to run example on IAR
	- Open \RVMDK\*.uvproj project file to run example on Keil        