/**********************************************************************
* $Id$		abstract.txt 			
*//**
* @file		abstract.txt 
* @brief	Example description file
* @version	2.0
* @date		
* @author	NXP MCU SW Application Team/Micromint USA Support
*
* Copyright(C) 2010, NXP Semiconductor
* All rights reserved.
*
***********************************************************************
* Software that is described herein is for illustrative purposes only
* which provides customers with programming information regarding the
* products. This software is supplied "AS IS" without any warranties.
* NXP Semiconductors assumes no responsibility or liability for the
* use of the software, conveys no license or title under any patent,
* copyright, or mask work right to the product. NXP Semiconductors
* reserves the right to make changes in the software without
* notification. NXP Semiconductors also make no representation or
* warranty that such application will be suitable for the specified
* use without further testing or modification.
**********************************************************************/
  
@Example description:
Purpose:
	This example describes how to configure System Tick timer to generate 
	interrupt each 10ms
Process:
	In this example, System Tick timer is clocked internal by the CPU clock
	In this case, CPU clock = cclk = 100MHz
	System Tick timer configure:
		- time interval = 10ms
		- Enable System Tick interrupt
	After each 10ms, System Tick will generate interrupt, interrupt service 
        routine 'SysTick_Handler( )' will be invoke and toggle P0.4 pin.
	Use oscilloscope to observe signal on P0.4 and measure time between 
        falling and rising edge, it would be: 10ms.
					
@Directory contents:
	\EWARM: includes EWARM (IAR) project and configuration files
	\Keil:	includes RVMDK (Keil)project and configuration files 
	 
lpc17xx_libcfg.h: Library configuration file - include needed driver library for
this example makefile: Example's makefile (to build with GNU toolchain)
	10ms_base.c: Main program
			
Step to run:
	- Step 1: Build example.
	- Step 2: Burn hex file into board (if run on ROM mode)
	- Step 3: Run example, observe System Tick operation via J2 pin 3 (P0.4)
                  signal

(Pls see "LPC17xx Example Description" document - chapter "Examples > SysTick > 
10ms_base" for more details)
		
@Tip:
	- Open \EWARM\*.eww project file to run example on IAR
	- Open \RVMDK\*.uvproj project file to run example on Keil