/**********************************************************************
* $Id$		abstract.txt 			
*//**
* @file		abstract.txt 
* @brief	Example description file
* @version	2.0
* @date		
* @author	NXP MCU SW Application Team
*
* Copyright(C) 2010, NXP Semiconductor
* All rights reserved.
*
***********************************************************************
* Software that is described herein is for illustrative purposes only
* which provides customers with programming information regarding the
* products. This software is supplied "AS IS" without any warranties.
* NXP Semiconductors assumes no responsibility or liability for the
* use of the software, conveys no license or title under any patent,
* copyright, or mask work right to the product. NXP Semiconductors
* reserves the right to make changes in the software without
* notification. NXP Semiconductors also make no representation or
* warranty that such application will be suitable for the specified
* use without further testing or modification.
**********************************************************************/
  
@Example description:
Purpose:
	This example describes how to handle a  single network interface and 
	contains the IP, ICMP, UDP and TCP protocols. 
Process:
	The uIP TCP/IP stack is an extremely small implementation of the TCP/IP 
	protocol suite intended for embedded systems running low-end 8 or 16-bit 
	microcontrollers. The code size and RAM requirements of uIP is an order 
        of magnitude smaller than other generic TCP/IP stacks today. 
		
	  The uip_webserver implements WEB server.
	  The default IP address is:
	  	192.168.0.100
	  The default router's IP address is:
		192.168.0.1
	  The subnet mask is:
		255.255.255.0
	  IP address on your PC should not be one of these IP addresses above
			
@Directory contents:
\EWARM: includes EWARM (IAR) project and configuration files
\Keil:	includes RVMDK (Keil)project and configuration files	
\apps: contains a few example applications
	+ \dhcpc: Implementation of DHCPC protocol
	+ \hello-world: A small example showing how to write applications with
          protosockets.
	+ \resolv: DNS resolver
	+ \smtp: SMTP E-mail sender
	+ \telnetd: Implementation of TELNET network protocol
	+ \webclient: Implementation of the HTTP client.
	+ \webserver: Implementation of an HTTP server
\common: implement some supported standard functions (printf, serial..) 
 \uip: contains files that implement uIP stack
\lpc17xx_port: include main program
makefile: Example's makefile (to build with GNU toolchain)

@How to run:
Serial display configuration: (e.g: TeraTerm, Hyperterminal, Flash Magic...) 
	– 115200bps 
	– 8 data bit 
	– No parity 
	– 1 stop bit 
	– No flow control 
	
Running mode:
This example can run only on ROM mode.
Step to run:
	- Step 1: Build example.
	- Step 2: Burn hex file into board 
	- Step 3: Connect the Lincoln to the same network the computer is on
	- Step 4: Connect COM1 on the Lincoln board to COM port on your computer
	- Step 5: Configure hardware and serial display as above instruction 
	- Step 7: Reset board, monitor the status via serial display until EMAC 
                  initialized
	- Step 8: Open command prompt window, execute 'ping 192.168.1.100' 
                  command
	- Step 9: Open web browser, access to address "http://192.168.1.100" to 
                  display the content of the webpage.	
		           
@Tip:
	- Open \EWARM\*.eww project file to run example on IAR
	- Open \RVMDK\*.uvproj project file to run example on Keil	
	
			