/**********************************************************************
* $Id$		abstract.txt 			
*//**
* @file		abstract.txt 
* @brief	Example description file
* @version	2.0
* @date		
* @author	NXP MCU SW Application Team
*
* Copyright(C) 2010, NXP Semiconductor
* All rights reserved.
*
***********************************************************************
* Software that is described herein is for illustrative purposes only
* which provides customers with programming information regarding the
* products. This software is supplied "AS IS" without any warranties.
* NXP Semiconductors assumes no responsibility or liability for the
* use of the software, conveys no license or title under any patent,
* copyright, or mask work right to the product. NXP Semiconductors
* reserves the right to make changes in the software without
* notification. NXP Semiconductors also make no representation or
* warranty that such application will be suitable for the specified
* use without further testing or modification.
**********************************************************************/
  
@Example description:
Purpose:
	This example describes how to use PWM Match function in interrupt mode.
Process:
	This program illustrates the PWM signal on 6 Channels in single edge 
        mode. Peripheral clock for PWM: 
        PWM_PCLK = CCLK / 4 = 72MHz/4 = 18MHz and there is no prescale for PWM. 
        The PWM timer/counter clock is at 18MHz. The base rate is set to 256
 	The base PWM frequency is at 18MHz/256 = 70.312 KHz 
        (Period = ~14.22 microsecond)
 	Each PWM channel (1 to 6) will be configured as following:
	    + PWM1.1 = (10/256) (period = 0.56 microsecond) (P1.18) USER LED1
	    + PWM1.2 = (20/256) (period = 1.11 microsecond) (P1.20) J12 pin 21
	    + PWM1.3 = (30/256) (period = 1.67 microsecond) (P2.2)  J2 pin 21
	    + PWM1.4 = (40/256) (period = 2.22 microsecond) (P2.3)  J2 pin 22
	    + PWM1.5 = (50/256) (period = 2.78 microsecond) (P2.4)  J2 pin 23
	    + PWM1.6 = (60/256) (period = 3.33 microsecond) (P2.5)  J2 pin 24
	 Using Oscilloscope to observe the PWM signals
	 Here, PWM1.1 value keeps changing, it will increase by the time from 0 
         to 256 period and restart. Match interrupt for channel 0 is set, when 
         timer of PWM reach to 256 (value of channel 0 match), an interrupt for 
         matching will generate and update the value of PWM1.1, this value will 
         be updated every 4096 match interrupts or:
	 Period * 4096 = 14.22 * 4096 = 58,245 (microsecond)
	 And this value will be reset to 0 after:
	 Period * 4096 * 256 = 14,910,750.72 (microsecond) = ~15 (second)

@Directory contents:
\EWARM: includes EWARM (IAR) project and configuration files
\Keil:	includes RVMDK (Keil)project and configuration files 
	 
lpc17xx_libcfg.h: Library configuration file - include needed driver library for 
this example makefile: Example's makefile (to build with GNU toolchain)
pwm_match_int.c: Main program

@How to run:
Hardware configuration:		
   PWM pin selected:
	Observe PWM wave signal on these pin
		- PWM1.1 (channel 1): P1.18 USER LED1
		- PWM1.2 (channel 2): P1.20 J12 pin 21
		- PWM1.3 (channel 3): P2.2  J2 pin 21
		- PWM1.4 (channel 4): P2.3  J2 pin 22
		- PWM1.5 (channel 5): P2.4  J2 pin 23
		- PWM1.6 (channel 6): P2.5  J2 pin 24
		
	
Running mode:
	This example can run on RAM/ROM mode.
					
(Please reference "LPC1000 Software Development Toolchain" - chapter 4 "Creating
and working with LPC1000CMSIS project" for more information)
	
Step to run:
	- Step 1: Build example.
	- Step 2: Burn hex file into board (if run on ROM mode)
	- Step 3: Configure hardware as above instruction 
	- Step 4: Run example, Use oscilloscope to monitor the wave form 
		
(Pls see "LPC17xx Example Description" document - chapter "Examples > PWM > 
Match_Interrupt" for more details)
		
@Tip:
	- Open \EWARM\*.eww project file to run example on IAR
	- Open \RVMDK\*.uvproj project file to run example on Keil
