/**********************************************************************
* $Id$		abstract.txt 			
*//**
* @file		abstract.txt 
* @brief	Example description file
* @version	2.0
* @date		
* @author	Micromint USA Support
*
* Copyright(C) 2010, Micromint
* All rights reserved.
*
***********************************************************************
* Software that is described herein is for illustrative purposes only
* which provides customers with programming information regarding the
* products. This software is supplied "AS IS" without any warranties.
* NXP Semiconductors assumes no responsibility or liability for the
* use of the software, conveys no license or title under any patent,
* copyright, or mask work right to the product. NXP Semiconductors
* reserves the right to make changes in the software without
* notification. NXP Semiconductors also make no representation or
* warranty that such application will be suitable for the specified
* use without further testing or modification.
**********************************************************************/
  
@Example description:
Purpose:
	This example describes how to use USBHOST on the Lincoln 60 to
	read and write to a USB memory stick.
	
        Process:	                                                 
	UART configuration:
		– 115200bps 
		– 8 data bit 
		– No parity 
		– 1 stop bit 
		– No flow control 
		- Receive and transmit enable
		
         UART will print welcome screen first, then ask for the user to plug in
         a USB memory stick. The memory stick needs to have a file with the name
         of MSREAD.txt on it with some text written in the file. The Lincoln 60 
         will then read the MSREAD.txt file and write it to a MSWRITE.txt file. 
         
         
@Directory contents:
	\EWARM: includes EWARM (IAR) project and configuration files
	\Keil:	includes RVMDK (Keil)project and configuration files 
	
	
@How to run:
	
Hardware configuration:		
	These jumpers must be configured as following:
			- JP2 pin 3 and 5 (HOST)
			- JP2 pin 4 and 6 (HOST)
Running mode:
This example can only run in ROM mode.
					
(Please reference "LPC1000 Software Development Toolchain" - chapter 4 "Creating 
and working with LPC1000CMSIS project" for more information)
	
Step to run:
	- Step 1: Build example.
	- Step 2: Burn hex file into board (if run on ROM mode)
	- Step 3: Connect COM1 on the Lincoln board to COM port on your computer
	- Step 4: Configure hardware and serial display as above instruction 
	- Step 5: Run example, use serial display to view the status and 
                  instructions. If an error happens press RESET.
		
@Tip:
	- Open \EWARM\*.eww project file to run example on IAR
	- Open \RVMDK\*.uvproj project file to run example on Keil