# Static Call Graph for image .\Flash\LPC1700CMSIS.axf

#<CALLGRAPH># ARM Linker, 4.1 [Build 644]: Last Updated: Tue Jan 17 15:48:48 2012

### Maximum Stack Usage = 0 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

### Mutually Recursive functions

- NMI_Handler ⇒ NMI_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- BusFault_Handler ⇒ BusFault_Handler
- UsageFault_Handler ⇒ UsageFault_Handler
- SVC_Handler ⇒ SVC_Handler
- DebugMon_Handler ⇒ DebugMon_Handler
- PendSV_Handler ⇒ PendSV_Handler
- SysTick_Handler ⇒ SysTick_Handler
- ADC_IRQHandler ⇒ ADC_IRQHandler

  ### Function Pointers

  - ADC_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - BOD_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - BusFault_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - CANActivity_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - CAN_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - DMA_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - DebugMon_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - EINT0_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - EINT1_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - EINT2_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - EINT3_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - ENET_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - HardFault_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - I2C0_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - I2C1_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - I2C2_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - I2S_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - MCPWM_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - MemManage_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - NMI_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - PLL0_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - PLL1_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - PWM1_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - PendSV_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - QEI_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - RIT_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - RTC_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - Reset_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - SPI_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - SSP0_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - SSP1_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - SVC_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - SysTick_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - SystemInit from system_lpc17xx.o(.text) referenced from startup_lpc17xx.o(.text)
  - TIMER0_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - TIMER1_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - TIMER2_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - TIMER3_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - UART0_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - UART1_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - UART2_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - UART3_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - USBActivity_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - USB_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - UsageFault_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - WDT_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_lpc17xx.o(.text)
  - main from template.o(.text) referenced from entry7.o(.ARM.Collect$$$$00000007)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry7.o(.ARM.Collect$$$$00000007))

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> SVC_Handler
  [Called By]
  - >> SVC_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> DebugMon_Handler
  [Called By]
  - >> DebugMon_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> SysTick_Handler
  [Called By]
  - >> SysTick_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  ADC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> ADC_IRQHandler
  [Called By]
  - >> ADC_IRQHandler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  BOD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  CANActivity_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  CAN_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  DMA_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  EINT0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  EINT1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  EINT2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  EINT3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  ENET_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  I2C0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  I2C1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  I2C2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  I2S_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  MCPWM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  PLL0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  PLL1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  PWM1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  QEI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  RIT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  SPI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  SSP0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  SSP1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  TIMER0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  TIMER1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  TIMER2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  TIMER3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  UART0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  UART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  UART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  UART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  USBActivity_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  USB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  WDT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  c_entry (Thumb, 4 bytes, Stack size 0 bytes, template.o(.text))
  [Called By]

  - >> main

  main (Thumb, 4 bytes, Stack size 0 bytes, template.o(.text))
  [Calls]

  - >> c_entry
  [Address Reference Count : 1]
  - entry7.o(.ARM.Collect$$$$00000007)

  check_failed (Thumb, 4 bytes, Stack size 0 bytes, template.o(.text), UNUSED)

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  SystemCoreClockUpdate (Thumb, 316 bytes, Stack size 0 bytes, system_lpc17xx.o(.text), UNUSED)

  SystemInit (Thumb, 296 bytes, Stack size 0 bytes, system_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(.text)

  ### Local Symbols

  ### Undefined Global Symbols