/**********************************************************************
* $Id$		abstract.txt 			
*//**
* @file		abstract.txt 
* @brief	Example description file
* @version	2.0
* @date		
* @author	NXP MCU SW Application Team/Micromint USA Support
*
* Copyright(C) 2010, NXP Semiconductor
* All rights reserved.
*
***********************************************************************
* Software that is described herein is for illustrative purposes only
* which provides customers with programming information regarding the
* products. This software is supplied "AS IS" without any warranties.
* NXP Semiconductors assumes no responsibility or liability for the
* use of the software, conveys no license or title under any patent,
* copyright, or mask work right to the product. NXP Semiconductors
* reserves the right to make changes in the software without
* notification. NXP Semiconductors also make no representation or
* warranty that such application will be suitable for the specified
* use without further testing or modification.
**********************************************************************/
  
@Example description:
Purpose:
	This example describes how to write a simple USB Mass Storage 
        application on LPC1768.
Process:
	The MassStorage project is a Mass Storage simple demo run on LPC1768		                                                
	Clock Settings:
	   - XTAL                   =  12 MHz
	   - PLL                    =  400 MHz
	   - processor clock = CCLK =  100 MHz
	   - USB clock              =  48 MHz
	   - CCLK / 4 clock         =  25 MHz
	
	It demonstrates an USB Memory based on USB Mass Storage Class.		
	The USB Memory is automatically recognized by the host PC
	running Windows which will load a generic Mass Storage driver.

@Directory contents:
	\EWARM: includes EWARM (IAR) project and configuration files
	\Keil:	includes RVMDK (Keil)project and configuration files 
	
	DiskImg.c: 		Disk Image (LPC17xx) data
	lpc17xx_libcfg.h: Library configuration file - include needed driver 
                          library for this example 
	memory.h/.c: 	USB Memory Storage
	msc.h: 			USB Mass Storage Class Definition
	mscuser.h/.c: 	Mass Storage Class Custom User
	usb.h: 			USB Definitions
	usbcfg.h: 		USB Configurate Definition
	usbcore.h/.c:	USB Core Module
	usbdesc.h/.c: 	USB Descriptors
	usbhw.h/.c: 	USB Hardware Layer
	usbreg.h: 	USB Hardware Layer Definitions for NXP Semiconductors  
	usbuser.h/.c: 	USB Custom User Module
	memory.h/.c: 	USB Memory Storage Demo (main program)
	makefile: 		make file (to build with GNU toolchain)

@How to run:
Hardware configuration:		
	These jumpers must be configured as following:
			- JP2 pin 3 and 5 (DEVICE)
			- JP2 pin 4 and 6 (DEVICE)
	
Running mode:
RAM mode:   This example can be run on RAM mode with debugger. All files must be
            build to .elf file, this file will be loaded into RAM through a 
            debugger tool before running 
ROM(FLASH)mode: This example can be run on ROM mode with debugger or standalone 
                after burning. All files in each example must be built to .hex 
                file. This file will be burned into ROM(Flash) memory through an
                external tool (i.e: Flash Magic...) befor running.
					
(Please reference "LPC1000 Software Development Toolchain" - chapter 4 "Creating 
and working with LPC1000CMSIS project" for more information)
	
Step to run:
	- Step 1: Build example.
	- Step 2: Burn hex file into board (if run on ROM mode)
	- Step 3: Configure hardware as above instruction 
	- Step 4: Hit reset button to run example.
	- Step 5: After see UGL(USB Good Link). Open My Computer, you will see 
                  'LPC17xx' disk.
	- Step 6: Open this disk, you will see 'Readme.txt' file (it has 
                  read-only attribute)
	- Step 7: Try to copy/delete another file into disk to test if Mass 
                  Storage is work well or not
		
(Pls see "LPC17xx Example Description" document - chapter "Examples > USBDEV > 
USBMassStorage" for more details)
		
@Tip:
	- Open \EWARM\*.eww project file to run example on IAR
	- Open \RVMDK\*.uvproj project file to run example on Keil