/**********************************************************************
* $Id$		abstract.txt 			
*
* @file		abstract.txt 
* @brief	Example description file
* @version	2.0
* @date		
* @author	NXP MCU SW Application Team/Micromint USA Support
*
* Copyright(C) 2010, NXP Semiconductor
* All rights reserved.
*
***********************************************************************
* Software that is described herein is for illustrative purposes only
* which provides customers with programming information regarding the
* products. This software is supplied "AS IS" without any warranties.
* NXP Semiconductors assumes no responsibility or liability for the
* use of the software, conveys no license or title under any patent,
* copyright, or mask work right to the product. NXP Semiconductors
* reserves the right to make changes in the software without
* notification. NXP Semiconductors also make no representation or
* warranty that such application will be suitable for the specified
* use without further testing or modification.
**********************************************************************/
  
@Example description:
	Purpose:
		This example describes how to use ADC conversion in hardware-
                triggered mode.
	Process:
		The ADC conversion rate is 200KHz. A fully accurate conversion 
                requires 65 of these clocks. So ADC clock = 200KHz * 65 = 13MHz.
		Note that maximum ADC clock input is 13MHz.  
		
		When INT0 falling adge occurs, ADC will start converting.
		ADC will generate interrupt at the end of each conversion. ADC
                service routine will be invoked to check ADC status, if 
                "DONE bit" is set, ADC converted data will be stored in 
                "adc_value". ADC interrupt is disabled and re-enabled for the 
                next conversion. ADC converted data are displayed via COM1
                (UART0).
		
		Adjust the analog voltage to change ADC signal input.

@Directory contents:
	\EWARM: includes EWARM (IAR) project and configuration files
	\Keil:	includes RVMDK (Keil)project and configuration files 
	
	lpc17xx_libcfg.h: Library configuration file - include needed driver 
        library for this example 
	makefile: Example's makefile (to build with GNU toolchain)
	adc_hardware_trigger_test.c: Main program

@How to run:
  Serial display configuration: (e.g: TeraTerm, Hyperterminal, Flash Magic...) 
    – 115200bps 
    – 8 data bit 
    – No parity 
    – 1 stop bit 
    – No flow control 
	
  Running mode:
    This example can run on RAM/ROM mode.
      Step to run:
	- Step 1: Build example.
	- Step 2: Burn hex file into board (if run on ROM mode)
	- Step 3: Connect COM1 on the Lincoln board to COM port on your computer
	- Step 4: Configure hardware and serial display as above instruction 
	- Step 5: Run example
		  Press User Button button to start the ADC conversion
		  Adjust the analog voltage and the User Button again then 
                  observe data on serial display
		
@Tip:
	- Open \EWARM\*.eww project file to run example on IAR
	- Open \RVMDK\*.uvproj project file to run example on Keil