/**********************************************************************
* $Id$		abstract.txt 			
*//**
* @file		abstract.txt 
* @brief	Example description file
* @version	2.0
* @date		
* @author	NXP MCU SW Application Team/Micromint USA Support
*
*
* Copyright(C) 2010, NXP Semiconductor
* All rights reserved.
*
***********************************************************************
* Software that is described herein is for illustrative purposes only
* which provides customers with programming information regarding the
* products. This software is supplied "AS IS" without any warranties.
* NXP Semiconductors assumes no responsibility or liability for the
* use of the software, conveys no license or title under any patent,
* copyright, or mask work right to the product. NXP Semiconductors
* reserves the right to make changes in the software without
* notification. NXP Semiconductors also make no representation or
* warranty that such application will be suitable for the specified
* use without further testing or modification.
**********************************************************************/
  
@Example description:
Purpose:
	This example describes how to use WDT to generate chip reset after a 
        specific time.
Process:
	WDT setting:
		- generate reset chip when WDT times out.
		- time-out = 5s
		- clock source: IRC (Internal RC oscillator)
	After start, WDT counter decrease until underflow (5s) to generate a 
        chip reset. If between 5s, RESET button is pressed, chip force an 
        external reset. If not, WDT will reset chip after 5s automatically.
	After reset, the program will determine what cause of last reset time 
        (external reset or WDT Timeout reset) 
		
@Directory contents:
\EWARM: includes EWARM (IAR) project and configuration files
\Keil:	includes RVMDK (Keil)project and configuration files
	  
lpc17xx_libcfg.h: Library configuration file - include needed driver library for 
this example makefile: Example's makefile (to build with GNU toolchain)
wdt_reset_test.c: Main program

@How to run:
Hardware configuration:		

Serial display configuration: (e.g: TeraTerm, Hyperterminal, Flash Magic...) 
	– 115200bps 
	– 8 data bit 
	– No parity 
	– 1 stop bit 
	– No flow control 
	
Running mode:
RAM mode:   This example can be run on RAM mode with debugger. 
 	    All files must be build to .elf file, this file will be loaded into 
            RAM through a debugger tool before running 
ROM(FLASH)mode: This example can be run on ROM mode with debugger or standalone 
                after burning. 

(Please reference "LPC1000 Software Development Toolchain" - chapter 4 "Creating
and working with LPC1000CMSIS project" for more information)
	
Step to run:
	- Step 1: Build example.
	- Step 2: Burn hex file into board (if run on ROM mode)
	- Step 3: Connect COM1 on the Lincoln board to COM port on your computer
	- Step 4: Configure hardware and serial display as above instruction 
	- Step 5: Run example and observe data on serial display
 		   + If in between 5s, hit RESET button, after reset, we will 
                     have the notice
			" Last MCU reset caused by External!"
		   + If not, WDT cause chip reset and after reset, we will have 
                     the notice
			" Last MCU reset caused by WDT TimeOut!"
						
(Pls see "LPC17xx Example Description" document - chapter "Examples > WDT >
RESET" for more details)
		
@Tip:
	- Open \EWARM\*.eww project file to run example on IAR
	- Open \RVMDK\*.uvproj project file to run example on Keil
	