/**********************************************************************
* $Id$		abstract.txt 			
*//**
* @file		abstract.txt 
* @brief	Example description file
* @version	2.0
* @date		
* @author	NXP MCU SW Application Team
*
* Copyright(C) 2010, NXP Semiconductor
* All rights reserved.
*
***********************************************************************
* Software that is described herein is for illustrative purposes only
* which provides customers with programming information regarding the
* products. This software is supplied "AS IS" without any warranties.
* NXP Semiconductors assumes no responsibility or liability for the
* use of the software, conveys no license or title under any patent,
* copyright, or mask work right to the product. NXP Semiconductors
* reserves the right to make changes in the software without
* notification. NXP Semiconductors also make no representation or
* warranty that such application will be suitable for the specified
* use without further testing or modification.
**********************************************************************/
  
@Example description:
Purpose:
	This example describes how to enter system in Deep PowerDown mode and 
        wake-up by using the RTC (Real-time clock) interrupt
Process:
	When system enter in Deep PowerDown mode, it just can be waked up when 
        an external reset signal is applied, or the RTC interrupt is enabled 
        and an RTC interrupt is generated.
	In this case, we can use both RTC interrupt or hit RESET button to 
        wake-up system
	RTC configure:
		- Alarm time: 5s
	So, after each 5s, RTC will generate Alarm interrupt to wake up system. 
					
@Directory contents:
	\EWARM: includes EWARM (IAR) project and configuration files
	\Keil:	includes RVMDK (Keil)project and configuration files 

@How to run:
Serial display configuration:(e.g: TeraTerm, Hyperterminal, Flash Magic...) 
	– 115200bps 
	– 8 data bit 
	– No parity 
	– 1 stop bit 
	– No flow control 
	
Running mode:
	This example can run on RAM/ROM mode.
				
Step to run:
   - Step 1: Build example.
   - Step 2: Burn hex file into board (if run on ROM mode)
   - Step 3: Connect COM1 on the Lincoln board to COM port on your computer
   - Step 4: Configure hardware and serial display as above instruction 
- Step 5: Run example and observe on serial display
	+ Press '1' to enter system in Deep PowerDown mode
	and wait 5s to RTC wake-up system automatically or press 
	"RESET" button to wake it up immediatly.
			
@Tip:
	- Open \EWARM\*.eww project file to run example on IAR
	- Open \RVMDK\*.uvproj project file to run example on Keil