/**********************************************************************
* $Id$		abstract.txt 			
*//**
* @file		abstract.txt 
* @brief	Example description file
* @version	2.0
* @date		
* @author	NXP MCU SW Application Team/Micromint USA Support
*
* Copyright(C) 2010, NXP Semiconductor
* All rights reserved.
*
***********************************************************************
* Software that is described herein is for illustrative purposes only
* which provides customers with programming information regarding the
* products. This software is supplied "AS IS" without any warranties.
* NXP Semiconductors assumes no responsibility or liability for the
* use of the software, conveys no license or title under any patent,
* copyright, or mask work right to the product. NXP Semiconductors
* reserves the right to make changes in the software without
* notification. NXP Semiconductors also make no representation or
* warranty that such application will be suitable for the specified
* use without further testing or modification.
**********************************************************************/

@Example description:
Purpose:
	This example describes how to use GPIO interrupt function.

Process:
	Hit the USER button on the Lincoln to make the interrupt happen.

@Directory contents:
	\EWARM: includes EWARM (IAR) project and configuration files
	\Keil:	includes RVMDK (Keil)project and configuration files 
	
	lpc17xx_libcfg.h: Library configuration file - include needed driver 
        library for this example 
	makefile: Example's makefile
	gpio_int.c: Main program

@How to run:
Running mode:
	This example can run on RAM/ROM mode.
					
Step to run:
	- Step 2: Build example.
	- Step 3: Burn hex file into board (if run in ROM mode)
	- Step 4: Reset the board
	- Step 5: Press the USER button then LED2 will be blinking 8 times
		
@Tip:
	- Open \EWARM\*.eww project file to run example on IAR
	- Open \RVMDK\*.uvproj project file to run example on Keil
