/**********************************************************************
* $Id$		abstract.txt 			
*//**
* @file		abstract.txt 
* @brief	Example description file
* @version	2.0
* @date		
* @author	NXP MCU SW Application Team/Micromint USA Support
*
* Copyright(C) 2010, NXP Semiconductor
* All rights reserved.
*
***********************************************************************
* Software that is described herein is for illustrative purposes only
* which provides customers with programming information regarding the
* products. This software is supplied "AS IS" without any warranties.
* NXP Semiconductors assumes no responsibility or liability for the
* use of the software, conveys no license or title under any patent,
* copyright, or mask work right to the product. NXP Semiconductors
* reserves the right to make changes in the software without
* notification. NXP Semiconductors also make no representation or
* warranty that such application will be suitable for the specified
* use without further testing or modification.
**********************************************************************/
  
@Example description:
Purpose:
	This example describes how to use RIT as a timer to generate interrupt
        to drive LED
Process:
	RIT time interval configure is 1000 ms = 1s.
	So each 1s, RIT will generate interrupt and invoke RIT_IRQHandler( ) to
        turn on/off LED1.		
		
@Directory contents:
\EWARM: includes EWARM (IAR) project and configuration files
\Keil:	includes RVMDK (Keil)project and configuration files
 
lpc17xx_libcfg.h: Library configuration file - include needed driver library for
                  this example 
makefile: Example's makefile (to build with GNU toolchain)
rit_interrupt.c: Main program

@How to run:

Serial display configuration:(e.g: TeraTerm, Hyperterminal, Flash Magic...) 
	– 115200bps 
	– 8 data bit 
	– No parity 
	– 1 stop bit 
	– No flow control 
	
Running mode:
This example can run on RAM/ROM mode.
				
Step to run:

   - Step 1: Build example.
   - Step 2: Burn hex file into board (if run on ROM mode)
   - Step 3: Connect COM1 on the Lincoln board to COM port on your computer
   - Step 5: Configure hardware and serial display as above instruction 
   - Step 6: Run example.
	   Note: LED1 will blink for testing
					
@Tip:
	- Open \EWARM\*.eww project file to run example on IAR
	- Open \RVMDK\*.uvproj project file to run example on Keil