/**********************************************************************
* $Id$		abstract.txt 			
*//**
* @file		abstract.txt 
* @brief	Example description file
* @version	2.0
* @date		
* @author	NXP MCU SW Application Team/Micromint USA Support
*
* Copyright(C) 2010, NXP Semiconductor
* All rights reserved.
*
***********************************************************************
* Software that is described herein is for illustrative purposes only
* which provides customers with programming information regarding the
* products. This software is supplied "AS IS" without any warranties.
* NXP Semiconductors assumes no responsibility or liability for the
* use of the software, conveys no license or title under any patent,
* copyright, or mask work right to the product. NXP Semiconductors
* reserves the right to make changes in the software without
* notification. NXP Semiconductors also make no representation or
* warranty that such application will be suitable for the specified
* use without further testing or modification.
**********************************************************************/
  
@Example description:
Purpose:
	This example describes how to use UART in DMA mode
Process:
	UART0 is configured as the following:
	 	+ Baudrate = 115200 bps
	 	+ 8 data bit
	 	+ 1 Stop bit
	 	+ None parity
 	GPDMA channel 0 using to transmit the welcome message (the destination 
        source is UART0 transmit pin)
 	GPDMA channel 1 using to receive the character (the destination source 
        is the UART0 receive pin)
 	
 	Note: If using this example to test with UART1, pls add conversion type 
        (LPC_UART_TypeDef *)LPC_UART1 because UART1 has different structure type
Ex: UART_Send((LPC_UART_TypeDef *)LPC_UART1, menu1, sizeof(menu1), BLOCKING);

@Directory contents:
\EWARM: includes EWARM (IAR) project and configuration files
\Keil:	includes RVMDK (Keil)project and configuration files 
	
lpc17xx_libcfg.h: Library configuration file - include needed driver library for 
                  this example 
makefile: Example's makefile (to build with GNU toolchain)
uart_dma_test.c: Main program

@How to run:
Hardware configuration:		

Serial display configuration: (e.g: TeraTerm, Hyperterminal, Flash Magic...) 
	– 115200bps 
	– 8 data bit 
	– No parity 
	– 1 stop bit 
	– No flow control 
        
Running mode:
This example can run on RAM/ROM mode.
				
(Please reference "LPC1000 Software Development Toolchain" - chapter 4 "Creating
and working with LPC1000CMSIS project" for more information)
	
Step to run:
	- Step 1: Build example.
	- Step 2: Burn hex file into board (if run on ROM mode)
	- Step 3: Connect COM1 on the Lincoln board to COM port on your computer
	- Step 4: Configure hardware and serial display as above instruction 
	- Step 5: Run example, using Serial display to monitor the message and 
                  to send a charater to UART

(Pls see "LPC17xx Example Description" document - chapter "Examples > UART > 
DMA" for more details)
		
@Tip:
	- Open \EWARM\*.eww project file to run example on IAR
	- Open \RVMDK\*.uvproj project file to run example on Keil
