/**********************************************************************
* $Id$		abstract.txt 			
*//**
* @file		abstract.txt 
* @brief	Example description file
* @version	2.0
* @date		
* @author	NXP MCU SW Application Team/Micromint USA Support
*
* Copyright(C) 2010, NXP Semiconductor
* All rights reserved.
*
***********************************************************************
* Software that is described herein is for illustrative purposes only
* which provides customers with programming information regarding the
* products. This software is supplied "AS IS" without any warranties.
* NXP Semiconductors assumes no responsibility or liability for the
* use of the software, conveys no license or title under any patent,
* copyright, or mask work right to the product. NXP Semiconductors
* reserves the right to make changes in the software without
* notification. NXP Semiconductors also make no representation or
* warranty that such application will be suitable for the specified
* use without further testing or modification.
**********************************************************************/
  
@Example description:
Purpose:
	This example describes how to enter system in DeepSleep mode and wake 
        it up by using WDT Interrupt
Process:
	WDT setting:
		- Source clock: IRC oscillator
		- Interrupt mode
		- Timeout = 2000000 us = 2s
	Enter system in DeepSleep by using CLKPWR_DeepSleep function 
        (call __WFI()). After 2s, WDT timeout and generate interrupt to wake up 
        the system.
					
@Directory contents:
	\EWARM: includes EWARM (IAR) project and configuration files
	\Keil:	includes RVMDK (Keil)project and configuration files 
	
@How to run:
Serial display configuration:(e.g: TeraTerm, Hyperterminal, Flash Magic...) 
	– 115200bps 
	– 8 data bit 
	– No parity 
	– 1 stop bit 
	– No flow control 
	
Running mode:
This example can run on RAM/ROM mode.
					
Step to run:
   - Step 1: Build example.
   - Step 2: Burn hex file into board (if run on ROM mode)
   - Step 3: Connect COM1 on the Lincoln board to COM port on your computer
   - Step 4: Configure hardware and serial display as above instruction 
   - Step 5: Run example and observe result on serial display
	+ Press '1' to enter system in DeepSleep mode
	+ After 2s, WDT timeout and wakes system up
        
@Tip:
	- Open \EWARM\*.eww project file to run example on IAR
	- Open \RVMDK\*.uvproj project file to run example on Keil