/**********************************************************************
* $Id$		abstract.txt 			
*//**
* @file		abstract.txt 
* @brief	Example description file
* @version	2.0
* @date		
* @author	NXP MCU SW Application Team/Micromint USA Support
*
* Copyright(C) 2010, NXP Semiconductor
* All rights reserved.
*
***********************************************************************
* Software that is described herein is for illustrative purposes only
* which provides customers with programming information regarding the
* products. This software is supplied "AS IS" without any warranties.
* NXP Semiconductors assumes no responsibility or liability for the
* use of the software, conveys no license or title under any patent,
* copyright, or mask work right to the product. NXP Semiconductors
* reserves the right to make changes in the software without
* notification. NXP Semiconductors also make no representation or
* warranty that such application will be suitable for the specified
* use without further testing or modification.
**********************************************************************/
  
@Example description:
Purpose:
	This example describes how to use UART in polling mode
Process:
	UART configuration:
		– 115200bps 
		– 8 data bit 
		– No parity 
		– 1 stop bit 
		– No flow control 
		- Receive and transmit enable
		
UART will print welcome screen first, then:
	- press any key to have it read in from the terminal and returned back 
          to the terminal.
	- Press ESC to exit.
	- Press 'r' to print welcome screen menu again.
		
Note: If using this example to test with UART1, pls add conversion type 
(LPC_UART_TypeDef *)LPC_UART1 because UART1 has different structure type
Ex: UART_Send((LPC_UART_TypeDef *)LPC_UART1, menu1, sizeof(menu1), BLOCKING);
		
@Directory contents:
	\EWARM: includes EWARM (IAR) project and configuration files
	\Keil:	includes RVMDK (Keil)project and configuration files 
	
lpc17xx_libcfg.h: Library configuration file - include needed driver library for
this example makefile: Example's makefile (to build with GNU toolchain)
uart_polling_test.c: Main program

@How to run:
Hardware configuration:		

Running mode:
	This example can run on RAM/ROM mode.
				
(Please reference "LPC1000 Software Development Toolchain" - chapter 4 "Creating
and working with LPC1000CMSIS project" for more information)
	
Step to run:
	- Step 1: Build example.
	- Step 2: Burn hex file into board (if run on ROM mode)
	- Step 3: Connect COM1 on the Lincoln board to COM port on your computer
	- Step 4: Configure hardware and serial display as above instruction 
	- Step 5: Run example, use serial display to control COM1 as the guide
                  on screen
		
(Pls see "LPC17xx Example Description" document - chapter "Examples > UART > 
Polling" for more details)
		
@Tip:
	- Open \EWARM\*.eww project file to run example on IAR
	- Open \RVMDK\*.uvproj project file to run example on Keil
