- Main Page
- Modules
- Data Structures
- Files
- Examples

- File List
- Globals

# arm_pid_init_f32.c

Go to the documentation of this file.

    00001 /* ----------------------------------------------------------------------
    00002 * Copyright (C) 2010 ARM Limited. All rights reserved.
    00003 *
    00004 * $Date:        29. November 2010
    00005 * $Revision:    V1.0.3
    00006 *
    00007 * Project:      CMSIS DSP Library
    00008 * Title:        arm_pid_init_f32.c
    00009 *
    00010 * Description:  Floating-point PID Control initialization function
    00011 *
    00012 *
    00013 * Target Processor: Cortex-M4/Cortex-M3
    00014 *
    00015 * Version 1.0.3 2010/11/29
    00016 *    Re-organized the CMSIS folders and updated documentation.
    00017 *
    00018 * Version 1.0.2 2010/11/11
    00019 *    Documentation updated.
    00020 *
    00021 * Version 1.0.1 2010/10/05
    00022 *    Production release and review comments incorporated.
    00023 *
    00024 * Version 1.0.0 2010/09/20
    00025 *    Production release and review comments incorporated.
    00026 * ------------------------------------------------------------------- */
    00027
    00028 #include "arm_math.h"
    00029
    00048 void arm_pid_init_f32(
    00049   arm_pid_instance_f32 * S,
    00050   int32_t resetStateFlag)
    00051 {
    00052
    00053   /* Derived coefficient A0 */
    00054   S->A0 = S->Kp + S->Ki + S->Kd;
    00055
    00056   /* Derived coefficient A1 */
    00057   S->A1 = (-S->Kp) - ((float32_t) 2.0 * S->Kd);
    00058
    00059   /* Derived coefficient A2 */
    00060   S->A2 = S->Kd;
    00061
    00062   /* Check whether state needs reset or not */
    00063   if(resetStateFlag)
    00064   {
    00065     /* Clear the state buffer.  The size will be always 3 samples */
    00066     memset(S->state, 0, 3u * sizeof(float32_t));
    00067   }
    00068
    00069 }
    00070

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines