/**********************************************************************
* $Id$		abstract.txt 			
*//**
* @file		abstract.txt 
* @brief	Example description file
* @version	2.0
* @date		
* @author	NXP MCU SW Application Team/Micromint USA Support
*
* Copyright(C) 2010, NXP Semiconductor
* All rights reserved.
*
***********************************************************************
* Software that is described herein is for illustrative purposes only
* which provides customers with programming information regarding the
* products. This software is supplied "AS IS" without any warranties.
* NXP Semiconductors assumes no responsibility or liability for the
* use of the software, conveys no license or title under any patent,
* copyright, or mask work right to the product. NXP Semiconductors
* reserves the right to make changes in the software without
* notification. NXP Semiconductors also make no representation or
* warranty that such application will be suitable for the specified
* use without further testing or modification.
**********************************************************************/
  
@Example description:
Purpose:
	This example describes how to generate interrupt in Second 
	Counter Increment Interrupt (1s) and generate Alarm interrupt at 10s
Process:
	After initialize RTC, set current time for RTC with this value:
	8:00:00PM, 2009-04-24
	And set Alarm time at 10s
	RTC is set generate interrupt each second, so each 1s it will call 
	RTC_IRQHandler( ), it will get time from RTC register and display on
	serial screen. It all check if alarm match interrupt occurs or not.
	(This interrupt just only occurs at 10s). So after 10s, alarm interrupt
	occurs and a notice sentence will be wirte on serial display screen.

@Directory contents:
\EWARM: includes EWARM (IAR) project and configuration files
\Keil:	includes RVMDK (Keil)project and configuration files 

lpc17xx_libcfg.h: Library configuration file - include needed driver library for
this example makefile: Example's makefile (to build with GNU toolchain)
rtc_alarm_cntincr_int.c: Main program

@How to run:
Hardware configuration:		
				
Serial display configuration:(e.g: TeraTerm, Hyperterminal, Flash Magic...) 
		– 115200bps 
		– 8 data bit 
		– No parity 
		– 1 stop bit 
		– No flow control 
	
Running mode:
This example can run on RAM/ROM mode.
						
Step to run:
	- Step 1: Build example.
	- Step 2: Burn hex file into board (if run on ROM mode) 
	- Step 3: Connect COM1 on the Lincoln board to COM port on your computer
	- Step 4: Configure hardware and serial display as above instruction 
	- Step 5: Run example and observe data from serial display
				
@Tip:
	- Open \EWARM\*.eww project file to run example on IAR
	- Open \RVMDK\*.uvproj project file to run example on Keil