- Main Page
- Modules
- Data Structures
- Files
- Examples

- File List
- Globals

# arm_mult_q31.c

Go to the documentation of this file.

    00001 /* ----------------------------------------------------------------------
    00002 * Copyright (C) 2010 ARM Limited. All rights reserved.
    00003 *
    00004 * $Date:        15. July 2011
    00005 * $Revision:    V1.0.10
    00006 *
    00007 * Project:      CMSIS DSP Library
    00008 * Title:        arm_mult_q31.c
    00009 *
    00010 * Description:  Q31 vector multiplication.
    00011 *
    00012 * Target Processor: Cortex-M4/Cortex-M3/Cortex-M0
    00013 *
    00014 * Version 1.0.10 2011/7/15
    00015 *    Big Endian support added and Merged M0 and M3/M4 Source code.
    00016 *
    00017 * Version 1.0.3 2010/11/29
    00018 *    Re-organized the CMSIS folders and updated documentation.
    00019 *
    00020 * Version 1.0.2 2010/11/11
    00021 *    Documentation updated.
    00022 *
    00023 * Version 1.0.1 2010/10/05
    00024 *    Production release and review comments incorporated.
    00025 *
    00026 * Version 1.0.0 2010/09/20
    00027 *    Production release and review comments incorporated.
    00028 *
    00029 * Version 0.0.5  2010/04/26
    00030 *    incorporated review comments and updated with latest CMSIS layer
    00031 *
    00032 * Version 0.0.3  2010/03/10
    00033 *    Initial version
    00034 * -------------------------------------------------------------------- */
    00035
    00036 #include "arm_math.h"
    00037
    00061 void arm_mult_q31(
    00062   q31_t * pSrcA,
    00063   q31_t * pSrcB,
    00064   q31_t * pDst,
    00065   uint32_t blockSize)
    00066 {
    00067   uint32_t blkCnt;                               /* loop counters */
    00068
    00069 #ifndef ARM_MATH_CM0
    00070
    00071 /* Run the below code for Cortex-M4 and Cortex-M3 */
    00072   /* loop Unrolling */
    00073   blkCnt = blockSize >> 2u;
    00074
    00075   /* First part of the processing with loop unrolling.  Compute 4 outputs at a time.
    00076    ** a second loop below computes the remaining 1 to 3 samples. */
    00077   while(blkCnt > 0u)
    00078   {
    00079     /* C = A * B */
    00080     /* Multiply the inputs and then store the results in the destination buffer. */
    00081     *pDst++ =
    00082       (q31_t) clip_q63_to_q31(((q63_t) (*pSrcA++) * (*pSrcB++)) >> 31);
    00083     *pDst++ =
    00084       (q31_t) clip_q63_to_q31(((q63_t) (*pSrcA++) * (*pSrcB++)) >> 31);
    00085     *pDst++ =
    00086       (q31_t) clip_q63_to_q31(((q63_t) (*pSrcA++) * (*pSrcB++)) >> 31);
    00087     *pDst++ =
    00088       (q31_t) clip_q63_to_q31(((q63_t) (*pSrcA++) * (*pSrcB++)) >> 31);
    00089
    00090     /* Decrement the blockSize loop counter */
    00091     blkCnt--;
    00092   }
    00093
    00094   /* If the blockSize is not a multiple of 4, compute any remaining output samples here.
    00095    ** No loop unrolling is used. */
    00096   blkCnt = blockSize % 0x4u;
    00097
    00098 #else
    00099
    00100   /* Run the below code for Cortex-M0 */
    00101
    00102   /* Initialize blkCnt with number of samples */
    00103   blkCnt = blockSize;
    00104
    00105 #endif /* #ifndef ARM_MATH_CM0 */
    00106
    00107   while(blkCnt > 0u)
    00108   {
    00109     /* C = A * B */
    00110     /* Multiply the inputs and then store the results in the destination buffer. */
    00111     *pDst++ =
    00112       (q31_t) clip_q63_to_q31(((q63_t) (*pSrcA++) * (*pSrcB++)) >> 31);
    00113
    00114     /* Decrement the blockSize loop counter */
    00115     blkCnt--;
    00116   }
    00117 }
    00118

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines