RELEASE: LPC1700CMSIS_120427

1./ Update ADC Driver:
    + Stop conversion before disabling a channel.
	+ Disable all channels before de-initialize ADC.
2./ Fix compile errors when selecting UART_PORT=1 in UART/Polling , IrDA/Transmit & IrDA/Receive example.
3./ Add IAP_Demo example.

*******************************************************************************************************************************
RELEASE: LPC1700CMSIS_120330

1./ Update example code to compile OK in Linux.
2./ Change the folder name from "Template" to "Templates" (in Core/Device/Source path) to match CMSISv2.1.
3./ Remove disabling BOD in  CLKPWR_DeepSleep function and CLKPWR_PowerDown function.
4./ Remove file libnosys_gnu.c from EmacRaw Example.

*******************************************************************************************************************************
RELEASE: LPC1700CMSIS_120229

1./ Set the burst size of ADC to 1 instead of 4.
2./ Update ADC_Burst Example: 
	+ Add DMA Support Option through __DMA_USED__ macro.
	+ Fix problem: injection test works improperly.
3./ Update SPI Master/Slave examples: 
	+ Use macro SPI_DATABIT_8~16 to set value for SPI_ConfigStruct.Databit.
	+ Update Buffer Initialization and Verification. 
4./ Fix the condition of waiting for PLL0/1 connected in SystemInit function.

*******************************************************************************************************************************
RELEASE: LPC1700CMSIS_120131

1./ Fix bug in Emac driver files:
	+ the loop condition when checking the status of PHY is incorrect.
	+ Remove waiting for auto-negotiation while configuring PHY.
2./ Update I2C Driver & examples:
        + The I2C pins should be configured as no pull-up, no pull-down resistor, open-drain mode.
	+ Create a common functions to handle I2C Master States, I2C Slave States.

*******************************************************************************************************************************
RELEASE: LPC1700CMSIS_111130

1./ Fix bug in Emac driver files:
	+ Add some new values to EMAC_clkdiv:
		const uint8_t EMAC_clkdiv[] = { 4, 6, 8, 10, 14, 20, 28, 36, 40, 44, 48, 52, 56, 60, 64 };
	+ Remove code line: LPC_EMAC->SUPP = EMAC_SUPP_RES_RMII;
		and definition: EMAC_SUPP_RES_RMII in header file (they are unnecessary)
2./ Change include file name "LPC17xx.h" instead of "lpc17xx.h"
	in: lpc17xx_clkpwr.h 
		lpc17xx_pinsel.h
	The incompatible include file name will cause error compile when run on Linux enviroment
3./ Remove remain warnings in all project (GNU, IAR, Keil)
4./ Update CHM document file 

*******************************************************************************************************************************

RELEASE: LPC1700CMSIS_111031

1./ Added casts to eliminate warnings in LPCXpresso in:
	+ debug_frmwrk.c
	+ lpc17xx_uart.c
2./ Eliminate redefinition warnings by checking for previous definitions of MAX and MIN in: lpc_types.h 
		
*******************************************************************************************************************************
		
RELEASE: LPC1700CMSIS_111029

1./ Update to new CMSIS verision (2.1)
	a./ Change the Core structure (follow by the new structure on CMSIS 2.1 package)
		- Remove Documentation & CM3 folder
		- Add Device and CMSIS folder
	b./ Modify include paths in Keil/IAR project files and GNU makefile to compatible with new structure 
	c./ Modify linker and starup file (IAR & GNU) to support handle CRP (Code Read Protection).
	d./ Change the default setting of J-link/J-Trace in IAR - Ram mode (choose Normal option instead of Reset option).
		Normal option may cause the debugger doesn't operate properly. 	
2./ .\makesection\makeconfig 
	Remove CMCORE_TYPE 
3./ Update CHM document:
	a./ Update document for CMSIS 2.1
		+ Add DSP Function & Example in Modules tab
	b./ Update paths for some hyperlinks
	c./ Update Keil version 4.0 (instead of version 3.14) and IAR version 6.0 (instead of version 5.5)
		
*******************************************************************************************************************************

RELEASE: LPC1700CMSIS_110929

1./ Fix bug in EXTI driver
2./ Fix bug in SSP driver:The issue is ,our data bits set to 16 bits (2 bytes) the counter will increase 2, 
every single rv or transmit, so if dataCfg->length is an odd number, the comparison will never match 
	Solution: Change from compare receive/transmit counter and length by "!=" operator into "<" operator
3./ update Core files to fix the IAR intrinsics errors in version 6.20 and newer
4./ Update abstract file in EMAC (Easy_Web and uIP) examples

*******************************************************************************************************************************

RELEASE: LPC1700CMSIS_110829

1./ Remove #elif #if in debug_frmwrk.c
2./ Change: #elif -> #else in SSP_MicroWire example: #elif without expression will cause error compile when using LPCXpresso

*******************************************************************************************************************************

RELEASE: LPC1700CMSIS_29July2011

1./ Fix bug in system_LPC17xx.h
	- 	CCLKSEL value could be from 2..255, but in system_LPC17xx.c, it checked "CCLKSEL must be contain odd values or 0"
2./ Fix bug in lpc17xx_uart.c > uart_set_divisor
	Remove line: 
	uClk = uClk >> 4; /* div by 16 */ 
3./ LPC17xx.h
	DMAREQSEL was placed at wrong address (it must be placed at 0x400FC1C4 instead of 0x4000C1C4)
4./ Update document: standadize same as LPC177x_8x chm doc
5./ Fix ADC bug: CLKDIV is not caculate correctly, caused by interger division always round by 0 
6./ Fix EMAC > Easy_Web > ADC.c : add "#define lpx17xx_emac.h"
7./ Update abstract file for Easy_Web and uIP: Use Straight cable instead of CrossOver cable
8./ Update CHM document file.
	
*******************************************************************************************************************************

RELEASE: LPC1700CMSIS_14June2011
1./ Fix USB Audio bug:
	Clean interrupt for SOF and ERROR in USB_IRQHandler()

*******************************************************************************************************************************

RELEASE: LPC1700CMSIS_07June2011

1./ Fix I2S bugs, see:
		- PARAM_I2S_DMA_DEPTH(n)
		- PARAM_I2S_IRQ_LEVEL(n)
		- PARAM_I2S_HALFPERIOD(n)
		- PARAM_I2S_BITRATE(n)
2./ Fix RTC bugs in:
		- RTC_SetTime()
		- RTC_SetAlarmTime()
3./ Fix UART bug in:
		- uart_set_divisors())
4./ Remove some warnings
5./ Update document
6./ Change headers in drivers, examples, abstract files
7./ Standadize Keil project files (abstract open only, default target: FLASH, remove breakpoints..)

*******************************************************************************************************************************

RELEASE: LPC1700CMSIS_31Mar2011

1./ Fix bug in I2C driver (customer feedback)
	Problem description: 
		I2C_MasterTransferData() is not able to 
		(1) Send, 
		(2) doing a repeated Start and 
		(3) starting to receive with one function call. 
		Problem is that the repeated start is not generated, but a retransmission of the 
		last word is startet. 
	Solve: change 
		I2Cx->I2CONCLR = I2C_I2CONCLR_SIC; 
		I2Cx->I2CONSET = I2C_I2CONSET_STA; 
	to 
		I2Cx->I2CONSET = I2C_I2CONSET_STA; 
		I2Cx->I2CONCLR = I2C_I2CONCLR_SIC; 
		in function I2C_Start () 
2./ Add function PWM_MultiMatchUpdate() to update match value for multi-channel at the same time
3./ Update .chm file 	

*******************************************************************************************************************************

RELEASE: LPC1700CMSIS_10March2011

1./Fix TIM bug (Customer feedback: Case 00001479): TIM clear pending functions will clear all interrupt pending instead of 
clearing specific interrupt bit.
	- fix functions:
		+ TIM_ClearIntPending
		+ TIM_ClearIntCapturePending


*******************************************************************************************************************************

RELEASE: LPC1700CMSIS_09March2011

1./Fix CAN bug (Customer feedback: Case 00001354): older driver does not support setting AFLUT with different controller.
	- modify functions:
		+ CAN_SetupAFLUT()
		+ CAN_LoadExplicitEntry()
		+ CAN_LoadFullCANEntry()
		+ CAN_LoadGroupEntry()		

*******************************************************************************************************************************

RELEASE: LPC1700CMSIS_26Jan2011

1./ Fix bugs:
	- debug_frmwrk.c > UARTPutDec32
	- lpc17xx_i2c.c > I2C_SetClock

*******************************************************************************************************************************

RELEASE: LPC1700CMSIS_30Dec2010

*** LPC1700CMSIS_30Dec2010 Lite***
1./ Update to CMSIS v2.0
	- update core_cm3.h/.c
	- add core_cmFunc.h
	- add core_cmInstr.h
	- update .chm document 
		+ update CMSIS Introduction (use v2.0 doc)
		+ update CMSIS's version
		+ re-organize CMSIS tab 
		
*** LPC1700CMSIS_30Dec2010 Full***
1./ Update to CMSIS v2.0
	- update core_cm3.h/.c
	- add core_cmFunc.h
	- add core_cmInstr.h
	- add folder DSP_Lib at ..\Core
	- add folder Document that includes CMSIS html files
	- add CMSIS Document at ..\Core that describes all details about CMSIS v2.0
	- modify .chm document (remove CMSIS Introduction link)
	- re-organize CMSIS Tab
			 
*******************************************************************************************************************************

RELEASE: LPC1700CMSIS_06Dec2010

1./ Fix CAN issue
	Issue: CAN code is running at a /4 frequency and the baud rate of 1Mbps cannot be hit exactly given a chip 
	       frequency of 100MHz.
	Fix: Change code to run the CAN at /2 instead.
	Function: 
		+ CAN_Init()
		+ can_SetBaudrate()
2./ Chang I2S set clock protocol. (old protocol generated bitrate value incorrect)
	Function: I2S_FreqConfig() 
	Modify I2S_Mclk example.
			 
*******************************************************************************************************************************

RELEASE: LPC1700CMSIS_24Aug2010

1./ Fix CAN bugs:
	- CAN_SendMsg() function
	- CAN_ReceiveMsg() function: add release buffer on the reception of REMOTE_FRAME
2./ Updat .chm document file

*******************************************************************************************************************************

RELEASE: LPC1700CMSIS_16July2010

1. Modify I2C driver.
	- Add function "I2C_MonitorHandler()"
2. Modify ADC > Burst example, add inject channel function
3. Add new examples:
	- CAN > CAN_LedControl
	- Cortex-M3 > MPU
	- DAC > WaveGenerate
	- I2C > Monitor
	- SPI > SDCard
	- TIMER > FreqMeasure
	- TIMER > Gen_Diff_Delay
	- TIMER > Gen_Diff_Freqs
	- SYSTICK > STCLK
	- USBDEV > USBAudio
	- USBDEV > USBCDC
4. Modify abstract.txt files
5. Rename author name into "NXP MCU SW Application Team"
6. Rename rar file into "LPC1700 Peripheral Driver Library_date.rar"
7. Update document files
8. Fix bug in lpc17xx_ssp.h driver
	- modify 'SSP_DMA_RX' and 'SSP_DMA_TX'
	
*******************************************************************************************************************************

RELEASE: LPC1700CMSIS_18June2010

1./ Modify/update drivers:
	- ADC:
		+ modify function "ADC_GlobalGetData()"
	- CAN:
		+ add function "CAN_SetCommand()"
		+ modify function: "CAN_ModeConfig()"
	- PWR:
		+ modify functions:
			. CLKPWR_DeepSleep()
			. CLKPWR_PowerDown()
	- EXTI:
		+ modify function: EXTI_Init()
	- DAC: 
		+ modify macro "DAC_CCNT_VALUE" value
	- GPIO:
		+ add functions: 
			. GPIO_IntCmd() 
			. GPIO_GetIntStatus()
			. GPIO_ClearInt()
			. FIO_IntCmd()
			. FIO_GetIntStatus()
			. FIO_ClearInt()
	- I2S:
		+ rename macros: 
			. "I2S_CLKSEL_0" -> "I2S_CLKSEL_FRDCLK"
			. "I2S_CLKSEL_1" -> "I2S_CLKSEL_MCLK"
		+ modify macros PARAM_I2S_BITRATE(n)
		+ add functions:
			. I2S_GetIRQStatus()
			. I2S_GetIRQDepth()
	- RTC:
		+ modify functions:
			. RTC_ClearIntPending()
			. RTC_CalibConfig()
	- SSP:
		+ add functions: SSP_GetRawIntStatusReg()
	- TIMER:
		+ modify function: TIM_Init()
	- UART:
		+ add functions:
			. UART_GetIntId()
			. UART_ABClearIntPending()			
2./ Add comment to embed example files in .chm document (generate by doxygen)
3./ Add macro "_DBGFWK" in libcfg files to disable/enable debug framework library
4./ Add new examples: (include both Keil and IAR project)
	- ADC:
		+ Burst
		+ HardwareTrigger
	- CAN:
		+ CAN_self_test
	- Cortex-M3: 
		+ Privilege_mode
	- DAC:
		+ SineWave
	- GPDMA:
		+ GPDMA_Sleep
	- I2S: 
		+ I2S_MCLK
	- NVIC:
		+ Priority
		+ VecTable_Relocation
	- PWR:
		+ NMI_PowerDown
		+ RTC_DeepPWD
		+ WDT_DeepSleep
	- RTC:
		+ Calibration
	- UART:
		+ IrDA (Transmit + Receive)
		+ HWFlowControl	
5./ Modify examples:
6./ Update AN10863_3 (LPC17xx Example Description) and LPC1700CMSIS Manual.chm
7./ Check errata sheet (Errata.lpc1768 rev.02 - 16 March 2010):
	- Errata 3.3 - User must disable and disconnect the main PLL before entering Deep Sleep and Power-down modes
	(apply in NMI_PowerDown and WDT_DeepSleep examples)
	- Errata 3.4: PCLKSELx.1: Peripheral Clock Selection Registers must be set before enabling and connecting PPL0
	(apply in system_LPC17xx.c file)
	- Errata 3.5: MCPWM.1: Input pin (MCI0-2) on the MCPWM peripheral are not functional 
	(removed MCI0-2 out of MCPWM example)
8./ Change using "#define DEBUG" instead of "#define DEBUG 	1" in some lpc17xx_libcfg.h files
9./ Remove instructions that use chip registers in application code, replaced by driver functions
	- EMAC/uIP
	- GIPO/GPIO_Interrupt
	- I2S/I2S_IRQ
	- I2S/I2S_two_kit
	- LCD/NOKIA6610
	- PWR/NMI_PowerDown
	- QEI/QEI_Velo
	- SPI/sc16is750_int
	- SSP/sc16is750_int
	- SSP/Slave
	- UART/Autobaud
	- UART/DMA
	- UART/Interrupt
	- UART/RS485_Slave
	- UART/RS485_Master
	- UART/FullModem
10./ Re-name some Keil projects files in order to keep the naming consistent across projects
11./ Solve error " The project contains the unknow tool 'Coder'" in each IAR projects
12./ Fix some bugs in some project files

*******************************************************************************************************************************

RELEASE: LPC1700CMSIS_21May2010

1./ core_cm3.h: Modify SysTick_Type registers name in core_cm3.h file (for compatible with LPC17xx UM Rev.01 - 4 January 2010)
2./ system_LPC17xx.c: Modify RTC_CLK value (32768Hz) (for compatible with MCB1700 and IAR-LPC1768KS board datasheet)
3./ system_LPC17xx.c > SystemInit(): Add some code lines at the end to set vector table offset value when intialize system
4./ header driver files: re-arrange definitions/structure/functions in header files with this order:
	- include files
	- Public macros
	- Private macros
		+ Bit definitions
		+ check parameter definitions
	- Public Types
		+ enumeration
		+ structure
	- Public Functions
5./ Header driver files:
	- Remove some unused defintion
	- Add new functions 
	- Remove functions that handle interrupt routine and setup call-back function
6./ Header & Source driver files: Remove functions that handle interrupt service routine & setup call-back functions
	- CAN: 
		+ CAN_SetupCBS()
		+ CAN_IntHandler()
	- EMAC:
		+ EMAC_StandardIRQHandler()
		+ EMAC_SetupIntCBS()
	- GPDMA:
		+ GPDMA_IntHandler()
	- I2C:
		+ I2C0_StdIntHandler()
		+ I2C1_StdIntHandler()
		+ I2C1_StdIntHandler()
	- I2S:
		+ I2S_IntHandler()
	- SPI:
		+ SPI_StdIntHandler()
	- SSP:
		+ SSP0_StdIntHandler()
		+ SSP1_StdIntHandler()
	- UART:
		+ UART0_StdIntHandler()
		+ UART1_StdIntHandler()
		+ UART2_StdIntHandler()
		+ UART3_StdIntHandler()
		+ UART_SetupCbs()
7./ Source files:
	- Change some function parameter input
	- Remove some variable used for debugger
	- Remove functions/variables that used to handle interrupt routine and setup call-back function
8./ Change some functions into static mode:
	- CAN:
		+ can_SetBaudrate()
	- EMAC:
		+ setEmacAddr()
		+ emac_CRCCalc()
	- GPIO:
		+ GPIO_GetPointer()
		+ FIO_HalfWordGetPointer()
		+ FIO_ByteGetPointer()
	- I2C:
		+ I2C_getNum()
		+ I2C_SetClock()
	- I2S:
		+ i2s_GetWordWidth()
		+ i2s_GetChannel()
	- PINSEL:
		+ set_PinFunc()
		+ set_ResistorMode()
		+ set_OpenDrainMode()	
9./ Change to define board MCB_LPC1768/IAR_LPC_1768 into #ifdef/#elif method
10./ Update abstract.txt file in each example into new format
11./ Add some functions in example to handle interrupt routine
12./ Add new example:
	- Cortex-M3: Bit-banding
	- GPDMA: Flash_2_Ram_Test
	- PWR: EXTI_Sleep
	- SysTick: 10ms_base
	- TIMER: Polling_Match, PWMSignal
13./ Rename some example
	- DAC: DAC->Speaker
	- GPDMA: Mem_2_Mem_Test -> Ram_2_Ram_Test
	- USBDEV: USBMem -> USBMassStorage
14./ Remove unused examples:
	- RIT:
		+ Polling
		+ Simple
	- TIMER
		+ Delay
15./ startup file for GNU: Add some assembly code line to clear .BSS section before enter to main function (in RAM mode)
16./ ldscript_ram_gnu.ld: Define two variable: 
		+ __bss_start__
		+ __bss_end__
	at the first and the end of .bss section
17./ makefile.ex: add "cleanall" before build ram/rom 
 	So examples can be built continuously without cleaning
18./ Remove FreeRTOS example
19./ Add *.ewd in each IAR example project to configure debugger.
20./ Modify documents:
	+ LPC1000 Software Development Toolchain
	+ LPC17xx Example Description
	+ index.chm (will be rename to "LPC1700CMSIS Manual")
21./ makeconfig: remove unused variable path "ADS_INSTALL_ROOT"
22./ Remove UartDev, SpiDev and EthDev example that delivered by CMSIS 
23./ Modify comments to re-arrange generated document	
24./ Fix bug in UART example (run with UART_PORT 1)
	
*******************************************************************************************************************************

RELEASE: LPC1700CMSIS_07Apr2010

1./ Change all author name into "MCU SW Team"
2./ Add KSZ8721BL PHY definition in emac.h (support for Ethernet Physical Layer Transceiver on IAR eval board)
3./ Remove define PARAM_I2S_DATA(data) in lpc17xx_i2s.h file
4./ Fix a bug in lpc17xx_i2s.h
	original: #define PARAM_I2S_WS_SEL(n)		((n==I2S_MASTER_MODE)||(n=I2S_SLAVE_MODE))
	fixed:    #define PARAM_I2S_WS_SEL(n)		((n==I2S_MASTER_MODE)||(n==I2S_SLAVE_MODE))
5./ Change lpc17xx_libcfg_default.h : use "#define _xxx" instead of "#define _xxx  1"
6./ Change all lpc17xx_libcfg.h in each example: use "#define _xxx" instead of "#define _xxx  1"
    Remove some unused define.
7./ Change lpc17xx_can.c
	- change function: CAN_SetBaudRate (can compute divisor that compliant with all standard CAN baudrate)
	- remove " const uint32_t CAN_BIT_TIME[] " 
	- fix bugs in "CAN_SendMsg" 
	original: 	CANx->TFI1 &= ~0x000F000;
	            CANx->TFI2 &= ~0x000F000;
	            CANx->TFI3 &= ~0x000F000;
	fixed:    	CANx->TFI1 &= ~0x000F0000;
				CANx->TFI2 &= ~0x000F0000;
				CANx->TFI3 &= ~0x000F0000;
8./ Update lpx17xx_emac.c (that can run on KSZ8721BL PHY on IAR eval board)
9./ Remove some unused "break" instruction in:
	- lpc17xx_gpdma.c
	- lpc17xx_i2c.c
	- lpc17xx_i2s.c
	- lpc17xx_pwm.c
	- lpc17xx_rtc.c
	- usbcore.c
10./ Remove CHECK_PARAM(PARAM_I2S_DATA (BufferData)) in I2S_Send( ) function.
11./ lpc17xx_pwm.c: move variable declaration to the head of function (to compatible with Keil platform)
12./ Remove some unused function/variable in lpc17xx_timer.c
13./ Add Keil project in each example
14./ Add one more group "Readme" in IAR projects that include abstract.txt files
15./ Update abstract.txt files some configure instructions to run example on IAR board.
16./ Remove Port_LCD example on GPIO folder.
17./ Add more folder "LCD" that include two example NOKIA6610_LCD that test LCD on MCB board
and QVGA_TFT_LCD that test LCD on IAR board
18./ Fix bugs about incorrect including file on target "LPC1700 Flash" in Keil_RealView_MDK template project
19./ Modify "DiskImg.c" in USBMem example to display "LPC17xx" drive instead "LPC2300" name.
20./ Modify some main functions that allow testing on IAR eval board:
	- ADC\DMA\adc_dma_test.c
	- ADC\INTERRUPT\adc_interrupt_test.c
	- ADC_Polling\adc_polling_test.c
	- EMAC\Easy_Web\Adc.c
	  EMAC\Easy_Web\easy_web.c
	  EMAC\Easy_Web\EMAC.h
	  EMAC\Easy_Web\tcpip.c
	- EMAC\EmacRaw\emactest.c
	- EMAC\uIP\lpc17xx_port\emac.c
	  EMAC\uIP\lpc17xx_port\emac.h
	  EMAC\uIP\lpc17xx_port\main.c
	- GPIO\EINT_PowerDown\eint_powerdown_test.c
	- GPIO\GPIO_Interrupt\gpio_int.c
	- GPIO\LedBlinky\LedBlinky.c
	- RIT\Interrupt\rit_interrupt.c
	- RIT\Polling\rit_polling.c
	- RIT\Simple\rit_simple.c
	- TIMER\Delay\timer_delay_test.c
	- TIMER\Interrupt_Match\timer_interrupt_test.c
	- UART\UART1_FullModem\uart_fullmodem_test.c
	- WDT\INTERRUPT\wdt_interrupt_test.c
	- WDT\RESET\wdt_reset_test.c
		

*******************************************************************************************************************************

RELEASE: LPC1700CMSIS_09Feb2010

1./ Update header file: LPC17xx.h:
	 + Add two more register: CANSLEEPCLR and CANWAKEFLAGS in LPC_SC_TypeDef structure
	 + Fix the wrong align of USB OTG I2C registers
2./ Update IAR and Keil startup file:
	 + Add two more interrupt sources of CAN and USB Activity
3./ Remove folder .\Core\CM3\Example

*******************************************************************************************************************************

RELEASE: LPC1700CMSIS_25Jan2010

1./ Standarlize AN10862_2 to AN10862_3 (LPC1100  Software Development Toolchain)
2./ Update index.chm
3./ Add Eclipse_GNU template in \Example\Project_Template folder

*******************************************************************************************************************************

RELEASE: LPC1700CMSIS_13Jan2010

1./ Fix more fault in coding style to generate properly document
2./ Remove part of the Flash configuration in the CMSIS Library 
    FLASHCFG[11..0]: Reserved (system_LPC17xx.c)

*******************************************************************************************************************************

RELEASE: LPC1700CMSIS_12Jan2010

1./ Modify "system_LPC17xx.c" to suit the PCLKSELx.1 bug (see the errata for LPC1766)
2./ Fix some fault in coding style to generate properly document
3./ Resolve inconsistent line ending in some remain files 

*******************************************************************************************************************************

RELEASE: LPC1700CMSIS_21Dec2009

1./ Update CMSIS ver1.2 to ver1.3
	. Change Core directory
	. Change startup file (from startup_LPC17xx.c into startup_LPC17xx.s)
	. Change LPC17xx header file
	. Change LPC17xx system file
	. Change linker file (both for ROM and RAM)
	. Change makefile
2./ In "makeconfig" file, add more argument "MANUFACTURE"
3./ Verify on Consistency Check report on MCB1700 board
4./ Modify directory for global file in IAR and Keil project
5./ Add "Pa050" in the 'Suppress these diagnostics' in the Diagnostics tab of the C/C++ Compiler options of the IAR project
6./ Update AN10862, AN10863, AN10867.pdf and index.chm 
7./ Remove flags:
	-ffunction-sections 
	-fdata-sections
	-Wl,--gc-sections 
8./ Remove AN10867 and add AN10864 (importing FreeRTOS to LPC17xx CMSIS project)) to index.chm
9./Create new IAR examples in 
	- CAN/CAN_AFLUT_dynamic
	- I2S/I2S_test_4_wire
	- RIT/Interrupt
	- RIT/Polling
	- TIMER/Capture
10./Update all Keil projects to new Keil version uVision 4
11./Resolve missing NVIC entries in startup and header files 
12./Resolve inconsistent line ending

		