- Main Page
- Modules
- Data Structures
- Files
- Examples

- File List
- Globals

# arm_conv_partial_fast_q15.c

Go to the documentation of this file.

    00001 /* ----------------------------------------------------------------------
    00002 * Copyright (C) 2010 ARM Limited. All rights reserved.
    00003 *
    00004 * $Date:        15. July 2011
    00005 * $Revision:    V1.0.10
    00006 *
    00007 * Project:      CMSIS DSP Library
    00008 * Title:        arm_conv_partial_fast_q15.c
    00009 *
    00010 * Description:  Fast Q15 Partial convolution.
    00011 *
    00012 * Target Processor: Cortex-M4/Cortex-M3
    00013 *
    00014 * Version 1.0.10 2011/7/15
    00015 *    Big Endian support added and Merged M0 and M3/M4 Source code.
    00016 *
    00017 * Version 1.0.3 2010/11/29
    00018 *    Re-organized the CMSIS folders and updated documentation.
    00019 *
    00020 * Version 1.0.2 2010/11/11
    00021 *    Documentation updated.
    00022 *
    00023 * Version 1.0.1 2010/10/05
    00024 *    Production release and review comments incorporated.
    00025 *
    00026 * Version 1.0.0 2010/09/20
    00027 *    Production release and review comments incorporated.
    00028 * -------------------------------------------------------------------- */
    00029
    00030 #include "arm_math.h"
    00031
    00056 arm_status arm_conv_partial_fast_q15(
    00057   q15_t * pSrcA,
    00058   uint32_t srcALen,
    00059   q15_t * pSrcB,
    00060   uint32_t srcBLen,
    00061   q15_t * pDst,
    00062   uint32_t firstIndex,
    00063   uint32_t numPoints)
    00064 {
    00065   q15_t *pIn1;                                   /* inputA pointer               */
    00066   q15_t *pIn2;                                   /* inputB pointer               */
    00067   q15_t *pOut = pDst;                            /* output pointer               */
    00068   q31_t sum, acc0, acc1, acc2, acc3;             /* Accumulator                  */
    00069   q15_t *px;                                     /* Intermediate inputA pointer  */
    00070   q15_t *py;                                     /* Intermediate inputB pointer  */
    00071   q15_t *pSrc1, *pSrc2;                          /* Intermediate pointers        */
    00072   q31_t x0, x1, x2, x3, c0;
    00073   uint32_t j, k, count, check, blkCnt;
    00074   int32_t blockSize1, blockSize2, blockSize3;    /* loop counters                 */
    00075   arm_status status;                             /* status of Partial convolution */
    00076   q31_t *pb;                                     /* 32 bit pointer for inputB buffer */
    00077
    00078   /* Check for range of output samples to be calculated */
    00079   if((firstIndex + numPoints) > ((srcALen + (srcBLen - 1u))))
    00080   {
    00081     /* Set status as ARM_MATH_ARGUMENT_ERROR */
    00082     status = ARM_MATH_ARGUMENT_ERROR;
    00083   }
    00084   else
    00085   {
    00086
    00087     /* The algorithm implementation is based on the lengths of the inputs. */
    00088     /* srcB is always made to slide across srcA. */
    00089     /* So srcBLen is always considered as shorter or equal to srcALen */
    00090     if(srcALen >= srcBLen)
    00091     {
    00092       /* Initialization of inputA pointer */
    00093       pIn1 = pSrcA;
    00094
    00095       /* Initialization of inputB pointer */
    00096       pIn2 = pSrcB;
    00097     }
    00098     else
    00099     {
    00100       /* Initialization of inputA pointer */
    00101       pIn1 = pSrcB;
    00102
    00103       /* Initialization of inputB pointer */
    00104       pIn2 = pSrcA;
    00105
    00106       /* srcBLen is always considered as shorter or equal to srcALen */
    00107       j = srcBLen;
    00108       srcBLen = srcALen;
    00109       srcALen = j;
    00110     }
    00111
    00112     /* Conditions to check which loopCounter holds
    00113      * the first and last indices of the output samples to be calculated. */
    00114     check = firstIndex + numPoints;
    00115     blockSize3 = ((int32_t) check - (int32_t) srcALen);
    00116     blockSize3 = (blockSize3 > 0) ? blockSize3 : 0;
    00117     blockSize1 = (((int32_t) srcBLen - 1) - (int32_t) firstIndex);
    00118     blockSize1 = (blockSize1 > 0) ? ((check > (srcBLen - 1u)) ? blockSize1 :
    00119                                      (int32_t) numPoints) : 0;
    00120     blockSize2 = (int32_t) check - ((blockSize3 + blockSize1) +
    00121                                     (int32_t) firstIndex);
    00122     blockSize2 = (blockSize2 > 0) ? blockSize2 : 0;
    00123
    00124     /* conv(x,y) at n = x[n] * y[0] + x[n-1] * y[1] + x[n-2] * y[2] + ...+ x[n-N+1] * y[N -1] */
    00125     /* The function is internally
    00126      * divided into three stages according to the number of multiplications that has to be
    00127      * taken place between inputA samples and inputB samples. In the first stage of the
    00128      * algorithm, the multiplications increase by one for every iteration.
    00129      * In the second stage of the algorithm, srcBLen number of multiplications are done.
    00130      * In the third stage of the algorithm, the multiplications decrease by one
    00131      * for every iteration. */
    00132
    00133     /* Set the output pointer to point to the firstIndex
    00134      * of the output sample to be calculated. */
    00135     pOut = pDst + firstIndex;
    00136
    00137     /* --------------------------
    00138      * Initializations of stage1
    00139      * -------------------------*/
    00140
    00141     /* sum = x[0] * y[0]
    00142      * sum = x[0] * y[1] + x[1] * y[0]
    00143      * ....
    00144      * sum = x[0] * y[srcBlen - 1] + x[1] * y[srcBlen - 2] +...+ x[srcBLen - 1] * y[0]
    00145      */
    00146
    00147     /* In this stage the MAC operations are increased by 1 for every iteration.
    00148        The count variable holds the number of MAC operations performed.
    00149        Since the partial convolution starts from firstIndex
    00150        Number of Macs to be performed is firstIndex + 1 */
    00151     count = 1u + firstIndex;
    00152
    00153     /* Working pointer of inputA */
    00154     px = pIn1;
    00155
    00156     /* Working pointer of inputB */
    00157     pSrc2 = pIn2 + firstIndex;
    00158     py = pSrc2;
    00159
    00160     /* ------------------------
    00161      * Stage1 process
    00162      * ----------------------*/
    00163
    00164     /* For loop unrolling by 4, this stage is divided into two. */
    00165     /* First part of this stage computes the MAC operations less than 4 */
    00166     /* Second part of this stage computes the MAC operations greater than or equal to 4 */
    00167
    00168     /* The first part of the stage starts here */
    00169     while((count < 4u) && (blockSize1 > 0))
    00170     {
    00171       /* Accumulator is made zero for every iteration */
    00172       sum = 0;
    00173
    00174       /* Loop over number of MAC operations between
    00175        * inputA samples and inputB samples */
    00176       k = count;
    00177
    00178       while(k > 0u)
    00179       {
    00180         /* Perform the multiply-accumulates */
    00181         sum = __SMLAD(*px++, *py--, sum);
    00182
    00183         /* Decrement the loop counter */
    00184         k--;
    00185       }
    00186
    00187       /* Store the result in the accumulator in the destination buffer. */
    00188       *pOut++ = (q15_t) (sum >> 15);
    00189
    00190       /* Update the inputA and inputB pointers for next MAC calculation */
    00191       py = ++pSrc2;
    00192       px = pIn1;
    00193
    00194       /* Increment the MAC count */
    00195       count++;
    00196
    00197       /* Decrement the loop counter */
    00198       blockSize1--;
    00199     }
    00200
    00201     /* The second part of the stage starts here */
    00202     /* The internal loop, over count, is unrolled by 4 */
    00203     /* To, read the last two inputB samples using SIMD:
    00204      * y[srcBLen] and y[srcBLen-1] coefficients, py is decremented by 1 */
    00205     py = py - 1;
    00206
    00207     while(blockSize1 > 0)
    00208     {
    00209       /* Accumulator is made zero for every iteration */
    00210       sum = 0;
    00211
    00212       /* Apply loop unrolling and compute 4 MACs simultaneously. */
    00213       k = count >> 2u;
    00214
    00215       /* First part of the processing with loop unrolling.  Compute 4 MACs at a time.
    00216        ** a second loop below computes MACs for the remaining 1 to 3 samples. */
    00217       while(k > 0u)
    00218       {
    00219         /* Perform the multiply-accumulates */
    00220         /* x[0], x[1] are multiplied with y[srcBLen - 1], y[srcBLen - 2] respectively */
    00221         sum = __SMLADX(*__SIMD32(px)++, *__SIMD32(py)--, sum);
    00222         /* x[2], x[3] are multiplied with y[srcBLen - 3], y[srcBLen - 4] respectively */
    00223         sum = __SMLADX(*__SIMD32(px)++, *__SIMD32(py)--, sum);
    00224
    00225         /* Decrement the loop counter */
    00226         k--;
    00227       }
    00228
    00229       /* For the next MAC operations, the pointer py is used without SIMD
    00230        * So, py is incremented by 1 */
    00231       py = py + 1u;
    00232
    00233       /* If the count is not a multiple of 4, compute any remaining MACs here.
    00234        ** No loop unrolling is used. */
    00235       k = count % 0x4u;
    00236
    00237       while(k > 0u)
    00238       {
    00239         /* Perform the multiply-accumulates */
    00240         sum = __SMLAD(*px++, *py--, sum);
    00241
    00242         /* Decrement the loop counter */
    00243         k--;
    00244       }
    00245
    00246       /* Store the result in the accumulator in the destination buffer. */
    00247       *pOut++ = (q15_t) (sum >> 15);
    00248
    00249       /* Update the inputA and inputB pointers for next MAC calculation */
    00250       py = ++pSrc2 - 1u;
    00251       px = pIn1;
    00252
    00253       /* Increment the MAC count */
    00254       count++;
    00255
    00256       /* Decrement the loop counter */
    00257       blockSize1--;
    00258     }
    00259
    00260     /* --------------------------
    00261      * Initializations of stage2
    00262      * ------------------------*/
    00263
    00264     /* sum = x[0] * y[srcBLen-1] + x[1] * y[srcBLen-2] +...+ x[srcBLen-1] * y[0]
    00265      * sum = x[1] * y[srcBLen-1] + x[2] * y[srcBLen-2] +...+ x[srcBLen] * y[0]
    00266      * ....
    00267      * sum = x[srcALen-srcBLen-2] * y[srcBLen-1] + x[srcALen] * y[srcBLen-2] +...+ x[srcALen-1] * y[0]
    00268      */
    00269
    00270     /* Working pointer of inputA */
    00271     px = pIn1;
    00272
    00273     /* Working pointer of inputB */
    00274     pSrc2 = pIn2 + (srcBLen - 1u);
    00275     py = pSrc2;
    00276
    00277     /* Initialize inputB pointer of type q31 */
    00278     pb = (q31_t *) (py - 1u);
    00279
    00280     /* count is the index by which the pointer pIn1 to be incremented */
    00281     count = 1u;
    00282
    00283
    00284     /* --------------------
    00285      * Stage2 process
    00286      * -------------------*/
    00287
    00288     /* Stage2 depends on srcBLen as in this stage srcBLen number of MACS are performed.
    00289      * So, to loop unroll over blockSize2,
    00290      * srcBLen should be greater than or equal to 4 */
    00291     if(srcBLen >= 4u)
    00292     {
    00293       /* Loop unroll over blockSize2, by 4 */
    00294       blkCnt = ((uint32_t) blockSize2 >> 2u);
    00295
    00296       while(blkCnt > 0u)
    00297       {
    00298         /* Set all accumulators to zero */
    00299         acc0 = 0;
    00300         acc1 = 0;
    00301         acc2 = 0;
    00302         acc3 = 0;
    00303
    00304
    00305         /* read x[0], x[1] samples */
    00306         x0 = *(q31_t *) (px++);
    00307         /* read x[1], x[2] samples */
    00308         x1 = *(q31_t *) (px++);
    00309
    00310
    00311         /* Apply loop unrolling and compute 4 MACs simultaneously. */
    00312         k = srcBLen >> 2u;
    00313
    00314         /* First part of the processing with loop unrolling.  Compute 4 MACs at a time.
    00315          ** a second loop below computes MACs for the remaining 1 to 3 samples. */
    00316         do
    00317         {
    00318           /* Read the last two inputB samples using SIMD:
    00319            * y[srcBLen - 1] and y[srcBLen - 2] */
    00320           c0 = *(pb--);
    00321
    00322           /* acc0 +=  x[0] * y[srcBLen - 1] + x[1] * y[srcBLen - 2] */
    00323           acc0 = __SMLADX(x0, c0, acc0);
    00324
    00325           /* acc1 +=  x[1] * y[srcBLen - 1] + x[2] * y[srcBLen - 2] */
    00326           acc1 = __SMLADX(x1, c0, acc1);
    00327
    00328           /* Read x[2], x[3] */
    00329           x2 = *(q31_t *) (px++);
    00330
    00331           /* Read x[3], x[4] */
    00332           x3 = *(q31_t *) (px++);
    00333
    00334           /* acc2 +=  x[2] * y[srcBLen - 1] + x[3] * y[srcBLen - 2] */
    00335           acc2 = __SMLADX(x2, c0, acc2);
    00336
    00337           /* acc3 +=  x[3] * y[srcBLen - 1] + x[4] * y[srcBLen - 2] */
    00338           acc3 = __SMLADX(x3, c0, acc3);
    00339
    00340           /* Read y[srcBLen - 3] and y[srcBLen - 4] */
    00341           c0 = *(pb--);
    00342
    00343           /* acc0 +=  x[2] * y[srcBLen - 3] + x[3] * y[srcBLen - 4] */
    00344           acc0 = __SMLADX(x2, c0, acc0);
    00345
    00346           /* acc1 +=  x[3] * y[srcBLen - 3] + x[4] * y[srcBLen - 4] */
    00347           acc1 = __SMLADX(x3, c0, acc1);
    00348
    00349           /* Read x[4], x[5] */
    00350           x0 = *(q31_t *) (px++);
    00351
    00352           /* Read x[5], x[6] */
    00353           x1 = *(q31_t *) (px++);
    00354
    00355           /* acc2 +=  x[4] * y[srcBLen - 3] + x[5] * y[srcBLen - 4] */
    00356           acc2 = __SMLADX(x0, c0, acc2);
    00357
    00358           /* acc3 +=  x[5] * y[srcBLen - 3] + x[6] * y[srcBLen - 4] */
    00359           acc3 = __SMLADX(x1, c0, acc3);
    00360
    00361         } while(--k);
    00362
    00363         /* For the next MAC operations, SIMD is not used
    00364          * So, the 16 bit pointer if inputB, py is updated */
    00365         py = (q15_t *) pb;
    00366         py = py + 1;
    00367
    00368         /* If the srcBLen is not a multiple of 4, compute any remaining MACs here.
    00369          ** No loop unrolling is used. */
    00370         k = srcBLen % 0x4u;
    00371
    00372         if(k == 1u)
    00373         {
    00374           /* Read y[srcBLen - 5] */
    00375           c0 = *(py);
    00376 #ifdef  ARM_MATH_BIG_ENDIAN
    00377
    00378           c0 = c0 << 16;
    00379
    00380 #endif /*      #ifdef  ARM_MATH_BIG_ENDIAN     */
    00381
    00382           /* Read x[7] */
    00383           x3 = *(q31_t *) px++;
    00384
    00385           /* Perform the multiply-accumulates */
    00386           acc0 = __SMLAD(x0, c0, acc0);
    00387           acc1 = __SMLAD(x1, c0, acc1);
    00388           acc2 = __SMLADX(x1, c0, acc2);
    00389           acc3 = __SMLADX(x3, c0, acc3);
    00390         }
    00391
    00392         if(k == 2u)
    00393         {
    00394           /* Read y[srcBLen - 5], y[srcBLen - 6] */
    00395           c0 = *(pb);
    00396
    00397           /* Read x[7], x[8] */
    00398           x3 = *(q31_t *) px++;
    00399
    00400           /* Read x[9] */
    00401           x2 = *(q31_t *) px++;
    00402
    00403           /* Perform the multiply-accumulates */
    00404           acc0 = __SMLADX(x0, c0, acc0);
    00405           acc1 = __SMLADX(x1, c0, acc1);
    00406           acc2 = __SMLADX(x3, c0, acc2);
    00407           acc3 = __SMLADX(x2, c0, acc3);
    00408         }
    00409
    00410         if(k == 3u)
    00411         {
    00412           /* Read y[srcBLen - 5], y[srcBLen - 6] */
    00413           c0 = *pb--;
    00414
    00415           /* Read x[7], x[8] */
    00416           x3 = *(q31_t *) px++;
    00417
    00418           /* Read x[9] */
    00419           x2 = *(q31_t *) px++;
    00420
    00421           /* Perform the multiply-accumulates */
    00422           acc0 = __SMLADX(x0, c0, acc0);
    00423           acc1 = __SMLADX(x1, c0, acc1);
    00424           acc2 = __SMLADX(x3, c0, acc2);
    00425           acc3 = __SMLADX(x2, c0, acc3);
    00426
    00427           /* Read y[srcBLen - 7] */
    00428 #ifdef  ARM_MATH_BIG_ENDIAN
    00429
    00430           c0 = (*pb);
    00431           c0 = (c0) << 16;
    00432
    00433 #else
    00434
    00435           c0 = (q15_t) (*pb >> 16);
    00436
    00437 #endif /*      #ifdef  ARM_MATH_BIG_ENDIAN     */
    00438
    00439           /* Read x[10] */
    00440           x3 = *(q31_t *) px++;
    00441
    00442           /* Perform the multiply-accumulates */
    00443           acc0 = __SMLADX(x1, c0, acc0);
    00444           acc1 = __SMLAD(x2, c0, acc1);
    00445           acc2 = __SMLADX(x2, c0, acc2);
    00446           acc3 = __SMLADX(x3, c0, acc3);
    00447         }
    00448
    00449         /* Store the results in the accumulators in the destination buffer. */
    00450 #ifndef ARM_MATH_BIG_ENDIAN
    00451
    00452         *__SIMD32(pOut)++ = __PKHBT(acc0 >> 15, acc1 >> 15, 16);
    00453         *__SIMD32(pOut)++ = __PKHBT(acc2 >> 15, acc3 >> 15, 16);
    00454
    00455 #else
    00456
    00457         *__SIMD32(pOut)++ = __PKHBT(acc1 >> 15, acc0 >> 15, 16);
    00458         *__SIMD32(pOut)++ = __PKHBT(acc3 >> 15, acc2 >> 15, 16);
    00459
    00460 #endif /*      #ifndef  ARM_MATH_BIG_ENDIAN    */
    00461
    00462         /* Update the inputA and inputB pointers for next MAC calculation */
    00463         px = pIn1 + (count * 4u);
    00464         py = pSrc2;
    00465         pb = (q31_t *) (py - 1);
    00466
    00467         /* Increment the pointer pIn1 index, count by 1 */
    00468         count++;
    00469
    00470         /* Decrement the loop counter */
    00471         blkCnt--;
    00472       }
    00473
    00474       /* If the blockSize2 is not a multiple of 4, compute any remaining output samples here.
    00475        ** No loop unrolling is used. */
    00476       blkCnt = (uint32_t) blockSize2 % 0x4u;
    00477
    00478       while(blkCnt > 0u)
    00479       {
    00480         /* Accumulator is made zero for every iteration */
    00481         sum = 0;
    00482
    00483         /* Apply loop unrolling and compute 4 MACs simultaneously. */
    00484         k = srcBLen >> 2u;
    00485
    00486         /* First part of the processing with loop unrolling.  Compute 4 MACs at a time.
    00487          ** a second loop below computes MACs for the remaining 1 to 3 samples. */
    00488         while(k > 0u)
    00489         {
    00490           /* Perform the multiply-accumulates */
    00491           sum += ((q31_t) * px++ * *py--);
    00492           sum += ((q31_t) * px++ * *py--);
    00493           sum += ((q31_t) * px++ * *py--);
    00494           sum += ((q31_t) * px++ * *py--);
    00495
    00496           /* Decrement the loop counter */
    00497           k--;
    00498         }
    00499
    00500         /* If the srcBLen is not a multiple of 4, compute any remaining MACs here.
    00501          ** No loop unrolling is used. */
    00502         k = srcBLen % 0x4u;
    00503
    00504         while(k > 0u)
    00505         {
    00506           /* Perform the multiply-accumulates */
    00507           sum += ((q31_t) * px++ * *py--);
    00508
    00509           /* Decrement the loop counter */
    00510           k--;
    00511         }
    00512
    00513         /* Store the result in the accumulator in the destination buffer. */
    00514         *pOut++ = (q15_t) (sum >> 15);
    00515
    00516         /* Update the inputA and inputB pointers for next MAC calculation */
    00517         px = pIn1 + count;
    00518         py = pSrc2;
    00519
    00520         /* Increment the pointer pIn1 index, count by 1 */
    00521         count++;
    00522
    00523         /* Decrement the loop counter */
    00524         blkCnt--;
    00525       }
    00526     }
    00527     else
    00528     {
    00529       /* If the srcBLen is not a multiple of 4,
    00530        * the blockSize2 loop cannot be unrolled by 4 */
    00531       blkCnt = (uint32_t) blockSize2;
    00532
    00533       while(blkCnt > 0u)
    00534       {
    00535         /* Accumulator is made zero for every iteration */
    00536         sum = 0;
    00537
    00538         /* srcBLen number of MACS should be performed */
    00539         k = srcBLen;
    00540
    00541         while(k > 0u)
    00542         {
    00543           /* Perform the multiply-accumulate */
    00544           sum += ((q31_t) * px++ * *py--);
    00545
    00546           /* Decrement the loop counter */
    00547           k--;
    00548         }
    00549
    00550         /* Store the result in the accumulator in the destination buffer. */
    00551         *pOut++ = (q15_t) (sum >> 15);
    00552
    00553         /* Update the inputA and inputB pointers for next MAC calculation */
    00554         px = pIn1 + count;
    00555         py = pSrc2;
    00556
    00557         /* Increment the MAC count */
    00558         count++;
    00559
    00560         /* Decrement the loop counter */
    00561         blkCnt--;
    00562       }
    00563     }
    00564
    00565
    00566     /* --------------------------
    00567      * Initializations of stage3
    00568      * -------------------------*/
    00569
    00570     /* sum += x[srcALen-srcBLen+1] * y[srcBLen-1] + x[srcALen-srcBLen+2] * y[srcBLen-2] +...+ x[srcALen-1] * y[1]
    00571      * sum += x[srcALen-srcBLen+2] * y[srcBLen-1] + x[srcALen-srcBLen+3] * y[srcBLen-2] +...+ x[srcALen-1] * y[2]
    00572      * ....
    00573      * sum +=  x[srcALen-2] * y[srcBLen-1] + x[srcALen-1] * y[srcBLen-2]
    00574      * sum +=  x[srcALen-1] * y[srcBLen-1]
    00575      */
    00576
    00577     /* In this stage the MAC operations are decreased by 1 for every iteration.
    00578        The count variable holds the number of MAC operations performed */
    00579     count = srcBLen - 1u;
    00580
    00581     /* Working pointer of inputA */
    00582     pSrc1 = (pIn1 + srcALen) - (srcBLen - 1u);
    00583     px = pSrc1;
    00584
    00585     /* Working pointer of inputB */
    00586     pSrc2 = pIn2 + (srcBLen - 1u);
    00587     pIn2 = pSrc2 - 1u;
    00588     py = pIn2;
    00589
    00590     /* -------------------
    00591      * Stage3 process
    00592      * ------------------*/
    00593
    00594     /* For loop unrolling by 4, this stage is divided into two. */
    00595     /* First part of this stage computes the MAC operations greater than 4 */
    00596     /* Second part of this stage computes the MAC operations less than or equal to 4 */
    00597
    00598     /* The first part of the stage starts here */
    00599     j = count >> 2u;
    00600
    00601     while((j > 0u) && (blockSize3 > 0))
    00602     {
    00603       /* Accumulator is made zero for every iteration */
    00604       sum = 0;
    00605
    00606       /* Apply loop unrolling and compute 4 MACs simultaneously. */
    00607       k = count >> 2u;
    00608
    00609       /* First part of the processing with loop unrolling.  Compute 4 MACs at a time.
    00610        ** a second loop below computes MACs for the remaining 1 to 3 samples. */
    00611       while(k > 0u)
    00612       {
    00613         /* x[srcALen - srcBLen + 1], x[srcALen - srcBLen + 2] are multiplied
    00614          * with y[srcBLen - 1], y[srcBLen - 2] respectively */
    00615         sum = __SMLADX(*__SIMD32(px)++, *__SIMD32(py)--, sum);
    00616         /* x[srcALen - srcBLen + 3], x[srcALen - srcBLen + 4] are multiplied
    00617          * with y[srcBLen - 3], y[srcBLen - 4] respectively */
    00618         sum = __SMLADX(*__SIMD32(px)++, *__SIMD32(py)--, sum);
    00619
    00620         /* Decrement the loop counter */
    00621         k--;
    00622       }
    00623
    00624       /* For the next MAC operations, the pointer py is used without SIMD
    00625        * So, py is incremented by 1 */
    00626       py = py + 1u;
    00627
    00628       /* If the count is not a multiple of 4, compute any remaining MACs here.
    00629        ** No loop unrolling is used. */
    00630       k = count % 0x4u;
    00631
    00632       while(k > 0u)
    00633       {
    00634         /* sum += x[srcALen - srcBLen + 5] * y[srcBLen - 5] */
    00635         sum = __SMLAD(*px++, *py--, sum);
    00636
    00637         /* Decrement the loop counter */
    00638         k--;
    00639       }
    00640
    00641       /* Store the result in the accumulator in the destination buffer. */
    00642       *pOut++ = (q15_t) (sum >> 15);
    00643
    00644       /* Update the inputA and inputB pointers for next MAC calculation */
    00645       px = ++pSrc1;
    00646       py = pIn2;
    00647
    00648       /* Decrement the MAC count */
    00649       count--;
    00650
    00651       /* Decrement the loop counter */
    00652       blockSize3--;
    00653
    00654       j--;
    00655     }
    00656
    00657     /* The second part of the stage starts here */
    00658     /* SIMD is not used for the next MAC operations,
    00659      * so pointer py is updated to read only one sample at a time */
    00660     py = py + 1u;
    00661
    00662     while(blockSize3 > 0)
    00663     {
    00664       /* Accumulator is made zero for every iteration */
    00665       sum = 0;
    00666
    00667       /* Apply loop unrolling and compute 4 MACs simultaneously. */
    00668       k = count;
    00669
    00670       while(k > 0u)
    00671       {
    00672         /* Perform the multiply-accumulates */
    00673         /* sum +=  x[srcALen-1] * y[srcBLen-1] */
    00674         sum = __SMLAD(*px++, *py--, sum);
    00675
    00676         /* Decrement the loop counter */
    00677         k--;
    00678       }
    00679
    00680       /* Store the result in the accumulator in the destination buffer. */
    00681       *pOut++ = (q15_t) (sum >> 15);
    00682
    00683       /* Update the inputA and inputB pointers for next MAC calculation */
    00684       px = ++pSrc1;
    00685       py = pSrc2;
    00686
    00687       /* Decrement the MAC count */
    00688       count--;
    00689
    00690       /* Decrement the loop counter */
    00691       blockSize3--;
    00692     }
    00693
    00694     /* set status as ARM_MATH_SUCCESS */
    00695     status = ARM_MATH_SUCCESS;
    00696   }
    00697
    00698   /* Return to application */
    00699   return (status);
    00700
    00701 }
    00702

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines