- Main Page
- Modules
- Data Structures
- Files
- Examples

- File List
- Globals

# arm_q7_to_q15.c

Go to the documentation of this file.

    00001 /* ----------------------------------------------------------------------------
    00002 * Copyright (C) 2010 ARM Limited. All rights reserved.
    00003 *
    00004 * $Date:        15. July 2011
    00005 * $Revision:    V1.0.10
    00006 *
    00007 * Project:      CMSIS DSP Library
    00008 * Title:        arm_q7_to_q15.c
    00009 *
    00010 * Description:  Converts the elements of the Q7 vector to Q15 vector.
    00011 *
    00012 * Target Processor: Cortex-M4/Cortex-M3/Cortex-M0
    00013 *
    00014 * Version 1.0.10 2011/7/15
    00015 *    Big Endian support added and Merged M0 and M3/M4 Source code.
    00016 *
    00017 * Version 1.0.3 2010/11/29
    00018 *    Re-organized the CMSIS folders and updated documentation.
    00019 *
    00020 * Version 1.0.2 2010/11/11
    00021 *    Documentation updated.
    00022 *
    00023 * Version 1.0.1 2010/10/05
    00024 *    Production release and review comments incorporated.
    00025 *
    00026 * Version 1.0.0 2010/09/20
    00027 *    Production release and review comments incorporated.
    00028 * ---------------------------------------------------------------------------- */
    00029
    00030 #include "arm_math.h"
    00031
    00062 void arm_q7_to_q15(
    00063   q7_t * pSrc,
    00064   q15_t * pDst,
    00065   uint32_t blockSize)
    00066 {
    00067   q7_t *pIn = pSrc;                              /* Src pointer */
    00068   uint32_t blkCnt;                               /* loop counter */
    00069
    00070 #ifndef ARM_MATH_CM0
    00071
    00072   /* Run the below code for Cortex-M4 and Cortex-M3 */
    00073
    00074   /*loop Unrolling */
    00075   blkCnt = blockSize >> 2u;
    00076
    00077   /* First part of the processing with loop unrolling.  Compute 4 outputs at a time.
    00078    ** a second loop below computes the remaining 1 to 3 samples. */
    00079   while(blkCnt > 0u)
    00080   {
    00081     /* C = (q15_t) A << 8 */
    00082     /* convert from q7 to q15 and then store the results in the destination buffer */
    00083     *pDst++ = (q15_t) * pIn++ << 8;
    00084     *pDst++ = (q15_t) * pIn++ << 8;
    00085     *pDst++ = (q15_t) * pIn++ << 8;
    00086     *pDst++ = (q15_t) * pIn++ << 8;
    00087
    00088     /* Decrement the loop counter */
    00089     blkCnt--;
    00090   }
    00091
    00092   /* If the blockSize is not a multiple of 4, compute any remaining output samples here.
    00093    ** No loop unrolling is used. */
    00094   blkCnt = blockSize % 0x4u;
    00095
    00096 #else
    00097
    00098   /* Run the below code for Cortex-M0 */
    00099
    00100   /* Loop over blockSize number of values */
    00101   blkCnt = blockSize;
    00102
    00103 #endif /* #ifndef ARM_MATH_CM0 */
    00104
    00105   while(blkCnt > 0u)
    00106   {
    00107     /* C = (q15_t) A << 8 */
    00108     /* convert from q7 to q15 and then store the results in the destination buffer */
    00109     *pDst++ = (q15_t) * pIn++ << 8;
    00110
    00111     /* Decrement the loop counter */
    00112     blkCnt--;
    00113   }
    00114
    00115 }
    00116

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines