- Main Page
- Modules
- Data Structures
- Files
- Examples

- File List
- Globals

# arm_mult_q7.c

Go to the documentation of this file.

    00001 /* ----------------------------------------------------------------------
    00002 * Copyright (C) 2010 ARM Limited. All rights reserved.
    00003 *
    00004 * $Date:        15. July 2011
    00005 * $Revision:    V1.0.10
    00006 *
    00007 * Project:      CMSIS DSP Library
    00008 * Title:        arm_mult_q7.c
    00009 *
    00010 * Description:  Q7 vector multiplication.
    00011 *
    00012 * Target Processor: Cortex-M4/Cortex-M3/Cortex-M0
    00013 *
    00014 * Version 1.0.10 2011/7/15
    00015 *    Big Endian support added and Merged M0 and M3/M4 Source code.
    00016 *
    00017 * Version 1.0.3 2010/11/29
    00018 *    Re-organized the CMSIS folders and updated documentation.
    00019 *
    00020 * Version 1.0.2 2010/11/11
    00021 *    Documentation updated.
    00022 *
    00023 * Version 1.0.1 2010/10/05
    00024 *    Production release and review comments incorporated.
    00025 *
    00026 * Version 1.0.0 2010/09/20
    00027 *    Production release and review comments incorporated.
    00028 *
    00029 * Version 0.0.7  2010/06/10
    00030 *    Misra-C changes done
    00031 *
    00032 * Version 0.0.5  2010/04/26
    00033 *    incorporated review comments and updated with latest CMSIS layer
    00034 *
    00035 * Version 0.0.3  2010/03/10 DP
    00036 *    Initial version
    00037 * -------------------------------------------------------------------- */
    00038
    00039 #include "arm_math.h"
    00040
    00064 void arm_mult_q7(
    00065   q7_t * pSrcA,
    00066   q7_t * pSrcB,
    00067   q7_t * pDst,
    00068   uint32_t blockSize)
    00069 {
    00070   uint32_t blkCnt;                               /* loop counters */
    00071
    00072 #ifndef ARM_MATH_CM0
    00073
    00074 /* Run the below code for Cortex-M4 and Cortex-M3 */
    00075   q7_t out1, out2, out3, out4;                   /* Temporary variables to store the product */
    00076
    00077   /* loop Unrolling */
    00078   blkCnt = blockSize >> 2u;
    00079
    00080   /* First part of the processing with loop unrolling.  Compute 4 outputs at a time.
    00081    ** a second loop below computes the remaining 1 to 3 samples. */
    00082   while(blkCnt > 0u)
    00083   {
    00084     /* C = A * B */
    00085     /* Multiply the inputs and store the results in temporary variables */
    00086     out1 = (q7_t) (((q15_t) (*pSrcA++) * (*pSrcB++)) >> 7);
    00087     out2 = (q7_t) (((q15_t) (*pSrcA++) * (*pSrcB++)) >> 7);
    00088     out3 = (q7_t) (((q15_t) (*pSrcA++) * (*pSrcB++)) >> 7);
    00089     out4 = (q7_t) (((q15_t) (*pSrcA++) * (*pSrcB++)) >> 7);
    00090
    00091     /* Store the results of 4 inputs in the destination buffer in single cycle by packing */
    00092     *__SIMD32(pDst)++ = __PACKq7(out1, out2, out3, out4);
    00093
    00094     /* Decrement the blockSize loop counter */
    00095     blkCnt--;
    00096   }
    00097
    00098   /* If the blockSize is not a multiple of 4, compute any remaining output samples here.
    00099    ** No loop unrolling is used. */
    00100   blkCnt = blockSize % 0x4u;
    00101
    00102 #else
    00103
    00104   /* Run the below code for Cortex-M0 */
    00105
    00106   /* Initialize blkCnt with number of samples */
    00107   blkCnt = blockSize;
    00108
    00109 #endif /* #ifndef ARM_MATH_CM0 */
    00110
    00111
    00112   while(blkCnt > 0u)
    00113   {
    00114     /* C = A * B */
    00115     /* Multiply the inputs and store the result in the destination buffer */
    00116     *pDst++ = (q7_t) (((q15_t) (*pSrcA++) * (*pSrcB++)) >> 7);
    00117
    00118     /* Decrement the blockSize loop counter */
    00119     blkCnt--;
    00120   }
    00121 }
    00122

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines