Version of RDC FPGA for 7111 (Russian) DDS/FLS system

Bin file is rdc1802.bin

This version has timing adjustments on the input serial data from the receivers as suggested by RAS. Since this version is not tested with older boards this will be a separate branch awaiting further testing and qualification. At which time if deemed appropriate it will become main line code.

This version does not have BITE but the revision register is implemented and should read 1802 (hex) when accessed thorough the debug board. 
