STX CPLD for 7150 transmitter boards

Board type register included 
Revision register is at offset D hex and bits 7:4 are the type and bits 3:0 are revision

There are two versions 

stxcpx11.jed – type = 1 rev = 1

stxcpx21.jed – type = 2 rev = 1

Both are identical except for the type field
