LCU FPGA (Rev “C”)
Bin file is lcuC22C.bin – dual uplink, non dual mpa
This revision has error reporting function on the receive ports and diagnostic register for DSP. 

Error reporting: The individual error bits (7:0) are presented to the DSP in the order indicated in the ICD. The error register is located at offset 25 (hexadecimal). The error register is updated after each DSP read to that address, synchronized to FPGA 80 MHz clock. Bit 15 is driven to 0 and unused bits (14:8) are driven to 0.

Diagnostic register: The DSP can write the register at offset 40 (hexadecimal) with an arbitrary 16 bit value and can read that value negated at offset 41 (hexadecimal).
