Revised code for 7125 MR4 release
lcu9224.bin – single uplink, BITE enabled, all Mezzanine switches power up inactive, DSP subsequently controls
