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[bookmark: _GoBack][bookmark: _GoBack]

	Date:
	[bookmark: Text81][bookmark: Text8][bookmark: Text8][bookmark: Text8]  Aug 18, 2020   

	Vehicle:
	[bookmark: __Fieldmark__23_3623662241][bookmark: __Fieldmark__23_3623662241][bookmark: __Fieldmark__23_3623662241]   CTD  

	Location:
	[bookmark: Text2][bookmark: Text21][bookmark: Text2][bookmark: Text2]   MRY Bay  

	Major Objective:
	[bookmark: __Fieldmark__46_3623662241][bookmark: __Fieldmark__46_3623662241][bookmark: __Fieldmark__46_3623662241] CTD Diamond    

	Dive Plan:
	[bookmark: Text4][bookmark: Text41][bookmark: Text4][bookmark: Text4]  Standard Diamond, with modified gulp locations   



Accomplishments:
[bookmark: Text51][bookmark: Text5][bookmark: Text5][bookmark: Text5]     Deployed and recovered without issue.





Vehicle Issues:
[bookmark: Text61][bookmark: Text6][bookmark: Text6]     Apollo was raised up with additional mount bracketry. Doesn’t appear to be sufficient to provide reliable performance, except in the calmest of seas.

Thus, we likely need more height from Apollo. 

[bookmark: Text6]SBD Warrior performance was also not the greatest. Antenna was taped slightly shorter into the mast than previously, perhaps it can be extended a half inch or more to get more distance between whip and GPS patch antenna and Aluminum mast spar.

These comments are based on the fact that during some surfacings, an SBD Warrior SBD would get out, but not from the Apollo, and vice versa, and the Apollo SBDs were greatly under represented.



Note(s):
[bookmark: Text71][bookmark: Text7][bookmark: Text7][bookmark: Text7]     Gulpers 9 & 10 appeared to fire appropriately after extending trigger bolt. 
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